Component: ARM Compiler 5.06 update 1 (build 61) Tool: armlink [4d35a8]

==============================================================================

Section Cross References

    main.o(i.assert_nrf_callback) refers to app_error.o(i.app_error_handler) for app_error_handler
    main.o(i.ble_evt_handler) refers to main.o(i.is_uuid_present) for is_uuid_present
    main.o(i.ble_evt_handler) refers to bsp.o(i.bsp_indication_set) for bsp_indication_set
    main.o(i.ble_evt_handler) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    main.o(i.ble_evt_handler) refers to nrf_log_frontend.o(i.nrf_log_frontend_std_6) for nrf_log_frontend_std_6
    main.o(i.ble_evt_handler) refers to nrf_log_frontend.o(i.nrf_log_frontend_std_0) for nrf_log_frontend_std_0
    main.o(i.ble_evt_handler) refers to ble_nus_c.o(i.ble_nus_c_handles_assign) for ble_nus_c_handles_assign
    main.o(i.ble_evt_handler) refers to ble_db_discovery.o(i.ble_db_discovery_start) for ble_db_discovery_start
    main.o(i.ble_evt_handler) refers to main.o(i.scan_start) for scan_start
    main.o(i.ble_evt_handler) refers to main.o(.constdata) for m_nus_uuid
    main.o(i.ble_evt_handler) refers to nrf_log_frontend.o(log_dynamic_data) for m_nrf_log_app_logs_data_dynamic
    main.o(i.ble_evt_handler) refers to main.o(.bss) for m_ble_nus_c
    main.o(i.ble_evt_handler) refers to main.o(.data) for m_db_disc
    main.o(i.ble_nus_c_evt_handler) refers to nrf_log_frontend.o(i.nrf_log_frontend_std_0) for nrf_log_frontend_std_0
    main.o(i.ble_nus_c_evt_handler) refers to ble_nus_c.o(i.ble_nus_c_handles_assign) for ble_nus_c_handles_assign
    main.o(i.ble_nus_c_evt_handler) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    main.o(i.ble_nus_c_evt_handler) refers to ble_nus_c.o(i.ble_nus_c_tx_notif_enable) for ble_nus_c_tx_notif_enable
    main.o(i.ble_nus_c_evt_handler) refers to main.o(i.ble_nus_chars_received_uart_print) for ble_nus_chars_received_uart_print
    main.o(i.ble_nus_c_evt_handler) refers to main.o(i.scan_start) for scan_start
    main.o(i.ble_nus_c_evt_handler) refers to nrf_log_frontend.o(log_dynamic_data) for m_nrf_log_app_logs_data_dynamic
    main.o(i.ble_nus_chars_received_uart_print) refers to app_uart_fifo.o(i.app_uart_put) for app_uart_put
    main.o(i.ble_nus_chars_received_uart_print) refers to nrf_log_frontend.o(i.nrf_log_frontend_std_1) for nrf_log_frontend_std_1
    main.o(i.ble_nus_chars_received_uart_print) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    main.o(i.ble_nus_chars_received_uart_print) refers to ble_nus_c.o(i.ble_nus_c_string_send) for ble_nus_c_string_send
    main.o(i.ble_nus_chars_received_uart_print) refers to nrf_log_frontend.o(log_dynamic_data) for m_nrf_log_app_logs_data_dynamic
    main.o(i.ble_nus_chars_received_uart_print) refers to main.o(.bss) for m_ble_nus_c
    main.o(i.ble_stack_init) refers to nrf_sdh.o(i.nrf_sdh_enable_request) for nrf_sdh_enable_request
    main.o(i.ble_stack_init) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    main.o(i.ble_stack_init) refers to nrf_sdh_ble.o(i.nrf_sdh_ble_default_cfg_set) for nrf_sdh_ble_default_cfg_set
    main.o(i.ble_stack_init) refers to nrf_sdh_ble.o(i.nrf_sdh_ble_enable) for nrf_sdh_ble_enable
    main.o(i.bsp_event_handler) refers to nrf_pwr_mgmt.o(i.nrf_pwr_mgmt_shutdown) for nrf_pwr_mgmt_shutdown
    main.o(i.bsp_event_handler) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    main.o(i.bsp_event_handler) refers to main.o(.bss) for m_ble_nus_c
    main.o(i.buttons_leds_init) refers to bsp.o(i.bsp_init) for bsp_init
    main.o(i.buttons_leds_init) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    main.o(i.buttons_leds_init) refers to bsp_btn_ble.o(i.bsp_btn_ble_init) for bsp_btn_ble_init
    main.o(i.buttons_leds_init) refers to main.o(i.bsp_event_handler) for bsp_event_handler
    main.o(i.db_disc_handler) refers to ble_nus_c.o(i.ble_nus_c_on_db_disc_evt) for ble_nus_c_on_db_disc_evt
    main.o(i.db_disc_handler) refers to main.o(.bss) for m_ble_nus_c
    main.o(i.db_discovery_init) refers to ble_db_discovery.o(i.ble_db_discovery_init) for ble_db_discovery_init
    main.o(i.db_discovery_init) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    main.o(i.db_discovery_init) refers to main.o(i.db_disc_handler) for db_disc_handler
    main.o(i.gatt_evt_handler) refers to nrf_log_frontend.o(i.nrf_log_frontend_std_0) for nrf_log_frontend_std_0
    main.o(i.gatt_evt_handler) refers to nrf_log_frontend.o(i.nrf_log_frontend_std_2) for nrf_log_frontend_std_2
    main.o(i.gatt_evt_handler) refers to nrf_log_frontend.o(log_dynamic_data) for m_nrf_log_app_logs_data_dynamic
    main.o(i.gatt_evt_handler) refers to main.o(.data) for m_ble_nus_max_data_len
    main.o(i.gatt_init) refers to nrf_ble_gatt.o(i.nrf_ble_gatt_init) for nrf_ble_gatt_init
    main.o(i.gatt_init) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    main.o(i.gatt_init) refers to nrf_ble_gatt.o(i.nrf_ble_gatt_att_mtu_central_set) for nrf_ble_gatt_att_mtu_central_set
    main.o(i.gatt_init) refers to main.o(i.gatt_evt_handler) for gatt_evt_handler
    main.o(i.gatt_init) refers to main.o(.bss) for m_gatt
    main.o(i.log_init) refers to nrf_log_frontend.o(i.nrf_log_init) for nrf_log_init
    main.o(i.log_init) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    main.o(i.log_init) refers to nrf_log_default_backends.o(i.nrf_log_default_backends_init) for nrf_log_default_backends_init
    main.o(i.main) refers to main.o(i.log_init) for log_init
    main.o(i.main) refers to main.o(i.timer_init) for timer_init
    main.o(i.main) refers to main.o(i.power_init) for power_init
    main.o(i.main) refers to main.o(i.uart_init) for uart_init
    main.o(i.main) refers to main.o(i.buttons_leds_init) for buttons_leds_init
    main.o(i.main) refers to main.o(i.db_discovery_init) for db_discovery_init
    main.o(i.main) refers to main.o(i.ble_stack_init) for ble_stack_init
    main.o(i.main) refers to main.o(i.gatt_init) for gatt_init
    main.o(i.main) refers to main.o(i.nus_c_init) for nus_c_init
    main.o(i.main) refers to printfb.o(i.__0printf$bare) for __2printf
    main.o(i.main) refers to nrf_log_frontend.o(i.nrf_log_frontend_std_0) for nrf_log_frontend_std_0
    main.o(i.main) refers to main.o(i.scan_start) for scan_start
    main.o(i.main) refers to nrf_log_frontend.o(i.nrf_log_frontend_dequeue) for nrf_log_frontend_dequeue
    main.o(i.main) refers to nrf_pwr_mgmt.o(i.nrf_pwr_mgmt_run) for nrf_pwr_mgmt_run
    main.o(i.main) refers to nrf_log_frontend.o(log_dynamic_data) for m_nrf_log_app_logs_data_dynamic
    main.o(i.nus_c_init) refers to ble_nus_c.o(i.ble_nus_c_init) for ble_nus_c_init
    main.o(i.nus_c_init) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    main.o(i.nus_c_init) refers to main.o(i.ble_nus_c_evt_handler) for ble_nus_c_evt_handler
    main.o(i.nus_c_init) refers to main.o(.bss) for m_ble_nus_c
    main.o(i.power_init) refers to nrf_pwr_mgmt.o(i.nrf_pwr_mgmt_init) for nrf_pwr_mgmt_init
    main.o(i.power_init) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    main.o(i.scan_start) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    main.o(i.scan_start) refers to bsp.o(i.bsp_indication_set) for bsp_indication_set
    main.o(i.scan_start) refers to main.o(.constdata) for m_scan_params
    main.o(i.shutdown_handler) refers to bsp.o(i.bsp_indication_set) for bsp_indication_set
    main.o(i.shutdown_handler) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    main.o(i.shutdown_handler) refers to bsp_btn_ble.o(i.bsp_btn_ble_sleep_mode_prepare) for bsp_btn_ble_sleep_mode_prepare
    main.o(i.timer_init) refers to app_timer.o(i.app_timer_init) for app_timer_init
    main.o(i.timer_init) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    main.o(i.uart_event_handle) refers to app_uart_fifo.o(i.app_uart_get) for app_uart_get
    main.o(i.uart_event_handle) refers to ble_nus_c.o(i.ble_nus_c_string_send) for ble_nus_c_string_send
    main.o(i.uart_event_handle) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    main.o(i.uart_event_handle) refers to nrf_log_frontend.o(i.nrf_log_frontend_std_0) for nrf_log_frontend_std_0
    main.o(i.uart_event_handle) refers to main.o(.bss) for data_array
    main.o(i.uart_event_handle) refers to main.o(.data) for index
    main.o(i.uart_event_handle) refers to nrf_log_frontend.o(log_dynamic_data) for m_nrf_log_app_logs_data_dynamic
    main.o(i.uart_init) refers to memcpya.o(.text) for __aeabi_memcpy4
    main.o(i.uart_init) refers to app_uart_fifo.o(i.app_uart_init) for app_uart_init
    main.o(i.uart_init) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    main.o(i.uart_init) refers to main.o(.constdata) for .constdata
    main.o(i.uart_init) refers to main.o(.bss) for rx_buf
    main.o(i.uart_init) refers to main.o(i.uart_event_handle) for uart_event_handle
    main.o(pwr_mgmt_data1) refers to main.o(i.shutdown_handler) for shutdown_handler
    main.o(sdh_ble_observers1) refers to nrf_ble_gatt.o(i.nrf_ble_gatt_on_ble_evt) for nrf_ble_gatt_on_ble_evt
    main.o(sdh_ble_observers1) refers to main.o(.bss) for m_gatt
    main.o(sdh_ble_observers1) refers to ble_db_discovery.o(i.ble_db_discovery_on_ble_evt) for ble_db_discovery_on_ble_evt
    main.o(sdh_ble_observers1) refers to main.o(.data) for m_db_disc
    main.o(sdh_ble_observers2) refers to ble_nus_c.o(i.ble_nus_c_on_ble_evt) for ble_nus_c_on_ble_evt
    main.o(sdh_ble_observers2) refers to main.o(.bss) for m_ble_nus_c
    main.o(sdh_ble_observers3) refers to main.o(i.ble_evt_handler) for ble_evt_handler
    boards.o(i.bsp_board_button_idx_to_pin) refers to boards.o(.constdata) for m_board_btn_list
    boards.o(i.bsp_board_button_state_get) refers to boards.o(i.nrf_gpio_pin_port_decode) for nrf_gpio_pin_port_decode
    boards.o(i.bsp_board_button_state_get) refers to boards.o(.constdata) for m_board_btn_list
    boards.o(i.bsp_board_buttons_init) refers to boards.o(i.nrf_gpio_cfg) for nrf_gpio_cfg
    boards.o(i.bsp_board_buttons_init) refers to boards.o(.constdata) for m_board_btn_list
    boards.o(i.bsp_board_led_idx_to_pin) refers to boards.o(.constdata) for m_board_led_list
    boards.o(i.bsp_board_led_invert) refers to boards.o(i.nrf_gpio_pin_port_decode) for nrf_gpio_pin_port_decode
    boards.o(i.bsp_board_led_invert) refers to boards.o(.constdata) for m_board_led_list
    boards.o(i.bsp_board_led_off) refers to boards.o(i.nrf_gpio_pin_write) for nrf_gpio_pin_write
    boards.o(i.bsp_board_led_off) refers to boards.o(.constdata) for m_board_led_list
    boards.o(i.bsp_board_led_on) refers to boards.o(i.nrf_gpio_pin_write) for nrf_gpio_pin_write
    boards.o(i.bsp_board_led_on) refers to boards.o(.constdata) for m_board_led_list
    boards.o(i.bsp_board_led_state_get) refers to boards.o(i.nrf_gpio_pin_port_decode) for nrf_gpio_pin_port_decode
    boards.o(i.bsp_board_led_state_get) refers to boards.o(.constdata) for m_board_led_list
    boards.o(i.bsp_board_leds_init) refers to boards.o(i.nrf_gpio_cfg) for nrf_gpio_cfg
    boards.o(i.bsp_board_leds_init) refers to boards.o(i.bsp_board_leds_off) for bsp_board_leds_off
    boards.o(i.bsp_board_leds_init) refers to boards.o(.constdata) for m_board_led_list
    boards.o(i.bsp_board_leds_off) refers to boards.o(i.bsp_board_led_off) for bsp_board_led_off
    boards.o(i.bsp_board_leds_on) refers to boards.o(i.bsp_board_led_on) for bsp_board_led_on
    boards.o(i.bsp_board_pin_to_button_idx) refers to boards.o(.constdata) for m_board_btn_list
    boards.o(i.bsp_board_pin_to_led_idx) refers to boards.o(.constdata) for m_board_led_list
    boards.o(i.nrf_gpio_cfg) refers to boards.o(i.nrf_gpio_pin_port_decode) for nrf_gpio_pin_port_decode
    boards.o(i.nrf_gpio_pin_write) refers to boards.o(i.nrf_gpio_pin_port_decode) for nrf_gpio_pin_port_decode
    bsp.o(i.alert_timer_handler) refers to boards.o(i.bsp_board_led_invert) for bsp_board_led_invert
    bsp.o(i.bsp_button_event_handler) refers to boards.o(i.bsp_board_pin_to_button_idx) for bsp_board_pin_to_button_idx
    bsp.o(i.bsp_button_event_handler) refers to app_timer.o(i.app_timer_start) for app_timer_start
    bsp.o(i.bsp_button_event_handler) refers to app_timer.o(i.app_timer_stop) for app_timer_stop
    bsp.o(i.bsp_button_event_handler) refers to bsp.o(.bss) for m_events_list
    bsp.o(i.bsp_button_event_handler) refers to bsp.o(.data) for current_long_push_pin_no
    bsp.o(i.bsp_button_event_handler) refers to bsp.o(.constdata) for m_button_timer_id
    bsp.o(i.bsp_button_is_pressed) refers to boards.o(i.bsp_board_button_state_get) for bsp_board_button_state_get
    bsp.o(i.bsp_buttons_disable) refers to app_button.o(i.app_button_disable) for app_button_disable
    bsp.o(i.bsp_buttons_enable) refers to app_button.o(i.app_button_enable) for app_button_enable
    bsp.o(i.bsp_event_to_button_action_assign) refers to bsp.o(.bss) for m_events_list
    bsp.o(i.bsp_indication_set) refers to bsp.o(i.bsp_led_indication) for bsp_led_indication
    bsp.o(i.bsp_indication_set) refers to bsp.o(.data) for m_indication_type
    bsp.o(i.bsp_init) refers to bsp.o(i.bsp_event_to_button_action_assign) for bsp_event_to_button_action_assign
    bsp.o(i.bsp_init) refers to app_button.o(i.app_button_init) for app_button_init
    bsp.o(i.bsp_init) refers to app_button.o(i.app_button_enable) for app_button_enable
    bsp.o(i.bsp_init) refers to app_timer.o(i.app_timer_create) for app_timer_create
    bsp.o(i.bsp_init) refers to boards.o(i.bsp_board_leds_init) for bsp_board_leds_init
    bsp.o(i.bsp_init) refers to bsp.o(.data) for m_indication_type
    bsp.o(i.bsp_init) refers to bsp.o(.constdata) for app_buttons
    bsp.o(i.bsp_init) refers to bsp.o(i.button_timer_handler) for button_timer_handler
    bsp.o(i.bsp_init) refers to bsp.o(i.leds_timer_handler) for leds_timer_handler
    bsp.o(i.bsp_init) refers to bsp.o(i.alert_timer_handler) for alert_timer_handler
    bsp.o(i.bsp_led_indication) refers to bsp.o(i.leds_off) for leds_off
    bsp.o(i.bsp_led_indication) refers to boards.o(i.bsp_board_led_state_get) for bsp_board_led_state_get
    bsp.o(i.bsp_led_indication) refers to boards.o(i.bsp_board_led_off) for bsp_board_led_off
    bsp.o(i.bsp_led_indication) refers to boards.o(i.bsp_board_led_on) for bsp_board_led_on
    bsp.o(i.bsp_led_indication) refers to uldiv.o(.text) for __aeabi_uldivmod
    bsp.o(i.bsp_led_indication) refers to app_timer.o(i.app_timer_start) for app_timer_start
    bsp.o(i.bsp_led_indication) refers to boards.o(i.bsp_board_led_invert) for bsp_board_led_invert
    bsp.o(i.bsp_led_indication) refers to boards.o(i.bsp_board_leds_on) for bsp_board_leds_on
    bsp.o(i.bsp_led_indication) refers to app_timer.o(i.app_timer_stop) for app_timer_stop
    bsp.o(i.bsp_led_indication) refers to bsp.o(.data) for m_leds_clear
    bsp.o(i.bsp_led_indication) refers to bsp.o(.constdata) for m_leds_timer_id
    bsp.o(i.bsp_wakeup_button_disable) refers to boards.o(i.bsp_board_button_idx_to_pin) for bsp_board_button_idx_to_pin
    bsp.o(i.bsp_wakeup_button_disable) refers to bsp.o(i.nrf_gpio_cfg_sense_set) for nrf_gpio_cfg_sense_set
    bsp.o(i.bsp_wakeup_button_enable) refers to boards.o(i.bsp_board_button_idx_to_pin) for bsp_board_button_idx_to_pin
    bsp.o(i.bsp_wakeup_button_enable) refers to bsp.o(i.nrf_gpio_cfg_sense_set) for nrf_gpio_cfg_sense_set
    bsp.o(i.button_timer_handler) refers to bsp.o(i.bsp_button_event_handler) for bsp_button_event_handler
    bsp.o(i.leds_off) refers to boards.o(i.bsp_board_led_off) for bsp_board_led_off
    bsp.o(i.leds_off) refers to boards.o(i.bsp_board_leds_off) for bsp_board_leds_off
    bsp.o(i.leds_off) refers to bsp.o(.data) for m_alert_on
    bsp.o(i.leds_timer_handler) refers to bsp.o(i.bsp_led_indication) for bsp_led_indication
    bsp.o(i.leds_timer_handler) refers to bsp.o(.data) for m_indication_type
    bsp.o(.constdata) refers to bsp.o(.bss) for m_leds_timer_id_data
    bsp.o(.constdata) refers to bsp.o(i.bsp_button_event_handler) for bsp_button_event_handler
    bsp_btn_ble.o(i.advertising_buttons_configure) refers to bsp.o(i.bsp_event_to_button_action_assign) for bsp_event_to_button_action_assign
    bsp_btn_ble.o(i.ble_evt_handler) refers to bsp_btn_ble.o(i.connection_buttons_configure) for connection_buttons_configure
    bsp_btn_ble.o(i.ble_evt_handler) refers to bsp_btn_ble.o(i.advertising_buttons_configure) for advertising_buttons_configure
    bsp_btn_ble.o(i.ble_evt_handler) refers to bsp_btn_ble.o(.data) for m_num_connections
    bsp_btn_ble.o(i.bsp_btn_ble_init) refers to bsp_btn_ble.o(i.startup_event_extract) for startup_event_extract
    bsp_btn_ble.o(i.bsp_btn_ble_init) refers to bsp_btn_ble.o(i.advertising_buttons_configure) for advertising_buttons_configure
    bsp_btn_ble.o(i.bsp_btn_ble_init) refers to bsp_btn_ble.o(.data) for m_error_handler
    bsp_btn_ble.o(i.bsp_btn_ble_sleep_mode_prepare) refers to bsp.o(i.bsp_wakeup_button_enable) for bsp_wakeup_button_enable
    bsp_btn_ble.o(i.connection_buttons_configure) refers to bsp.o(i.bsp_event_to_button_action_assign) for bsp_event_to_button_action_assign
    bsp_btn_ble.o(i.startup_event_extract) refers to bsp.o(i.bsp_button_is_pressed) for bsp_button_is_pressed
    bsp_btn_ble.o(sdh_ble_observers1) refers to bsp_btn_ble.o(i.ble_evt_handler) for ble_evt_handler
    bsp_nfc.o(i.bsp_nfc_btn_deinit) refers to bsp.o(i.bsp_event_to_button_action_assign) for bsp_event_to_button_action_assign
    bsp_nfc.o(i.bsp_nfc_btn_init) refers to bsp.o(i.bsp_event_to_button_action_assign) for bsp_event_to_button_action_assign
    bsp_nfc.o(i.bsp_nfc_sleep_mode_prepare) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    bsp_nfc.o(i.bsp_nfc_sleep_mode_prepare) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    ble_advdata.o(i.appearance_encode) refers to ble_advdata.o(i.uint16_encode) for uint16_encode
    ble_advdata.o(i.ble_advdata_encode) refers to ble_advdata.o(i.ble_device_addr_encode) for ble_device_addr_encode
    ble_advdata.o(i.ble_advdata_encode) refers to ble_advdata.o(i.appearance_encode) for appearance_encode
    ble_advdata.o(i.ble_advdata_encode) refers to ble_advdata.o(i.flags_encode) for flags_encode
    ble_advdata.o(i.ble_advdata_encode) refers to ble_advdata.o(i.tx_power_level_encode) for tx_power_level_encode
    ble_advdata.o(i.ble_advdata_encode) refers to ble_advdata.o(i.uuid_list_encode) for uuid_list_encode
    ble_advdata.o(i.ble_advdata_encode) refers to ble_advdata.o(i.conn_int_encode) for conn_int_encode
    ble_advdata.o(i.ble_advdata_encode) refers to ble_advdata.o(i.manuf_specific_data_encode) for manuf_specific_data_encode
    ble_advdata.o(i.ble_advdata_encode) refers to ble_advdata.o(i.service_data_encode) for service_data_encode
    ble_advdata.o(i.ble_advdata_encode) refers to ble_advdata.o(i.name_encode) for name_encode
    ble_advdata.o(i.ble_advdata_set) refers to ble_advdata.o(i.advdata_check) for advdata_check
    ble_advdata.o(i.ble_advdata_set) refers to ble_advdata.o(i.ble_advdata_encode) for ble_advdata_encode
    ble_advdata.o(i.ble_advdata_set) refers to ble_advdata.o(i.srdata_check) for srdata_check
    ble_advdata.o(i.conn_int_encode) refers to ble_advdata.o(i.conn_int_check) for conn_int_check
    ble_advdata.o(i.conn_int_encode) refers to ble_advdata.o(i.uint16_encode) for uint16_encode
    ble_advdata.o(i.manuf_specific_data_encode) refers to ble_advdata.o(i.uint16_encode) for uint16_encode
    ble_advdata.o(i.manuf_specific_data_encode) refers to memcpya.o(.text) for __aeabi_memcpy
    ble_advdata.o(i.service_data_encode) refers to ble_advdata.o(i.uint16_encode) for uint16_encode
    ble_advdata.o(i.service_data_encode) refers to memcpya.o(.text) for __aeabi_memcpy
    ble_advdata.o(i.uuid_list_encode) refers to ble_advdata.o(i.uuid_list_sized_encode) for uuid_list_sized_encode
    ble_db_discovery.o(i.ble_db_discovery_close) refers to ble_db_discovery.o(.data) for m_num_of_handlers_reg
    ble_db_discovery.o(i.ble_db_discovery_evt_register) refers to ble_db_discovery.o(i.registered_handler_set) for registered_handler_set
    ble_db_discovery.o(i.ble_db_discovery_evt_register) refers to ble_db_discovery.o(.data) for m_initialized
    ble_db_discovery.o(i.ble_db_discovery_init) refers to ble_db_discovery.o(.data) for m_num_of_handlers_reg
    ble_db_discovery.o(i.ble_db_discovery_on_ble_evt) refers to ble_db_discovery.o(i.on_primary_srv_discovery_rsp) for on_primary_srv_discovery_rsp
    ble_db_discovery.o(i.ble_db_discovery_on_ble_evt) refers to ble_db_discovery.o(i.on_characteristic_discovery_rsp) for on_characteristic_discovery_rsp
    ble_db_discovery.o(i.ble_db_discovery_on_ble_evt) refers to ble_db_discovery.o(i.on_descriptor_discovery_rsp) for on_descriptor_discovery_rsp
    ble_db_discovery.o(i.ble_db_discovery_on_ble_evt) refers to ble_db_discovery.o(i.on_disconnected) for on_disconnected
    ble_db_discovery.o(i.ble_db_discovery_on_ble_evt) refers to ble_db_discovery.o(i.discovery_start) for discovery_start
    ble_db_discovery.o(i.ble_db_discovery_on_ble_evt) refers to ble_db_discovery.o(.data) for m_initialized
    ble_db_discovery.o(i.ble_db_discovery_start) refers to ble_db_discovery.o(i.discovery_start) for discovery_start
    ble_db_discovery.o(i.ble_db_discovery_start) refers to ble_db_discovery.o(.data) for m_initialized
    ble_db_discovery.o(i.descriptors_discover) refers to ble_db_discovery.o(i.is_desc_discovery_reqd) for is_desc_discovery_reqd
    ble_db_discovery.o(i.discovery_complete_evt_trigger) refers to ble_db_discovery.o(i.registered_handler_get) for registered_handler_get
    ble_db_discovery.o(i.discovery_complete_evt_trigger) refers to memcpya.o(.text) for __aeabi_memcpy
    ble_db_discovery.o(i.discovery_complete_evt_trigger) refers to ble_db_discovery.o(i.pending_user_evts_send) for pending_user_evts_send
    ble_db_discovery.o(i.discovery_complete_evt_trigger) refers to ble_db_discovery.o(.data) for m_pending_usr_evt_index
    ble_db_discovery.o(i.discovery_complete_evt_trigger) refers to ble_db_discovery.o(.bss) for m_pending_user_evts
    ble_db_discovery.o(i.discovery_error_evt_trigger) refers to ble_db_discovery.o(i.registered_handler_get) for registered_handler_get
    ble_db_discovery.o(i.discovery_error_evt_trigger) refers to memcpya.o(.text) for __aeabi_memcpy4
    ble_db_discovery.o(i.discovery_error_evt_trigger) refers to ble_db_discovery.o(.constdata) for .constdata
    ble_db_discovery.o(i.discovery_start) refers to memseta.o(.text) for __aeabi_memclr
    ble_db_discovery.o(i.discovery_start) refers to ble_db_discovery.o(.data) for m_pending_usr_evt_index
    ble_db_discovery.o(i.discovery_start) refers to ble_db_discovery.o(.bss) for m_registered_handlers
    ble_db_discovery.o(i.on_characteristic_discovery_rsp) refers to ble_db_discovery.o(i.is_char_discovery_reqd) for is_char_discovery_reqd
    ble_db_discovery.o(i.on_characteristic_discovery_rsp) refers to ble_db_discovery.o(i.characteristics_discover) for characteristics_discover
    ble_db_discovery.o(i.on_characteristic_discovery_rsp) refers to ble_db_discovery.o(i.discovery_error_evt_trigger) for discovery_error_evt_trigger
    ble_db_discovery.o(i.on_characteristic_discovery_rsp) refers to ble_db_discovery.o(i.descriptors_discover) for descriptors_discover
    ble_db_discovery.o(i.on_characteristic_discovery_rsp) refers to ble_db_discovery.o(i.discovery_complete_evt_trigger) for discovery_complete_evt_trigger
    ble_db_discovery.o(i.on_characteristic_discovery_rsp) refers to ble_db_discovery.o(i.on_srv_disc_completion) for on_srv_disc_completion
    ble_db_discovery.o(i.on_characteristic_discovery_rsp) refers to ble_db_discovery.o(.bss) for m_pending_user_evts
    ble_db_discovery.o(i.on_descriptor_discovery_rsp) refers to ble_db_discovery.o(i.descriptors_discover) for descriptors_discover
    ble_db_discovery.o(i.on_descriptor_discovery_rsp) refers to ble_db_discovery.o(i.discovery_error_evt_trigger) for discovery_error_evt_trigger
    ble_db_discovery.o(i.on_descriptor_discovery_rsp) refers to ble_db_discovery.o(i.discovery_complete_evt_trigger) for discovery_complete_evt_trigger
    ble_db_discovery.o(i.on_descriptor_discovery_rsp) refers to ble_db_discovery.o(i.on_srv_disc_completion) for on_srv_disc_completion
    ble_db_discovery.o(i.on_descriptor_discovery_rsp) refers to ble_db_discovery.o(.bss) for m_pending_user_evts
    ble_db_discovery.o(i.on_primary_srv_discovery_rsp) refers to ble_db_discovery.o(i.characteristics_discover) for characteristics_discover
    ble_db_discovery.o(i.on_primary_srv_discovery_rsp) refers to ble_db_discovery.o(i.discovery_error_evt_trigger) for discovery_error_evt_trigger
    ble_db_discovery.o(i.on_primary_srv_discovery_rsp) refers to ble_db_discovery.o(i.discovery_complete_evt_trigger) for discovery_complete_evt_trigger
    ble_db_discovery.o(i.on_primary_srv_discovery_rsp) refers to ble_db_discovery.o(i.on_srv_disc_completion) for on_srv_disc_completion
    ble_db_discovery.o(i.on_primary_srv_discovery_rsp) refers to ble_db_discovery.o(.bss) for m_pending_user_evts
    ble_db_discovery.o(i.on_srv_disc_completion) refers to ble_db_discovery.o(i.discovery_error_evt_trigger) for discovery_error_evt_trigger
    ble_db_discovery.o(i.on_srv_disc_completion) refers to ble_db_discovery.o(.data) for m_num_of_handlers_reg
    ble_db_discovery.o(i.on_srv_disc_completion) refers to ble_db_discovery.o(.bss) for m_registered_handlers
    ble_db_discovery.o(i.pending_user_evts_send) refers to ble_db_discovery.o(.bss) for m_pending_user_evts
    ble_db_discovery.o(i.pending_user_evts_send) refers to ble_db_discovery.o(.data) for m_num_of_handlers_reg
    ble_db_discovery.o(i.registered_handler_get) refers to ble_db_discovery.o(.bss) for m_registered_handlers
    ble_db_discovery.o(i.registered_handler_get) refers to ble_db_discovery.o(.data) for m_evt_handler
    ble_db_discovery.o(i.registered_handler_set) refers to ble_db_discovery.o(i.registered_handler_get) for registered_handler_get
    ble_db_discovery.o(i.registered_handler_set) refers to ble_db_discovery.o(.data) for m_num_of_handlers_reg
    ble_db_discovery.o(i.registered_handler_set) refers to ble_db_discovery.o(.bss) for m_registered_handlers
    ble_db_discovery.o(log_const_data) refers to ble_db_discovery.o(.conststrlit) for .conststrlit
    ble_srv_common.o(i.ble_srv_ascii_to_utf8) refers to strlen.o(.text) for strlen
    ble_srv_common.o(i.ble_srv_is_indication_enabled) refers to ble_srv_common.o(i.uint16_decode) for uint16_decode
    ble_srv_common.o(i.ble_srv_is_notification_enabled) refers to ble_srv_common.o(i.uint16_decode) for uint16_decode
    ble_srv_common.o(i.ble_srv_report_ref_encode) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    ble_srv_common.o(i.characteristic_add) refers to ble_srv_common.o(i.set_security_req) for set_security_req
    ble_srv_common.o(i.characteristic_add) refers to memseta.o(.text) for __aeabi_memclr4
    ble_srv_common.o(i.descriptor_add) refers to memseta.o(.text) for __aeabi_memclr4
    ble_srv_common.o(i.descriptor_add) refers to ble_srv_common.o(i.set_security_req) for set_security_req
    nrf_ble_gatt.o(i.data_length_update) refers to nrf_log_frontend.o(i.nrf_log_frontend_std_2) for nrf_log_frontend_std_2
    nrf_ble_gatt.o(i.data_length_update) refers to nrf_ble_gatt.o(log_dynamic_data) for m_nrf_log_ble_gatt_logs_data_dynamic
    nrf_ble_gatt.o(i.data_length_update) refers to nrf_ble_gatt.o(.conststring) for .conststring
    nrf_ble_gatt.o(i.nrf_ble_gatt_init) refers to nrf_ble_gatt.o(i.link_init) for link_init
    nrf_ble_gatt.o(i.nrf_ble_gatt_on_ble_evt) refers to nrf_ble_gatt.o(i.on_connected_evt) for on_connected_evt
    nrf_ble_gatt.o(i.nrf_ble_gatt_on_ble_evt) refers to nrf_ble_gatt.o(i.on_disconnected_evt) for on_disconnected_evt
    nrf_ble_gatt.o(i.nrf_ble_gatt_on_ble_evt) refers to nrf_ble_gatt.o(i.on_exchange_mtu_rsp_evt) for on_exchange_mtu_rsp_evt
    nrf_ble_gatt.o(i.nrf_ble_gatt_on_ble_evt) refers to nrf_ble_gatt.o(i.on_exchange_mtu_request_evt) for on_exchange_mtu_request_evt
    nrf_ble_gatt.o(i.nrf_ble_gatt_on_ble_evt) refers to nrf_ble_gatt.o(i.on_data_length_update_evt) for on_data_length_update_evt
    nrf_ble_gatt.o(i.nrf_ble_gatt_on_ble_evt) refers to nrf_ble_gatt.o(i.on_data_length_update_request_evt) for on_data_length_update_request_evt
    nrf_ble_gatt.o(i.nrf_ble_gatt_on_ble_evt) refers to nrf_log_frontend.o(i.nrf_log_frontend_std_1) for nrf_log_frontend_std_1
    nrf_ble_gatt.o(i.nrf_ble_gatt_on_ble_evt) refers to nrf_ble_gatt.o(log_dynamic_data) for m_nrf_log_ble_gatt_logs_data_dynamic
    nrf_ble_gatt.o(i.nrf_ble_gatt_on_ble_evt) refers to nrf_ble_gatt.o(.conststring) for .conststring
    nrf_ble_gatt.o(i.on_connected_evt) refers to nrf_log_frontend.o(i.nrf_log_frontend_std_1) for nrf_log_frontend_std_1
    nrf_ble_gatt.o(i.on_connected_evt) refers to nrf_ble_gatt.o(i.data_length_update) for data_length_update
    nrf_ble_gatt.o(i.on_connected_evt) refers to nrf_ble_gatt.o(log_dynamic_data) for m_nrf_log_ble_gatt_logs_data_dynamic
    nrf_ble_gatt.o(i.on_connected_evt) refers to nrf_ble_gatt.o(.conststring) for .conststring
    nrf_ble_gatt.o(i.on_data_length_update_evt) refers to memcpya.o(.text) for __aeabi_memcpy4
    nrf_ble_gatt.o(i.on_data_length_update_evt) refers to nrf_ble_gatt.o(.constdata) for .constdata
    nrf_ble_gatt.o(i.on_data_length_update_request_evt) refers to nrf_log_frontend.o(i.nrf_log_frontend_std_1) for nrf_log_frontend_std_1
    nrf_ble_gatt.o(i.on_data_length_update_request_evt) refers to nrf_ble_gatt.o(log_dynamic_data) for m_nrf_log_ble_gatt_logs_data_dynamic
    nrf_ble_gatt.o(i.on_data_length_update_request_evt) refers to nrf_ble_gatt.o(.conststring) for .conststring
    nrf_ble_gatt.o(i.on_disconnected_evt) refers to nrf_ble_gatt.o(i.link_init) for link_init
    nrf_ble_gatt.o(i.on_exchange_mtu_request_evt) refers to nrf_log_frontend.o(i.nrf_log_frontend_std_1) for nrf_log_frontend_std_1
    nrf_ble_gatt.o(i.on_exchange_mtu_request_evt) refers to nrf_ble_gatt.o(log_dynamic_data) for m_nrf_log_ble_gatt_logs_data_dynamic
    nrf_ble_gatt.o(i.on_exchange_mtu_request_evt) refers to nrf_ble_gatt.o(.conststring) for .conststring
    nrf_ble_gatt.o(i.on_exchange_mtu_request_evt) refers to nrf_ble_gatt.o(.constdata) for .constdata
    nrf_ble_gatt.o(i.on_exchange_mtu_rsp_evt) refers to nrf_ble_gatt.o(.constdata) for .constdata
    nrf_ble_gatt.o(log_const_data) refers to nrf_ble_gatt.o(.conststrlit) for .conststrlit
    ble_nus_c.o(i.ble_nus_c_init) refers to ble_db_discovery.o(i.ble_db_discovery_evt_register) for ble_db_discovery_evt_register
    ble_nus_c.o(i.ble_nus_c_init) refers to ble_nus_c.o(.constdata) for .constdata
    ble_nus_c.o(i.ble_nus_c_on_ble_evt) refers to ble_nus_c.o(i.on_hvx) for on_hvx
    ble_nus_c.o(i.ble_nus_c_on_db_disc_evt) refers to memseta.o(.text) for __aeabi_memclr4
    ble_nus_c.o(i.ble_nus_c_string_send) refers to nrf_log_frontend.o(i.nrf_log_frontend_std_0) for nrf_log_frontend_std_0
    ble_nus_c.o(i.ble_nus_c_string_send) refers to ble_nus_c.o(log_dynamic_data) for m_nrf_log_ble_nus_logs_data_dynamic
    ble_nus_c.o(i.ble_nus_c_string_send) refers to ble_nus_c.o(.constdata) for .constdata
    ble_nus_c.o(i.ble_nus_c_tx_notif_enable) refers to ble_nus_c.o(i.cccd_configure) for cccd_configure
    ble_nus_c.o(i.cccd_configure) refers to ble_nus_c.o(.constdata) for .constdata
    ble_nus_c.o(log_const_data) refers to ble_nus_c.o(.conststrlit) for .conststrlit
    nrf_drv_clock.o(i.POWER_CLOCK_IRQHandler) refers to nrf_drv_clock.o(i.nrf_clock_event_check) for nrf_clock_event_check
    nrf_drv_clock.o(i.POWER_CLOCK_IRQHandler) refers to nrf_drv_clock.o(i.nrf_clock_event_clear) for nrf_clock_event_clear
    nrf_drv_clock.o(i.POWER_CLOCK_IRQHandler) refers to nrf_drv_clock.o(i.nrf_clock_int_disable) for nrf_clock_int_disable
    nrf_drv_clock.o(i.POWER_CLOCK_IRQHandler) refers to nrf_drv_clock.o(i.clock_clk_started_notify) for clock_clk_started_notify
    nrf_drv_clock.o(i.POWER_CLOCK_IRQHandler) refers to nrf_drv_clock.o(.bss) for m_clock_cb
    nrf_drv_clock.o(i.clock_clk_started_notify) refers to nrf_drv_clock.o(i.item_dequeue) for item_dequeue
    nrf_drv_clock.o(i.clock_clk_started_notify) refers to nrf_drv_clock.o(.bss) for m_clock_cb
    nrf_drv_clock.o(i.hfclk_start) refers to nrf_sdh.o(i.nrf_sdh_is_enabled) for nrf_sdh_is_enabled
    nrf_drv_clock.o(i.hfclk_start) refers to nrf_drv_clock.o(i.nrf_clock_event_clear) for nrf_clock_event_clear
    nrf_drv_clock.o(i.hfclk_start) refers to nrf_drv_clock.o(i.nrf_clock_int_enable) for nrf_clock_int_enable
    nrf_drv_clock.o(i.hfclk_start) refers to nrf_drv_clock.o(i.nrf_clock_task_trigger) for nrf_clock_task_trigger
    nrf_drv_clock.o(i.hfclk_stop) refers to nrf_sdh.o(i.nrf_sdh_is_enabled) for nrf_sdh_is_enabled
    nrf_drv_clock.o(i.hfclk_stop) refers to nrf_drv_clock.o(i.nrf_clock_task_trigger) for nrf_clock_task_trigger
    nrf_drv_clock.o(i.hfclk_stop) refers to nrf_drv_clock.o(i.nrf_clock_hf_is_running) for nrf_clock_hf_is_running
    nrf_drv_clock.o(i.hfclk_stop) refers to nrf_drv_clock.o(.bss) for m_clock_cb
    nrf_drv_clock.o(i.lfclk_start) refers to nrf_drv_clock.o(i.nrf_clock_event_clear) for nrf_clock_event_clear
    nrf_drv_clock.o(i.lfclk_start) refers to nrf_drv_clock.o(i.nrf_clock_int_enable) for nrf_clock_int_enable
    nrf_drv_clock.o(i.lfclk_start) refers to nrf_drv_clock.o(i.nrf_clock_task_trigger) for nrf_clock_task_trigger
    nrf_drv_clock.o(i.lfclk_stop) refers to nrf_drv_clock.o(i.nrf_clock_task_trigger) for nrf_clock_task_trigger
    nrf_drv_clock.o(i.lfclk_stop) refers to nrf_drv_clock.o(i.nrf_clock_lf_is_running) for nrf_clock_lf_is_running
    nrf_drv_clock.o(i.lfclk_stop) refers to nrf_drv_clock.o(.bss) for m_clock_cb
    nrf_drv_clock.o(i.nrf_drv_clock_hfclk_is_running) refers to nrf_sdh.o(i.nrf_sdh_is_enabled) for nrf_sdh_is_enabled
    nrf_drv_clock.o(i.nrf_drv_clock_hfclk_is_running) refers to nrf_drv_clock.o(i.nrf_clock_hf_is_running) for nrf_clock_hf_is_running
    nrf_drv_clock.o(i.nrf_drv_clock_hfclk_release) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    nrf_drv_clock.o(i.nrf_drv_clock_hfclk_release) refers to nrf_drv_clock.o(i.hfclk_stop) for hfclk_stop
    nrf_drv_clock.o(i.nrf_drv_clock_hfclk_release) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    nrf_drv_clock.o(i.nrf_drv_clock_hfclk_release) refers to nrf_drv_clock.o(.bss) for m_clock_cb
    nrf_drv_clock.o(i.nrf_drv_clock_hfclk_request) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    nrf_drv_clock.o(i.nrf_drv_clock_hfclk_request) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    nrf_drv_clock.o(i.nrf_drv_clock_hfclk_request) refers to nrf_drv_clock.o(i.item_enqueue) for item_enqueue
    nrf_drv_clock.o(i.nrf_drv_clock_hfclk_request) refers to nrf_drv_clock.o(i.hfclk_start) for hfclk_start
    nrf_drv_clock.o(i.nrf_drv_clock_hfclk_request) refers to nrf_drv_clock.o(.bss) for m_clock_cb
    nrf_drv_clock.o(i.nrf_drv_clock_init) refers to nrf_drv_common.o(i.nrf_drv_common_irq_enable) for nrf_drv_common_irq_enable
    nrf_drv_clock.o(i.nrf_drv_clock_init) refers to nrf_sdh.o(i.nrf_sdh_is_enabled) for nrf_sdh_is_enabled
    nrf_drv_clock.o(i.nrf_drv_clock_init) refers to nrf_drv_clock.o(.bss) for m_clock_cb
    nrf_drv_clock.o(i.nrf_drv_clock_init_check) refers to nrf_drv_clock.o(.bss) for m_clock_cb
    nrf_drv_clock.o(i.nrf_drv_clock_lfclk_is_running) refers to nrf_sdh.o(i.nrf_sdh_is_enabled) for nrf_sdh_is_enabled
    nrf_drv_clock.o(i.nrf_drv_clock_lfclk_is_running) refers to nrf_drv_clock.o(i.nrf_clock_lf_is_running) for nrf_clock_lf_is_running
    nrf_drv_clock.o(i.nrf_drv_clock_lfclk_release) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    nrf_drv_clock.o(i.nrf_drv_clock_lfclk_release) refers to nrf_drv_clock.o(i.lfclk_stop) for lfclk_stop
    nrf_drv_clock.o(i.nrf_drv_clock_lfclk_release) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    nrf_drv_clock.o(i.nrf_drv_clock_lfclk_release) refers to nrf_drv_clock.o(.bss) for m_clock_cb
    nrf_drv_clock.o(i.nrf_drv_clock_lfclk_request) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    nrf_drv_clock.o(i.nrf_drv_clock_lfclk_request) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    nrf_drv_clock.o(i.nrf_drv_clock_lfclk_request) refers to nrf_drv_clock.o(i.item_enqueue) for item_enqueue
    nrf_drv_clock.o(i.nrf_drv_clock_lfclk_request) refers to nrf_drv_clock.o(i.lfclk_start) for lfclk_start
    nrf_drv_clock.o(i.nrf_drv_clock_lfclk_request) refers to nrf_drv_clock.o(.bss) for m_clock_cb
    nrf_drv_clock.o(i.nrf_drv_clock_uninit) refers to nrf_drv_common.o(i.nrf_drv_common_clock_irq_disable) for nrf_drv_common_clock_irq_disable
    nrf_drv_clock.o(i.nrf_drv_clock_uninit) refers to nrf_drv_clock.o(i.nrf_clock_int_disable) for nrf_clock_int_disable
    nrf_drv_clock.o(i.nrf_drv_clock_uninit) refers to nrf_drv_clock.o(i.lfclk_stop) for lfclk_stop
    nrf_drv_clock.o(i.nrf_drv_clock_uninit) refers to nrf_drv_clock.o(i.hfclk_stop) for hfclk_stop
    nrf_drv_clock.o(i.nrf_drv_clock_uninit) refers to nrf_drv_clock.o(.bss) for m_clock_cb
    nrf_drv_clock.o(i.sd_state_evt_handler) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    nrf_drv_clock.o(i.sd_state_evt_handler) refers to nrf_drv_clock.o(i.nrf_drv_clock_init) for nrf_drv_clock_init
    nrf_drv_clock.o(i.sd_state_evt_handler) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    nrf_drv_clock.o(i.sd_state_evt_handler) refers to nrf_drv_common.o(i.nrf_drv_common_irq_enable) for nrf_drv_common_irq_enable
    nrf_drv_clock.o(i.sd_state_evt_handler) refers to nrf_drv_clock.o(i.nrf_drv_clock_lfclk_release) for nrf_drv_clock_lfclk_release
    nrf_drv_clock.o(i.sd_state_evt_handler) refers to nrf_drv_clock.o(.bss) for m_clock_cb
    nrf_drv_clock.o(i.soc_evt_handler) refers to nrf_drv_clock.o(i.clock_clk_started_notify) for clock_clk_started_notify
    nrf_drv_clock.o(log_const_data) refers to nrf_drv_clock.o(.conststrlit) for .conststrlit
    nrf_drv_clock.o(sdh_soc_observers0) refers to nrf_drv_clock.o(i.soc_evt_handler) for soc_evt_handler
    nrf_drv_clock.o(sdh_state_observers0) refers to nrf_drv_clock.o(i.sd_state_evt_handler) for sd_state_evt_handler
    nrf_drv_gpiote.o(i.GPIOTE_IRQHandler) refers to nrf_drv_gpiote.o(i.nrf_gpiote_event_is_set) for nrf_gpiote_event_is_set
    nrf_drv_gpiote.o(i.GPIOTE_IRQHandler) refers to nrf_drv_gpiote.o(i.nrf_gpiote_event_clear) for nrf_gpiote_event_clear
    nrf_drv_gpiote.o(i.GPIOTE_IRQHandler) refers to nrf_drv_gpiote.o(i.nrf_gpio_ports_read) for nrf_gpio_ports_read
    nrf_drv_gpiote.o(i.GPIOTE_IRQHandler) refers to nrf_drv_gpiote.o(i.channel_handler_get) for channel_handler_get
    nrf_drv_gpiote.o(i.GPIOTE_IRQHandler) refers to nrf_drv_gpiote.o(i.nrf_bitmask_bit_is_set) for nrf_bitmask_bit_is_set
    nrf_drv_gpiote.o(i.GPIOTE_IRQHandler) refers to nrf_drv_gpiote.o(i.channel_port_get) for channel_port_get
    nrf_drv_gpiote.o(i.GPIOTE_IRQHandler) refers to nrf_drv_gpiote.o(i.nrf_gpio_pin_port_decode) for nrf_gpio_pin_port_decode
    nrf_drv_gpiote.o(i.GPIOTE_IRQHandler) refers to nrf_drv_gpiote.o(i.nrf_gpio_cfg_sense_set) for nrf_gpio_cfg_sense_set
    nrf_drv_gpiote.o(i.GPIOTE_IRQHandler) refers to nrf_drv_gpiote.o(.bss) for m_cb
    nrf_drv_gpiote.o(i.channel_free) refers to nrf_drv_gpiote.o(.bss) for m_cb
    nrf_drv_gpiote.o(i.channel_handler_get) refers to nrf_drv_gpiote.o(.bss) for m_cb
    nrf_drv_gpiote.o(i.channel_port_alloc) refers to nrf_drv_gpiote.o(.bss) for m_cb
    nrf_drv_gpiote.o(i.channel_port_get) refers to nrf_drv_gpiote.o(.bss) for m_cb
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_clr_task_addr_get) refers to nrf_drv_gpiote.o(i.channel_port_get) for channel_port_get
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_clr_task_addr_get) refers to nrf_drv_gpiote.o(i.nrf_gpiote_task_addr_get) for nrf_gpiote_task_addr_get
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_clr_task_trigger) refers to nrf_drv_gpiote.o(i.channel_port_get) for channel_port_get
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_in_event_addr_get) refers to nrf_drv_gpiote.o(i.pin_in_use_by_te) for pin_in_use_by_te
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_in_event_addr_get) refers to nrf_drv_gpiote.o(i.channel_port_get) for channel_port_get
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_in_event_addr_get) refers to nrf_drv_gpiote.o(i.nrf_gpiote_event_addr_get) for nrf_gpiote_event_addr_get
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_in_event_disable) refers to nrf_drv_gpiote.o(i.pin_in_use_by_port) for pin_in_use_by_port
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_in_event_disable) refers to nrf_drv_gpiote.o(i.nrf_gpio_cfg_sense_set) for nrf_gpio_cfg_sense_set
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_in_event_disable) refers to nrf_drv_gpiote.o(i.pin_in_use_by_te) for pin_in_use_by_te
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_in_event_disable) refers to nrf_drv_gpiote.o(i.channel_port_get) for channel_port_get
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_in_event_enable) refers to nrf_drv_gpiote.o(i.pin_in_use_by_port) for pin_in_use_by_port
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_in_event_enable) refers to nrf_drv_gpiote.o(i.channel_port_get) for channel_port_get
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_in_event_enable) refers to nrf_drv_gpiote.o(i.nrf_gpio_pin_read) for nrf_gpio_pin_read
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_in_event_enable) refers to nrf_drv_gpiote.o(i.nrf_gpio_cfg_sense_set) for nrf_gpio_cfg_sense_set
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_in_event_enable) refers to nrf_drv_gpiote.o(i.pin_in_use_by_te) for pin_in_use_by_te
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_in_event_enable) refers to nrf_drv_gpiote.o(i.nrf_gpiote_event_clear) for nrf_gpiote_event_clear
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_in_event_enable) refers to nrf_drv_gpiote.o(i.channel_handler_get) for channel_handler_get
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_in_event_enable) refers to nrf_drv_gpiote.o(i.nrf_gpiote_int_enable) for nrf_gpiote_int_enable
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_in_event_enable) refers to nrf_drv_gpiote.o(.bss) for m_cb
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_in_init) refers to nrf_drv_gpiote.o(i.pin_in_use_by_gpiote) for pin_in_use_by_gpiote
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_in_init) refers to nrf_drv_gpiote.o(i.channel_port_alloc) for channel_port_alloc
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_in_init) refers to nrf_drv_gpiote.o(i.nrf_gpio_pin_port_decode) for nrf_gpio_pin_port_decode
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_in_init) refers to nrf_drv_gpiote.o(i.nrf_gpio_cfg) for nrf_gpio_cfg
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_in_init) refers to nrf_drv_gpiote.o(.bss) for m_cb
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_in_is_set) refers to nrf_drv_gpiote.o(i.nrf_gpio_pin_read) for nrf_gpio_pin_read
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_in_uninit) refers to nrf_drv_gpiote.o(i.nrf_drv_gpiote_in_event_disable) for nrf_drv_gpiote_in_event_disable
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_in_uninit) refers to nrf_drv_gpiote.o(i.pin_in_use_by_te) for pin_in_use_by_te
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_in_uninit) refers to nrf_drv_gpiote.o(i.channel_port_get) for channel_port_get
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_in_uninit) refers to nrf_drv_gpiote.o(i.nrf_gpiote_te_default) for nrf_gpiote_te_default
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_in_uninit) refers to nrf_drv_gpiote.o(i.nrf_gpio_cfg_default) for nrf_gpio_cfg_default
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_in_uninit) refers to nrf_drv_gpiote.o(i.channel_free) for channel_free
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_in_uninit) refers to nrf_drv_gpiote.o(i.pin_in_use_clear) for pin_in_use_clear
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_init) refers to nrf_drv_gpiote.o(i.pin_in_use_clear) for pin_in_use_clear
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_init) refers to nrf_drv_gpiote.o(i.channel_free) for channel_free
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_init) refers to nrf_drv_common.o(i.nrf_drv_common_irq_enable) for nrf_drv_common_irq_enable
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_init) refers to nrf_drv_gpiote.o(i.nrf_gpiote_event_clear) for nrf_gpiote_event_clear
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_init) refers to nrf_drv_gpiote.o(i.nrf_gpiote_int_enable) for nrf_gpiote_int_enable
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_init) refers to nrf_drv_gpiote.o(.bss) for m_cb
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_is_init) refers to nrf_drv_gpiote.o(.bss) for m_cb
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_out_clear) refers to nrf_drv_gpiote.o(i.nrf_gpio_pin_clear) for nrf_gpio_pin_clear
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_out_init) refers to nrf_drv_gpiote.o(i.channel_port_alloc) for channel_port_alloc
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_out_init) refers to nrf_drv_gpiote.o(i.nrf_gpio_pin_set) for nrf_gpio_pin_set
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_out_init) refers to nrf_drv_gpiote.o(i.nrf_gpio_pin_clear) for nrf_gpio_pin_clear
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_out_init) refers to nrf_drv_gpiote.o(i.nrf_gpio_cfg) for nrf_gpio_cfg
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_out_init) refers to nrf_drv_gpiote.o(.bss) for m_cb
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_out_set) refers to nrf_drv_gpiote.o(i.nrf_gpio_pin_set) for nrf_gpio_pin_set
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_out_task_addr_get) refers to nrf_drv_gpiote.o(i.channel_port_get) for channel_port_get
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_out_task_addr_get) refers to nrf_drv_gpiote.o(i.nrf_gpiote_task_addr_get) for nrf_gpiote_task_addr_get
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_out_task_disable) refers to nrf_drv_gpiote.o(.bss) for m_cb
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_out_task_enable) refers to nrf_drv_gpiote.o(.bss) for m_cb
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_out_task_force) refers to nrf_drv_gpiote.o(.bss) for m_cb
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_out_task_trigger) refers to nrf_drv_gpiote.o(i.channel_port_get) for channel_port_get
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_out_toggle) refers to nrf_drv_gpiote.o(i.nrf_gpio_pin_port_decode) for nrf_gpio_pin_port_decode
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_out_uninit) refers to nrf_drv_gpiote.o(i.pin_in_use_by_te) for pin_in_use_by_te
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_out_uninit) refers to nrf_drv_gpiote.o(i.channel_port_get) for channel_port_get
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_out_uninit) refers to nrf_drv_gpiote.o(i.channel_free) for channel_free
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_out_uninit) refers to nrf_drv_gpiote.o(i.nrf_gpiote_te_default) for nrf_gpiote_te_default
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_out_uninit) refers to nrf_drv_gpiote.o(i.pin_in_use_clear) for pin_in_use_clear
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_out_uninit) refers to nrf_drv_gpiote.o(i.nrf_gpio_cfg_default) for nrf_gpio_cfg_default
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_set_task_addr_get) refers to nrf_drv_gpiote.o(i.channel_port_get) for channel_port_get
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_set_task_addr_get) refers to nrf_drv_gpiote.o(i.nrf_gpiote_task_addr_get) for nrf_gpiote_task_addr_get
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_set_task_trigger) refers to nrf_drv_gpiote.o(i.channel_port_get) for channel_port_get
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_uninit) refers to nrf_drv_gpiote.o(i.nrf_drv_gpiote_out_uninit) for nrf_drv_gpiote_out_uninit
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_uninit) refers to nrf_drv_gpiote.o(i.pin_in_use_by_gpiote) for pin_in_use_by_gpiote
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_uninit) refers to nrf_drv_gpiote.o(i.nrf_drv_gpiote_in_uninit) for nrf_drv_gpiote_in_uninit
    nrf_drv_gpiote.o(i.nrf_drv_gpiote_uninit) refers to nrf_drv_gpiote.o(.bss) for m_cb
    nrf_drv_gpiote.o(i.nrf_gpio_cfg) refers to nrf_drv_gpiote.o(i.nrf_gpio_pin_port_decode) for nrf_gpio_pin_port_decode
    nrf_drv_gpiote.o(i.nrf_gpio_cfg_default) refers to nrf_drv_gpiote.o(i.nrf_gpio_cfg) for nrf_gpio_cfg
    nrf_drv_gpiote.o(i.nrf_gpio_cfg_sense_set) refers to nrf_drv_gpiote.o(i.nrf_gpio_pin_port_decode) for nrf_gpio_pin_port_decode
    nrf_drv_gpiote.o(i.nrf_gpio_pin_clear) refers to nrf_drv_gpiote.o(i.nrf_gpio_pin_port_decode) for nrf_gpio_pin_port_decode
    nrf_drv_gpiote.o(i.nrf_gpio_pin_read) refers to nrf_drv_gpiote.o(i.nrf_gpio_pin_port_decode) for nrf_gpio_pin_port_decode
    nrf_drv_gpiote.o(i.nrf_gpio_pin_set) refers to nrf_drv_gpiote.o(i.nrf_gpio_pin_port_decode) for nrf_gpio_pin_port_decode
    nrf_drv_gpiote.o(i.nrf_gpio_ports_read) refers to nrf_drv_gpiote.o(.constdata) for .constdata
    nrf_drv_gpiote.o(i.nrf_gpiote_event_clear) refers to nrf_drv_gpiote.o(i.nrf_gpiote_event_addr_get) for nrf_gpiote_event_addr_get
    nrf_drv_gpiote.o(i.nrf_gpiote_event_is_set) refers to nrf_drv_gpiote.o(i.nrf_gpiote_event_addr_get) for nrf_gpiote_event_addr_get
    nrf_drv_gpiote.o(i.pin_in_use_by_gpiote) refers to nrf_drv_gpiote.o(.bss) for m_cb
    nrf_drv_gpiote.o(i.pin_in_use_by_port) refers to nrf_drv_gpiote.o(.bss) for m_cb
    nrf_drv_gpiote.o(i.pin_in_use_by_te) refers to nrf_drv_gpiote.o(.bss) for m_cb
    nrf_drv_gpiote.o(i.pin_in_use_clear) refers to nrf_drv_gpiote.o(.bss) for m_cb
    nrf_drv_gpiote.o(log_const_data) refers to nrf_drv_gpiote.o(.conststrlit) for .conststrlit
    nrf_drv_uart.o(i.UARTE0_UART0_IRQHandler) refers to nrf_drv_uart.o(i.uarte_irq_handler) for uarte_irq_handler
    nrf_drv_uart.o(i.UARTE0_UART0_IRQHandler) refers to nrf_drv_uart.o(i.uart_irq_handler) for uart_irq_handler
    nrf_drv_uart.o(i.UARTE0_UART0_IRQHandler) refers to nrf_drv_uart.o(.bss) for m_cb
    nrf_drv_uart.o(i.apply_config) refers to nrf_drv_uart.o(i.nrf_gpio_pin_set) for nrf_gpio_pin_set
    nrf_drv_uart.o(i.apply_config) refers to nrf_drv_uart.o(i.nrf_gpio_cfg_output) for nrf_gpio_cfg_output
    nrf_drv_uart.o(i.apply_config) refers to nrf_drv_uart.o(i.nrf_gpio_cfg_input) for nrf_gpio_cfg_input
    nrf_drv_uart.o(i.apply_config) refers to nrf_drv_uart.o(i.nrf_uarte_txrx_pins_set) for nrf_uarte_txrx_pins_set
    nrf_drv_uart.o(i.apply_config) refers to nrf_drv_uart.o(i.nrf_uarte_hwfc_pins_set) for nrf_uarte_hwfc_pins_set
    nrf_drv_uart.o(i.apply_config) refers to nrf_drv_uart.o(i.nrf_uart_txrx_pins_set) for nrf_uart_txrx_pins_set
    nrf_drv_uart.o(i.apply_config) refers to nrf_drv_uart.o(i.nrf_uart_hwfc_pins_set) for nrf_uart_hwfc_pins_set
    nrf_drv_uart.o(i.apply_config) refers to nrf_drv_uart.o(.bss) for m_cb
    nrf_drv_uart.o(i.interrupts_enable) refers to nrf_drv_uart.o(i.nrf_uarte_event_clear) for nrf_uarte_event_clear
    nrf_drv_uart.o(i.interrupts_enable) refers to nrf_drv_uart.o(i.nrf_uarte_int_enable) for nrf_uarte_int_enable
    nrf_drv_uart.o(i.interrupts_enable) refers to nrf_drv_uart.o(i.nrf_drv_get_IRQn) for nrf_drv_get_IRQn
    nrf_drv_uart.o(i.interrupts_enable) refers to nrf_drv_common.o(i.nrf_drv_common_irq_enable) for nrf_drv_common_irq_enable
    nrf_drv_uart.o(i.interrupts_enable) refers to nrf_drv_uart.o(i.nrf_uart_event_clear) for nrf_uart_event_clear
    nrf_drv_uart.o(i.interrupts_enable) refers to nrf_drv_uart.o(i.nrf_uart_int_enable) for nrf_uart_int_enable
    nrf_drv_uart.o(i.interrupts_enable) refers to nrf_drv_uart.o(.bss) for m_cb
    nrf_drv_uart.o(i.nrf_drv_uart_errorsrc_get) refers to nrf_drv_uart.o(i.nrf_uarte_event_clear) for nrf_uarte_event_clear
    nrf_drv_uart.o(i.nrf_drv_uart_errorsrc_get) refers to nrf_drv_uart.o(i.nrf_uarte_errorsrc_get_and_clear) for nrf_uarte_errorsrc_get_and_clear
    nrf_drv_uart.o(i.nrf_drv_uart_errorsrc_get) refers to nrf_drv_uart.o(i.nrf_uart_event_clear) for nrf_uart_event_clear
    nrf_drv_uart.o(i.nrf_drv_uart_errorsrc_get) refers to nrf_drv_uart.o(i.nrf_uart_errorsrc_get_and_clear) for nrf_uart_errorsrc_get_and_clear
    nrf_drv_uart.o(i.nrf_drv_uart_errorsrc_get) refers to nrf_drv_uart.o(.bss) for m_cb
    nrf_drv_uart.o(i.nrf_drv_uart_init) refers to nrf_drv_uart.o(i.apply_config) for apply_config
    nrf_drv_uart.o(i.nrf_drv_uart_init) refers to nrf_drv_uart.o(i.interrupts_enable) for interrupts_enable
    nrf_drv_uart.o(i.nrf_drv_uart_init) refers to nrf_drv_uart.o(.bss) for m_cb
    nrf_drv_uart.o(i.nrf_drv_uart_rx) refers to nrf_drv_uart.o(i.nrf_drv_is_in_RAM) for nrf_drv_is_in_RAM
    nrf_drv_uart.o(i.nrf_drv_uart_rx) refers to nrf_drv_uart.o(i.nrf_uarte_int_disable) for nrf_uarte_int_disable
    nrf_drv_uart.o(i.nrf_drv_uart_rx) refers to nrf_drv_uart.o(i.nrf_uart_int_disable) for nrf_uart_int_disable
    nrf_drv_uart.o(i.nrf_drv_uart_rx) refers to nrf_drv_uart.o(i.nrf_uarte_int_enable) for nrf_uarte_int_enable
    nrf_drv_uart.o(i.nrf_drv_uart_rx) refers to nrf_drv_uart.o(i.nrf_uart_int_enable) for nrf_uart_int_enable
    nrf_drv_uart.o(i.nrf_drv_uart_rx) refers to nrf_drv_uart.o(i.nrf_drv_uart_rx_for_uarte) for nrf_drv_uart_rx_for_uarte
    nrf_drv_uart.o(i.nrf_drv_uart_rx) refers to nrf_drv_uart.o(i.nrf_drv_uart_rx_for_uart) for nrf_drv_uart_rx_for_uart
    nrf_drv_uart.o(i.nrf_drv_uart_rx) refers to nrf_drv_uart.o(.bss) for m_cb
    nrf_drv_uart.o(i.nrf_drv_uart_rx_abort) refers to nrf_drv_uart.o(i.nrf_uarte_task_trigger) for nrf_uarte_task_trigger
    nrf_drv_uart.o(i.nrf_drv_uart_rx_abort) refers to nrf_drv_uart.o(i.nrf_uart_int_disable) for nrf_uart_int_disable
    nrf_drv_uart.o(i.nrf_drv_uart_rx_abort) refers to nrf_drv_uart.o(i.nrf_uart_task_trigger) for nrf_uart_task_trigger
    nrf_drv_uart.o(i.nrf_drv_uart_rx_abort) refers to nrf_drv_uart.o(.bss) for m_cb
    nrf_drv_uart.o(i.nrf_drv_uart_rx_disable) refers to nrf_drv_uart.o(i.nrf_uart_task_trigger) for nrf_uart_task_trigger
    nrf_drv_uart.o(i.nrf_drv_uart_rx_disable) refers to nrf_drv_uart.o(.bss) for m_cb
    nrf_drv_uart.o(i.nrf_drv_uart_rx_enable) refers to nrf_drv_uart.o(i.rx_enable) for rx_enable
    nrf_drv_uart.o(i.nrf_drv_uart_rx_enable) refers to nrf_drv_uart.o(.bss) for m_cb
    nrf_drv_uart.o(i.nrf_drv_uart_rx_for_uart) refers to nrf_drv_uart.o(i.rx_enable) for rx_enable
    nrf_drv_uart.o(i.nrf_drv_uart_rx_for_uart) refers to nrf_drv_uart.o(i.nrf_uart_event_clear) for nrf_uart_event_clear
    nrf_drv_uart.o(i.nrf_drv_uart_rx_for_uart) refers to nrf_drv_uart.o(i.nrf_uart_event_check) for nrf_uart_event_check
    nrf_drv_uart.o(i.nrf_drv_uart_rx_for_uart) refers to nrf_drv_uart.o(i.rx_byte) for rx_byte
    nrf_drv_uart.o(i.nrf_drv_uart_rx_for_uart) refers to nrf_drv_uart.o(i.nrf_uart_task_trigger) for nrf_uart_task_trigger
    nrf_drv_uart.o(i.nrf_drv_uart_rx_for_uart) refers to nrf_drv_uart.o(i.nrf_uart_int_enable) for nrf_uart_int_enable
    nrf_drv_uart.o(i.nrf_drv_uart_rx_for_uart) refers to nrf_drv_uart.o(.bss) for m_cb
    nrf_drv_uart.o(i.nrf_drv_uart_rx_for_uarte) refers to nrf_drv_uart.o(i.nrf_uarte_event_clear) for nrf_uarte_event_clear
    nrf_drv_uart.o(i.nrf_drv_uart_rx_for_uarte) refers to nrf_drv_uart.o(i.nrf_uarte_task_trigger) for nrf_uarte_task_trigger
    nrf_drv_uart.o(i.nrf_drv_uart_rx_for_uarte) refers to nrf_drv_uart.o(i.nrf_uarte_event_check) for nrf_uarte_event_check
    nrf_drv_uart.o(i.nrf_drv_uart_rx_for_uarte) refers to nrf_drv_uart.o(i.nrf_uarte_int_enable) for nrf_uarte_int_enable
    nrf_drv_uart.o(i.nrf_drv_uart_rx_for_uarte) refers to nrf_drv_uart.o(.bss) for m_cb
    nrf_drv_uart.o(i.nrf_drv_uart_rx_ready) refers to nrf_drv_uart.o(i.nrf_uarte_event_check) for nrf_uarte_event_check
    nrf_drv_uart.o(i.nrf_drv_uart_rx_ready) refers to nrf_drv_uart.o(i.nrf_uart_event_check) for nrf_uart_event_check
    nrf_drv_uart.o(i.nrf_drv_uart_rx_ready) refers to nrf_drv_uart.o(.bss) for m_cb
    nrf_drv_uart.o(i.nrf_drv_uart_tx) refers to nrf_drv_uart.o(i.nrf_drv_is_in_RAM) for nrf_drv_is_in_RAM
    nrf_drv_uart.o(i.nrf_drv_uart_tx) refers to nrf_drv_uart.o(i.nrf_drv_uart_tx_in_progress) for nrf_drv_uart_tx_in_progress
    nrf_drv_uart.o(i.nrf_drv_uart_tx) refers to nrf_drv_uart.o(i.nrf_drv_uart_tx_for_uarte) for nrf_drv_uart_tx_for_uarte
    nrf_drv_uart.o(i.nrf_drv_uart_tx) refers to nrf_drv_uart.o(i.nrf_drv_uart_tx_for_uart) for nrf_drv_uart_tx_for_uart
    nrf_drv_uart.o(i.nrf_drv_uart_tx) refers to nrf_drv_uart.o(.bss) for m_cb
    nrf_drv_uart.o(i.nrf_drv_uart_tx_abort) refers to nrf_drv_uart.o(i.nrf_uarte_event_clear) for nrf_uarte_event_clear
    nrf_drv_uart.o(i.nrf_drv_uart_tx_abort) refers to nrf_drv_uart.o(i.nrf_uarte_task_trigger) for nrf_uarte_task_trigger
    nrf_drv_uart.o(i.nrf_drv_uart_tx_abort) refers to nrf_drv_uart.o(i.nrf_uarte_event_check) for nrf_uarte_event_check
    nrf_drv_uart.o(i.nrf_drv_uart_tx_abort) refers to nrf_drv_uart.o(i.nrf_uart_task_trigger) for nrf_uart_task_trigger
    nrf_drv_uart.o(i.nrf_drv_uart_tx_abort) refers to nrf_drv_uart.o(i.tx_done_event) for tx_done_event
    nrf_drv_uart.o(i.nrf_drv_uart_tx_abort) refers to nrf_drv_uart.o(.bss) for m_cb
    nrf_drv_uart.o(i.nrf_drv_uart_tx_for_uart) refers to nrf_drv_uart.o(i.nrf_uart_event_clear) for nrf_uart_event_clear
    nrf_drv_uart.o(i.nrf_drv_uart_tx_for_uart) refers to nrf_drv_uart.o(i.nrf_uart_task_trigger) for nrf_uart_task_trigger
    nrf_drv_uart.o(i.nrf_drv_uart_tx_for_uart) refers to nrf_drv_uart.o(i.tx_byte) for tx_byte
    nrf_drv_uart.o(i.nrf_drv_uart_tx_for_uart) refers to nrf_drv_uart.o(i.nrf_uart_event_check) for nrf_uart_event_check
    nrf_drv_uart.o(i.nrf_drv_uart_tx_for_uart) refers to nrf_drv_uart.o(.bss) for m_cb
    nrf_drv_uart.o(i.nrf_drv_uart_tx_for_uarte) refers to nrf_drv_uart.o(i.nrf_uarte_event_clear) for nrf_uarte_event_clear
    nrf_drv_uart.o(i.nrf_drv_uart_tx_for_uarte) refers to nrf_drv_uart.o(i.nrf_uarte_task_trigger) for nrf_uarte_task_trigger
    nrf_drv_uart.o(i.nrf_drv_uart_tx_for_uarte) refers to nrf_drv_uart.o(i.nrf_uarte_event_check) for nrf_uarte_event_check
    nrf_drv_uart.o(i.nrf_drv_uart_tx_for_uarte) refers to nrf_drv_uart.o(.bss) for m_cb
    nrf_drv_uart.o(i.nrf_drv_uart_tx_in_progress) refers to nrf_drv_uart.o(.bss) for m_cb
    nrf_drv_uart.o(i.nrf_drv_uart_uninit) refers to nrf_drv_uart.o(i.nrf_uarte_int_disable) for nrf_uarte_int_disable
    nrf_drv_uart.o(i.nrf_drv_uart_uninit) refers to nrf_drv_uart.o(i.nrf_drv_get_IRQn) for nrf_drv_get_IRQn
    nrf_drv_uart.o(i.nrf_drv_uart_uninit) refers to nrf_drv_uart.o(i.nrf_drv_common_irq_disable) for nrf_drv_common_irq_disable
    nrf_drv_uart.o(i.nrf_drv_uart_uninit) refers to nrf_drv_uart.o(i.nrf_uart_int_disable) for nrf_uart_int_disable
    nrf_drv_uart.o(i.nrf_drv_uart_uninit) refers to nrf_drv_uart.o(i.pins_to_default) for pins_to_default
    nrf_drv_uart.o(i.nrf_drv_uart_uninit) refers to nrf_drv_uart.o(.bss) for m_cb
    nrf_drv_uart.o(i.nrf_gpio_cfg) refers to nrf_drv_uart.o(i.nrf_gpio_pin_port_decode) for nrf_gpio_pin_port_decode
    nrf_drv_uart.o(i.nrf_gpio_cfg_default) refers to nrf_drv_uart.o(i.nrf_gpio_cfg) for nrf_gpio_cfg
    nrf_drv_uart.o(i.nrf_gpio_cfg_input) refers to nrf_drv_uart.o(i.nrf_gpio_cfg) for nrf_gpio_cfg
    nrf_drv_uart.o(i.nrf_gpio_cfg_output) refers to nrf_drv_uart.o(i.nrf_gpio_cfg) for nrf_gpio_cfg
    nrf_drv_uart.o(i.nrf_gpio_pin_set) refers to nrf_drv_uart.o(i.nrf_gpio_pin_port_decode) for nrf_gpio_pin_port_decode
    nrf_drv_uart.o(i.pins_to_default) refers to nrf_drv_uart.o(i.nrf_uarte_txrx_pins_set) for nrf_uarte_txrx_pins_set
    nrf_drv_uart.o(i.pins_to_default) refers to nrf_drv_uart.o(i.nrf_uarte_hwfc_pins_set) for nrf_uarte_hwfc_pins_set
    nrf_drv_uart.o(i.pins_to_default) refers to nrf_drv_uart.o(i.nrf_uart_txrx_pins_set) for nrf_uart_txrx_pins_set
    nrf_drv_uart.o(i.pins_to_default) refers to nrf_drv_uart.o(i.nrf_uart_hwfc_pins_set) for nrf_uart_hwfc_pins_set
    nrf_drv_uart.o(i.pins_to_default) refers to nrf_drv_uart.o(i.nrf_gpio_cfg_default) for nrf_gpio_cfg_default
    nrf_drv_uart.o(i.pins_to_default) refers to nrf_drv_uart.o(.bss) for m_cb
    nrf_drv_uart.o(i.rx_byte) refers to nrf_drv_uart.o(i.nrf_uart_event_clear) for nrf_uart_event_clear
    nrf_drv_uart.o(i.rx_enable) refers to nrf_drv_uart.o(i.nrf_uart_event_clear) for nrf_uart_event_clear
    nrf_drv_uart.o(i.rx_enable) refers to nrf_drv_uart.o(i.nrf_uart_task_trigger) for nrf_uart_task_trigger
    nrf_drv_uart.o(i.tx_byte) refers to nrf_drv_uart.o(i.nrf_uart_event_clear) for nrf_uart_event_clear
    nrf_drv_uart.o(i.uart_irq_handler) refers to nrf_drv_uart.o(i.nrf_uart_int_enable_check) for nrf_uart_int_enable_check
    nrf_drv_uart.o(i.uart_irq_handler) refers to nrf_drv_uart.o(i.nrf_uart_event_check) for nrf_uart_event_check
    nrf_drv_uart.o(i.uart_irq_handler) refers to nrf_drv_uart.o(i.nrf_uart_event_clear) for nrf_uart_event_clear
    nrf_drv_uart.o(i.uart_irq_handler) refers to nrf_drv_uart.o(i.nrf_uart_int_disable) for nrf_uart_int_disable
    nrf_drv_uart.o(i.uart_irq_handler) refers to nrf_drv_uart.o(i.nrf_uart_task_trigger) for nrf_uart_task_trigger
    nrf_drv_uart.o(i.uart_irq_handler) refers to nrf_drv_uart.o(i.nrf_uart_errorsrc_get_and_clear) for nrf_uart_errorsrc_get_and_clear
    nrf_drv_uart.o(i.uart_irq_handler) refers to nrf_drv_uart.o(i.rx_byte) for rx_byte
    nrf_drv_uart.o(i.uart_irq_handler) refers to nrf_drv_uart.o(i.rx_done_event) for rx_done_event
    nrf_drv_uart.o(i.uart_irq_handler) refers to nrf_drv_uart.o(i.tx_byte) for tx_byte
    nrf_drv_uart.o(i.uart_irq_handler) refers to nrf_drv_uart.o(i.tx_done_event) for tx_done_event
    nrf_drv_uart.o(i.uarte_irq_handler) refers to nrf_drv_uart.o(i.nrf_uarte_event_check) for nrf_uarte_event_check
    nrf_drv_uart.o(i.uarte_irq_handler) refers to nrf_drv_uart.o(i.nrf_uarte_event_clear) for nrf_uarte_event_clear
    nrf_drv_uart.o(i.uarte_irq_handler) refers to nrf_drv_uart.o(i.nrf_uarte_errorsrc_get_and_clear) for nrf_uarte_errorsrc_get_and_clear
    nrf_drv_uart.o(i.uarte_irq_handler) refers to nrf_drv_uart.o(i.nrf_uarte_rx_amount_get) for nrf_uarte_rx_amount_get
    nrf_drv_uart.o(i.uarte_irq_handler) refers to nrf_drv_uart.o(i.rx_done_event) for rx_done_event
    nrf_drv_uart.o(i.uarte_irq_handler) refers to nrf_drv_uart.o(i.tx_done_event) for tx_done_event
    nrf_drv_uart.o(log_const_data) refers to nrf_drv_uart.o(.conststrlit) for .conststrlit
    app_button.o(i.app_button_disable) refers to nrf_drv_gpiote.o(i.nrf_drv_gpiote_in_event_disable) for nrf_drv_gpiote_in_event_disable
    app_button.o(i.app_button_disable) refers to app_timer.o(i.app_timer_stop) for app_timer_stop
    app_button.o(i.app_button_disable) refers to app_button.o(.data) for mp_buttons
    app_button.o(i.app_button_disable) refers to app_button.o(.constdata) for m_detection_delay_timer_id
    app_button.o(i.app_button_enable) refers to nrf_drv_gpiote.o(i.nrf_drv_gpiote_in_event_enable) for nrf_drv_gpiote_in_event_enable
    app_button.o(i.app_button_enable) refers to app_button.o(.data) for mp_buttons
    app_button.o(i.app_button_init) refers to nrf_drv_gpiote.o(i.nrf_drv_gpiote_is_init) for nrf_drv_gpiote_is_init
    app_button.o(i.app_button_init) refers to nrf_drv_gpiote.o(i.nrf_drv_gpiote_init) for nrf_drv_gpiote_init
    app_button.o(i.app_button_init) refers to nrf_drv_gpiote.o(i.nrf_drv_gpiote_in_init) for nrf_drv_gpiote_in_init
    app_button.o(i.app_button_init) refers to app_timer.o(i.app_timer_create) for app_timer_create
    app_button.o(i.app_button_init) refers to app_button.o(.data) for mp_buttons
    app_button.o(i.app_button_init) refers to app_button.o(.constdata) for .constdata
    app_button.o(i.app_button_init) refers to app_button.o(i.gpiote_event_handler) for gpiote_event_handler
    app_button.o(i.app_button_init) refers to app_button.o(i.detection_delay_timeout_handler) for detection_delay_timeout_handler
    app_button.o(i.app_button_is_pushed) refers to nrf_drv_gpiote.o(i.nrf_drv_gpiote_in_is_set) for nrf_drv_gpiote_in_is_set
    app_button.o(i.app_button_is_pushed) refers to app_button.o(.data) for mp_buttons
    app_button.o(i.detection_delay_timeout_handler) refers to nrf_drv_gpiote.o(i.nrf_drv_gpiote_in_is_set) for nrf_drv_gpiote_in_is_set
    app_button.o(i.detection_delay_timeout_handler) refers to app_button.o(.data) for mp_buttons
    app_button.o(i.gpiote_event_handler) refers to app_timer.o(i.app_timer_stop) for app_timer_stop
    app_button.o(i.gpiote_event_handler) refers to nrf_drv_gpiote.o(i.nrf_drv_gpiote_in_is_set) for nrf_drv_gpiote_in_is_set
    app_button.o(i.gpiote_event_handler) refers to app_timer.o(i.app_timer_start) for app_timer_start
    app_button.o(i.gpiote_event_handler) refers to app_button.o(.constdata) for m_detection_delay_timer_id
    app_button.o(i.gpiote_event_handler) refers to app_button.o(.data) for m_pin_transition
    app_button.o(.constdata) refers to app_button.o(.bss) for m_detection_delay_timer_id_data
    app_error.o(i.app_error_handler) refers to app_error_weak.o(i.app_error_fault_handler) for app_error_fault_handler
    app_error.o(i.app_error_handler_bare) refers to app_error_weak.o(i.app_error_fault_handler) for app_error_fault_handler
    app_error.o(i.app_error_save_and_stop) refers to app_error.o(.bss) for m_error_data
    app_error_weak.o(i.app_error_fault_handler) refers to nrf_log_frontend.o(i.nrf_log_panic) for nrf_log_panic
    app_error_weak.o(i.app_error_fault_handler) refers to nrf_log_frontend.o(i.nrf_log_frontend_dequeue) for nrf_log_frontend_dequeue
    app_error_weak.o(i.app_error_fault_handler) refers to nrf_log_frontend.o(i.nrf_log_frontend_std_0) for nrf_log_frontend_std_0
    app_error_weak.o(i.app_error_fault_handler) refers to nrf_log_frontend.o(log_dynamic_data) for m_nrf_log_app_logs_data_dynamic
    app_fifo.o(i.app_fifo_get) refers to app_fifo.o(i.fifo_length) for fifo_length
    app_fifo.o(i.app_fifo_get) refers to app_fifo.o(i.fifo_get) for fifo_get
    app_fifo.o(i.app_fifo_peek) refers to app_fifo.o(i.fifo_length) for fifo_length
    app_fifo.o(i.app_fifo_peek) refers to app_fifo.o(i.fifo_peek) for fifo_peek
    app_fifo.o(i.app_fifo_put) refers to app_fifo.o(i.fifo_length) for fifo_length
    app_fifo.o(i.app_fifo_put) refers to app_fifo.o(i.fifo_put) for fifo_put
    app_fifo.o(i.app_fifo_read) refers to app_fifo.o(i.fifo_length) for fifo_length
    app_fifo.o(i.app_fifo_read) refers to app_fifo.o(i.fifo_get) for fifo_get
    app_fifo.o(i.app_fifo_write) refers to app_fifo.o(i.fifo_length) for fifo_length
    app_fifo.o(i.app_fifo_write) refers to app_fifo.o(i.fifo_put) for fifo_put
    app_fifo.o(i.fifo_get) refers to app_fifo.o(i.fifo_peek) for fifo_peek
    app_scheduler.o(i.app_sched_event_put) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    app_scheduler.o(i.app_sched_event_put) refers to app_scheduler.o(i.next_index) for next_index
    app_scheduler.o(i.app_sched_event_put) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    app_scheduler.o(i.app_sched_event_put) refers to memcpya.o(.text) for __aeabi_memcpy
    app_scheduler.o(i.app_sched_event_put) refers to app_scheduler.o(.data) for m_queue_event_size
    app_scheduler.o(i.app_sched_execute) refers to app_scheduler.o(i.next_index) for next_index
    app_scheduler.o(i.app_sched_execute) refers to app_scheduler.o(.data) for m_queue_start_index
    app_scheduler.o(i.app_sched_init) refers to app_scheduler.o(.data) for m_queue_event_headers
    app_scheduler.o(i.app_sched_queue_space_get) refers to app_scheduler.o(.data) for m_queue_start_index
    app_scheduler.o(i.next_index) refers to app_scheduler.o(.data) for m_queue_size
    app_timer.o(i.RTC1_IRQHandler) refers to app_timer.o(i.timer_timeouts_check) for timer_timeouts_check
    app_timer.o(i.SWI0_EGU0_IRQHandler) refers to app_timer.o(i.timer_list_handler) for timer_list_handler
    app_timer.o(i.app_timer_cnt_diff_compute) refers to app_timer.o(i.ticks_diff_get) for ticks_diff_get
    app_timer.o(i.app_timer_cnt_get) refers to app_timer.o(i.rtc1_counter_get) for rtc1_counter_get
    app_timer.o(i.app_timer_create) refers to app_timer.o(.bss) for m_op_queue
    app_timer.o(i.app_timer_init) refers to app_timer.o(i.rtc1_stop) for rtc1_stop
    app_timer.o(i.app_timer_init) refers to app_timer.o(i.NVIC_ClearPendingIRQ) for NVIC_ClearPendingIRQ
    app_timer.o(i.app_timer_init) refers to app_timer.o(i.NVIC_SetPriority) for NVIC_SetPriority
    app_timer.o(i.app_timer_init) refers to app_timer.o(i.NVIC_EnableIRQ) for NVIC_EnableIRQ
    app_timer.o(i.app_timer_init) refers to app_timer.o(i.rtc1_init) for rtc1_init
    app_timer.o(i.app_timer_init) refers to app_timer.o(i.rtc1_counter_get) for rtc1_counter_get
    app_timer.o(i.app_timer_init) refers to app_timer.o(.bss) for m_op_queue
    app_timer.o(i.app_timer_init) refers to app_timer.o(.data) for mp_timer_id_head
    app_timer.o(i.app_timer_start) refers to app_timer.o(i.timer_start_op_schedule) for timer_start_op_schedule
    app_timer.o(i.app_timer_start) refers to app_timer.o(.bss) for m_op_queue
    app_timer.o(i.app_timer_stop) refers to app_timer.o(i.timer_stop_op_schedule) for timer_stop_op_schedule
    app_timer.o(i.app_timer_stop) refers to app_timer.o(.bss) for m_op_queue
    app_timer.o(i.app_timer_stop_all) refers to app_timer.o(i.timer_stop_op_schedule) for timer_stop_op_schedule
    app_timer.o(i.app_timer_stop_all) refers to app_timer.o(.bss) for m_op_queue
    app_timer.o(i.compare_reg_update) refers to app_timer.o(i.rtc1_counter_get) for rtc1_counter_get
    app_timer.o(i.compare_reg_update) refers to app_timer.o(i.ticks_diff_get) for ticks_diff_get
    app_timer.o(i.compare_reg_update) refers to app_timer.o(i.rtc1_start) for rtc1_start
    app_timer.o(i.compare_reg_update) refers to app_timer.o(i.rtc1_compare0_set) for rtc1_compare0_set
    app_timer.o(i.compare_reg_update) refers to app_timer.o(i.nrf_delay_us) for nrf_delay_us
    app_timer.o(i.compare_reg_update) refers to app_timer.o(i.timer_timeouts_check_sched) for timer_timeouts_check_sched
    app_timer.o(i.compare_reg_update) refers to app_timer.o(i.rtc1_stop) for rtc1_stop
    app_timer.o(i.compare_reg_update) refers to app_timer.o(.data) for mp_timer_id_head
    app_timer.o(i.elapsed_ticks_acquire) refers to app_timer.o(.data) for m_ticks_elapsed_q_read_ind
    app_timer.o(i.expired_timers_handler) refers to app_timer.o(.data) for mp_timer_id_head
    app_timer.o(i.list_insertions_handler) refers to app_timer.o(i.timer_list_remove) for timer_list_remove
    app_timer.o(i.list_insertions_handler) refers to app_timer.o(i.ticks_diff_get) for ticks_diff_get
    app_timer.o(i.list_insertions_handler) refers to app_timer.o(i.timer_list_insert) for timer_list_insert
    app_timer.o(i.list_insertions_handler) refers to app_timer.o(.data) for mp_timer_id_head
    app_timer.o(i.list_insertions_handler) refers to app_timer.o(.bss) for m_op_queue
    app_timer.o(i.nrf_delay_us) refers to system_nrf52840.o(.data) for SystemCoreClock
    app_timer.o(i.rtc1_init) refers to app_timer.o(i.NVIC_SetPriority) for NVIC_SetPriority
    app_timer.o(i.rtc1_start) refers to app_timer.o(i.NVIC_ClearPendingIRQ) for NVIC_ClearPendingIRQ
    app_timer.o(i.rtc1_start) refers to app_timer.o(i.NVIC_EnableIRQ) for NVIC_EnableIRQ
    app_timer.o(i.rtc1_start) refers to app_timer.o(i.nrf_delay_us) for nrf_delay_us
    app_timer.o(i.rtc1_start) refers to app_timer.o(.data) for m_rtc1_running
    app_timer.o(i.rtc1_stop) refers to app_timer.o(i.nrf_delay_us) for nrf_delay_us
    app_timer.o(i.rtc1_stop) refers to app_timer.o(.data) for m_ticks_latest
    app_timer.o(i.timer_list_handler) refers to app_timer.o(i.elapsed_ticks_acquire) for elapsed_ticks_acquire
    app_timer.o(i.timer_list_handler) refers to app_timer.o(i.expired_timers_handler) for expired_timers_handler
    app_timer.o(i.timer_list_handler) refers to app_timer.o(i.list_insertions_handler) for list_insertions_handler
    app_timer.o(i.timer_list_handler) refers to app_timer.o(i.compare_reg_update) for compare_reg_update
    app_timer.o(i.timer_list_handler) refers to app_timer.o(.data) for m_ticks_latest
    app_timer.o(i.timer_list_handler_sched) refers to app_timer.o(i.NVIC_SetPendingIRQ) for NVIC_SetPendingIRQ
    app_timer.o(i.timer_list_insert) refers to app_timer.o(.data) for mp_timer_id_head
    app_timer.o(i.timer_list_remove) refers to app_timer.o(i.nrf_delay_us) for nrf_delay_us
    app_timer.o(i.timer_list_remove) refers to app_timer.o(.data) for mp_timer_id_head
    app_timer.o(i.timer_start_op_schedule) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    app_timer.o(i.timer_start_op_schedule) refers to app_timer.o(i.user_op_alloc) for user_op_alloc
    app_timer.o(i.timer_start_op_schedule) refers to app_timer.o(i.rtc1_counter_get) for rtc1_counter_get
    app_timer.o(i.timer_start_op_schedule) refers to app_timer.o(i.user_op_enque) for user_op_enque
    app_timer.o(i.timer_start_op_schedule) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    app_timer.o(i.timer_start_op_schedule) refers to app_timer.o(i.timer_list_handler_sched) for timer_list_handler_sched
    app_timer.o(i.timer_stop_op_schedule) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    app_timer.o(i.timer_stop_op_schedule) refers to app_timer.o(i.user_op_alloc) for user_op_alloc
    app_timer.o(i.timer_stop_op_schedule) refers to app_timer.o(i.user_op_enque) for user_op_enque
    app_timer.o(i.timer_stop_op_schedule) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    app_timer.o(i.timer_stop_op_schedule) refers to app_timer.o(i.timer_list_handler_sched) for timer_list_handler_sched
    app_timer.o(i.timer_timeouts_check) refers to app_timer.o(i.rtc1_counter_get) for rtc1_counter_get
    app_timer.o(i.timer_timeouts_check) refers to app_timer.o(i.ticks_diff_get) for ticks_diff_get
    app_timer.o(i.timer_timeouts_check) refers to app_timer.o(i.timeout_handler_exec) for timeout_handler_exec
    app_timer.o(i.timer_timeouts_check) refers to app_timer.o(i.timer_list_handler_sched) for timer_list_handler_sched
    app_timer.o(i.timer_timeouts_check) refers to app_timer.o(.data) for mp_timer_id_head
    app_timer.o(i.timer_timeouts_check_sched) refers to app_timer.o(i.NVIC_SetPendingIRQ) for NVIC_SetPendingIRQ
    app_timer.o(i.user_op_alloc) refers to app_timer.o(.bss) for m_op_queue
    app_timer.o(i.user_op_enque) refers to app_timer.o(.bss) for m_op_queue
    app_uart_fifo.o(i.app_uart_close) refers to nrf_drv_uart.o(i.nrf_drv_uart_uninit) for nrf_drv_uart_uninit
    app_uart_fifo.o(i.app_uart_close) refers to app_uart_fifo.o(.data) for app_uart_inst
    app_uart_fifo.o(i.app_uart_flush) refers to app_fifo.o(i.app_fifo_flush) for app_fifo_flush
    app_uart_fifo.o(i.app_uart_flush) refers to app_uart_fifo.o(.bss) for m_rx_fifo
    app_uart_fifo.o(i.app_uart_get) refers to app_fifo.o(i.app_fifo_get) for app_fifo_get
    app_uart_fifo.o(i.app_uart_get) refers to nrf_drv_uart.o(i.nrf_drv_uart_rx) for nrf_drv_uart_rx
    app_uart_fifo.o(i.app_uart_get) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    app_uart_fifo.o(i.app_uart_get) refers to app_uart_fifo.o(.data) for m_rx_ovf
    app_uart_fifo.o(i.app_uart_get) refers to app_uart_fifo.o(.bss) for m_rx_fifo
    app_uart_fifo.o(i.app_uart_init) refers to app_fifo.o(i.app_fifo_init) for app_fifo_init
    app_uart_fifo.o(i.app_uart_init) refers to memcpya.o(.text) for __aeabi_memcpy4
    app_uart_fifo.o(i.app_uart_init) refers to nrf_drv_uart.o(i.nrf_drv_uart_init) for nrf_drv_uart_init
    app_uart_fifo.o(i.app_uart_init) refers to nrf_drv_uart.o(i.nrf_drv_uart_rx_enable) for nrf_drv_uart_rx_enable
    app_uart_fifo.o(i.app_uart_init) refers to nrf_drv_uart.o(i.nrf_drv_uart_rx) for nrf_drv_uart_rx
    app_uart_fifo.o(i.app_uart_init) refers to app_uart_fifo.o(.data) for m_event_handler
    app_uart_fifo.o(i.app_uart_init) refers to app_uart_fifo.o(.bss) for m_rx_fifo
    app_uart_fifo.o(i.app_uart_init) refers to app_uart_fifo.o(.constdata) for .constdata
    app_uart_fifo.o(i.app_uart_init) refers to app_uart_fifo.o(i.uart_event_handler) for uart_event_handler
    app_uart_fifo.o(i.app_uart_put) refers to app_fifo.o(i.app_fifo_put) for app_fifo_put
    app_uart_fifo.o(i.app_uart_put) refers to nrf_drv_uart.o(i.nrf_drv_uart_tx_in_progress) for nrf_drv_uart_tx_in_progress
    app_uart_fifo.o(i.app_uart_put) refers to app_fifo.o(i.app_fifo_get) for app_fifo_get
    app_uart_fifo.o(i.app_uart_put) refers to nrf_drv_uart.o(i.nrf_drv_uart_tx) for nrf_drv_uart_tx
    app_uart_fifo.o(i.app_uart_put) refers to app_uart_fifo.o(.bss) for m_tx_fifo
    app_uart_fifo.o(i.app_uart_put) refers to app_uart_fifo.o(.data) for app_uart_inst
    app_uart_fifo.o(i.uart_event_handler) refers to app_fifo.o(i.app_fifo_put) for app_fifo_put
    app_uart_fifo.o(i.uart_event_handler) refers to app_uart_fifo.o(i.fifo_length) for fifo_length
    app_uart_fifo.o(i.uart_event_handler) refers to nrf_drv_uart.o(i.nrf_drv_uart_rx) for nrf_drv_uart_rx
    app_uart_fifo.o(i.uart_event_handler) refers to app_fifo.o(i.app_fifo_get) for app_fifo_get
    app_uart_fifo.o(i.uart_event_handler) refers to nrf_drv_uart.o(i.nrf_drv_uart_tx) for nrf_drv_uart_tx
    app_uart_fifo.o(i.uart_event_handler) refers to app_uart_fifo.o(.bss) for m_rx_fifo
    app_uart_fifo.o(i.uart_event_handler) refers to app_uart_fifo.o(.data) for m_event_handler
    app_util_platform.o(i.app_util_critical_region_enter) refers to app_util_platform.o(i.sd_nvic_critical_region_enter) for sd_nvic_critical_region_enter
    app_util_platform.o(i.app_util_critical_region_exit) refers to app_util_platform.o(i.__sd_nvic_irq_disable) for __sd_nvic_irq_disable
    app_util_platform.o(i.app_util_critical_region_exit) refers to app_util_platform.o(.bss) for nrf_nvic_state
    app_util_platform.o(i.app_util_disable_irq) refers to app_util_platform.o(.data) for m_in_critical_region
    app_util_platform.o(i.app_util_enable_irq) refers to app_util_platform.o(.data) for m_in_critical_region
    app_util_platform.o(i.sd_nvic_critical_region_enter) refers to app_util_platform.o(i.__sd_nvic_irq_disable) for __sd_nvic_irq_disable
    app_util_platform.o(i.sd_nvic_critical_region_enter) refers to app_util_platform.o(.bss) for nrf_nvic_state
    nrf_assert.o(i.assert_nrf_callback) refers to app_error_weak.o(i.app_error_fault_handler) for app_error_fault_handler
    nrf_atfifo.o(i.nrf_atfifo_alloc_put) refers to nrf_atfifo.o(i.nrf_atfifo_item_alloc) for nrf_atfifo_item_alloc
    nrf_atfifo.o(i.nrf_atfifo_alloc_put) refers to memcpya.o(.text) for __aeabi_memcpy
    nrf_atfifo.o(i.nrf_atfifo_alloc_put) refers to nrf_atfifo.o(i.nrf_atfifo_item_put) for nrf_atfifo_item_put
    nrf_atfifo.o(i.nrf_atfifo_clear) refers to nrf_atfifo.o(.emb_text) for __asm___12_nrf_atfifo_c_51f461e1__nrf_atfifo_space_clear
    nrf_atfifo.o(i.nrf_atfifo_get_free) refers to nrf_atfifo.o(i.nrf_atfifo_item_get) for nrf_atfifo_item_get
    nrf_atfifo.o(i.nrf_atfifo_get_free) refers to memcpya.o(.text) for __aeabi_memcpy
    nrf_atfifo.o(i.nrf_atfifo_get_free) refers to nrf_atfifo.o(i.nrf_atfifo_item_free) for nrf_atfifo_item_free
    nrf_atfifo.o(i.nrf_atfifo_item_alloc) refers to nrf_atfifo.o(.emb_text) for __asm___12_nrf_atfifo_c_51f461e1__nrf_atfifo_wspace_req
    nrf_atfifo.o(i.nrf_atfifo_item_free) refers to nrf_atfifo.o(.emb_text) for __asm___12_nrf_atfifo_c_51f461e1__nrf_atfifo_rspace_close
    nrf_atfifo.o(i.nrf_atfifo_item_get) refers to nrf_atfifo.o(.emb_text) for __asm___12_nrf_atfifo_c_51f461e1__nrf_atfifo_rspace_req
    nrf_atfifo.o(i.nrf_atfifo_item_put) refers to nrf_atfifo.o(.emb_text) for __asm___12_nrf_atfifo_c_51f461e1__nrf_atfifo_wspace_close
    nrf_balloc.o(i.nrf_balloc_alloc) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    nrf_balloc.o(i.nrf_balloc_alloc) refers to nrf_balloc.o(i.nrf_balloc_idx2block) for nrf_balloc_idx2block
    nrf_balloc.o(i.nrf_balloc_alloc) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    nrf_balloc.o(i.nrf_balloc_free) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    nrf_balloc.o(i.nrf_balloc_free) refers to nrf_balloc.o(i.nrf_balloc_block2idx) for nrf_balloc_block2idx
    nrf_balloc.o(i.nrf_balloc_free) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    nrf_balloc.o(log_const_data) refers to nrf_balloc.o(.conststrlit) for .conststrlit
    nrf_fprintf.o(i.nrf_fprintf) refers to nrf_fprintf_format.o(i.nrf_fprintf_fmt) for nrf_fprintf_fmt
    nrf_fprintf_format.o(i.buffer_add) refers to nrf_fprintf.o(i.nrf_fprintf_buffer_flush) for nrf_fprintf_buffer_flush
    nrf_fprintf_format.o(i.int_print) refers to nrf_fprintf_format.o(i.buffer_add) for buffer_add
    nrf_fprintf_format.o(i.int_print) refers to nrf_fprintf_format.o(i.unsigned_print) for unsigned_print
    nrf_fprintf_format.o(i.nrf_fprintf_fmt) refers to nrf_fprintf_format.o(i.buffer_add) for buffer_add
    nrf_fprintf_format.o(i.nrf_fprintf_fmt) refers to nrf_fprintf_format.o(i.int_print) for int_print
    nrf_fprintf_format.o(i.nrf_fprintf_fmt) refers to nrf_fprintf_format.o(i.unsigned_print) for unsigned_print
    nrf_fprintf_format.o(i.nrf_fprintf_fmt) refers to nrf_fprintf_format.o(i.string_print) for string_print
    nrf_fprintf_format.o(i.nrf_fprintf_fmt) refers to nrf_fprintf.o(i.nrf_fprintf_buffer_flush) for nrf_fprintf_buffer_flush
    nrf_fprintf_format.o(i.string_print) refers to nrf_fprintf_format.o(i.buffer_add) for buffer_add
    nrf_fprintf_format.o(i.string_print) refers to strlen.o(.text) for strlen
    nrf_fprintf_format.o(i.unsigned_print) refers to nrf_fprintf_format.o(i.buffer_add) for buffer_add
    nrf_fprintf_format.o(i.unsigned_print) refers to nrf_fprintf_format.o(.constdata) for _aV2C
    nrf_memobj.o(i.memobj_op) refers to memcpya.o(.text) for __aeabi_memcpy
    nrf_memobj.o(i.nrf_memobj_alloc) refers to nrf_balloc.o(i.nrf_balloc_alloc) for nrf_balloc_alloc
    nrf_memobj.o(i.nrf_memobj_alloc) refers to nrf_memobj.o(i.nrf_memobj_free) for nrf_memobj_free
    nrf_memobj.o(i.nrf_memobj_free) refers to nrf_balloc.o(i.nrf_balloc_free) for nrf_balloc_free
    nrf_memobj.o(i.nrf_memobj_get) refers to nrf_memobj.o(.emb_text) for __asm___12_nrf_memobj_c_9bb9f865__nrf_atomic_internal_add
    nrf_memobj.o(i.nrf_memobj_pool_init) refers to nrf_balloc.o(i.nrf_balloc_init) for nrf_balloc_init
    nrf_memobj.o(i.nrf_memobj_put) refers to nrf_memobj.o(.emb_text) for __asm___12_nrf_memobj_c_9bb9f865__nrf_atomic_internal_sub
    nrf_memobj.o(i.nrf_memobj_put) refers to nrf_memobj.o(i.nrf_memobj_free) for nrf_memobj_free
    nrf_memobj.o(i.nrf_memobj_read) refers to nrf_memobj.o(i.memobj_op) for memobj_op
    nrf_memobj.o(i.nrf_memobj_write) refers to nrf_memobj.o(i.memobj_op) for memobj_op
    nrf_pwr_mgmt.o(i.nrf_pwr_mgmt_init) refers to nrf_section_iter.o(i.nrf_section_iter_init) for nrf_section_iter_init
    nrf_pwr_mgmt.o(i.nrf_pwr_mgmt_init) refers to nrf_pwr_mgmt.o(.data) for m_shutdown_started
    nrf_pwr_mgmt.o(i.nrf_pwr_mgmt_init) refers to nrf_pwr_mgmt.o(.constdata) for pwr_mgmt_data
    nrf_pwr_mgmt.o(i.nrf_pwr_mgmt_init) refers to nrf_pwr_mgmt.o(.bss) for m_handlers_iter
    nrf_pwr_mgmt.o(i.nrf_pwr_mgmt_run) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    nrf_pwr_mgmt.o(i.nrf_pwr_mgmt_run) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    nrf_pwr_mgmt.o(i.nrf_pwr_mgmt_run) refers to nrf_sdh.o(i.nrf_sdh_is_enabled) for nrf_sdh_is_enabled
    nrf_pwr_mgmt.o(i.nrf_pwr_mgmt_shutdown) refers to nrf_pwr_mgmt.o(.emb_text) for __asm___14_nrf_pwr_mgmt_c_f22138a6__nrf_atomic_internal_mov
    nrf_pwr_mgmt.o(i.nrf_pwr_mgmt_shutdown) refers to nrf_pwr_mgmt.o(i.nrf_mtx_unlock) for nrf_mtx_unlock
    nrf_pwr_mgmt.o(i.nrf_pwr_mgmt_shutdown) refers to nrf_pwr_mgmt.o(i.shutdown_process) for shutdown_process
    nrf_pwr_mgmt.o(i.nrf_pwr_mgmt_shutdown) refers to nrf_pwr_mgmt.o(.data) for m_sysoff_mtx
    nrf_pwr_mgmt.o(i.shutdown_process) refers to nrf_section_iter.o(i.nrf_section_iter_next) for nrf_section_iter_next
    nrf_pwr_mgmt.o(i.shutdown_process) refers to nrf_log_frontend.o(i.nrf_log_panic) for nrf_log_panic
    nrf_pwr_mgmt.o(i.shutdown_process) refers to nrf_log_frontend.o(i.nrf_log_frontend_dequeue) for nrf_log_frontend_dequeue
    nrf_pwr_mgmt.o(i.shutdown_process) refers to nrf_sdh.o(i.nrf_sdh_is_enabled) for nrf_sdh_is_enabled
    nrf_pwr_mgmt.o(i.shutdown_process) refers to nrf_pwr_mgmt.o(.bss) for m_handlers_iter
    nrf_pwr_mgmt.o(i.shutdown_process) refers to nrf_pwr_mgmt.o(.data) for m_pwr_mgmt_evt
    nrf_pwr_mgmt.o(log_const_data) refers to nrf_pwr_mgmt.o(.conststrlit) for .conststrlit
    nrf_section_iter.o(i.nrf_section_iter_init) refers to nrf_section_iter.o(i.nrf_section_iter_item_set) for nrf_section_iter_item_set
    nrf_section_iter.o(i.nrf_section_iter_next) refers to nrf_section_iter.o(i.nrf_section_iter_item_set) for nrf_section_iter_item_set
    nrf_strerror.o(i.nrf_strerror_find) refers to nrf_strerror.o(.constdata) for nrf_strerror_array
    nrf_strerror.o(i.nrf_strerror_get) refers to nrf_strerror.o(i.nrf_strerror_find) for nrf_strerror_find
    nrf_strerror.o(i.nrf_strerror_get) refers to nrf_strerror.o(.constdata) for m_unknown_str
    nrf_strerror.o(.constdata) refers to nrf_strerror.o(.conststring) for .conststring
    retarget.o(i.fgetc) refers to app_uart_fifo.o(i.app_uart_get) for app_uart_get
    retarget.o(i.fputc) refers to app_uart_fifo.o(i.app_uart_put) for app_uart_put
    nrf_log_backend_rtt.o(i.nrf_log_backend_rtt_init) refers to segger_rtt.o(i.SEGGER_RTT_Init) for SEGGER_RTT_Init
    nrf_log_backend_rtt.o(i.nrf_log_backend_rtt_put) refers to nrf_log_backend_serial.o(i.nrf_log_backend_serial_put) for nrf_log_backend_serial_put
    nrf_log_backend_rtt.o(i.nrf_log_backend_rtt_put) refers to nrf_log_backend_rtt.o(i.serial_tx) for serial_tx
    nrf_log_backend_rtt.o(i.nrf_log_backend_rtt_put) refers to nrf_log_backend_rtt.o(.bss) for m_string_buff
    nrf_log_backend_rtt.o(i.serial_tx) refers to segger_rtt.o(i.SEGGER_RTT_WriteNoLock) for SEGGER_RTT_WriteNoLock
    nrf_log_backend_rtt.o(.constdata) refers to nrf_log_backend_rtt.o(i.nrf_log_backend_rtt_put) for nrf_log_backend_rtt_put
    nrf_log_backend_rtt.o(.constdata) refers to nrf_log_backend_rtt.o(i.nrf_log_backend_rtt_panic_set) for nrf_log_backend_rtt_panic_set
    nrf_log_backend_rtt.o(.constdata) refers to nrf_log_backend_rtt.o(i.nrf_log_backend_rtt_flush) for nrf_log_backend_rtt_flush
    nrf_log_backend_serial.o(i.nrf_log_backend_serial_put) refers to nrf_memobj.o(i.nrf_memobj_get) for nrf_memobj_get
    nrf_log_backend_serial.o(i.nrf_log_backend_serial_put) refers to memseta.o(.text) for __aeabi_memclr4
    nrf_log_backend_serial.o(i.nrf_log_backend_serial_put) refers to nrf_memobj.o(i.nrf_memobj_read) for nrf_memobj_read
    nrf_log_backend_serial.o(i.nrf_log_backend_serial_put) refers to nrf_log_str_formatter.o(i.nrf_log_std_entry_process) for nrf_log_std_entry_process
    nrf_log_backend_serial.o(i.nrf_log_backend_serial_put) refers to nrf_log_str_formatter.o(i.nrf_log_hexdump_entry_process) for nrf_log_hexdump_entry_process
    nrf_log_backend_serial.o(i.nrf_log_backend_serial_put) refers to nrf_memobj.o(i.nrf_memobj_put) for nrf_memobj_put
    nrf_log_default_backends.o(i.nrf_log_default_backends_init) refers to nrf_log_backend_rtt.o(i.nrf_log_backend_rtt_init) for nrf_log_backend_rtt_init
    nrf_log_default_backends.o(i.nrf_log_default_backends_init) refers to nrf_log_frontend.o(i.nrf_log_backend_add) for nrf_log_backend_add
    nrf_log_default_backends.o(i.nrf_log_default_backends_init) refers to nrf_log_default_backends.o(.data) for rtt_log_backend
    nrf_log_default_backends.o(.data) refers to nrf_log_backend_rtt.o(.constdata) for nrf_log_backend_rtt_api
    nrf_log_frontend.o(i.backend_id_assign) refers to nrf_log_frontend.o(.bss) for m_log_data
    nrf_log_frontend.o(i.buf_prealloc) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    nrf_log_frontend.o(i.buf_prealloc) refers to nrf_log_frontend.o(i.log_skip) for log_skip
    nrf_log_frontend.o(i.buf_prealloc) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    nrf_log_frontend.o(i.buf_prealloc) refers to nrf_log_frontend.o(.bss) for m_log_data
    nrf_log_frontend.o(i.buffer_is_empty) refers to nrf_log_frontend.o(.bss) for m_log_data
    nrf_log_frontend.o(i.cont_buf_prealloc) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    nrf_log_frontend.o(i.cont_buf_prealloc) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    nrf_log_frontend.o(i.cont_buf_prealloc) refers to nrf_log_frontend.o(.bss) for m_log_data
    nrf_log_frontend.o(i.log_skip) refers to nrf_log_frontend.o(i.nrf_atomic_flag_set) for nrf_atomic_flag_set
    nrf_log_frontend.o(i.log_skip) refers to nrf_log_frontend.o(.emb_text) for __asm___18_nrf_log_frontend_c_bc460776__nrf_atomic_internal_and
    nrf_log_frontend.o(i.log_skip) refers to nrf_log_frontend.o(.bss) for m_log_data
    nrf_log_frontend.o(i.module_idx_get) refers to nrf_log_frontend.o(i.nrf_log_module_cnt_get) for nrf_log_module_cnt_get
    nrf_log_frontend.o(i.nrf_atomic_flag_set) refers to nrf_log_frontend.o(.emb_text) for __asm___18_nrf_log_frontend_c_bc460776__nrf_atomic_internal_orr
    nrf_log_frontend.o(i.nrf_log_backend_add) refers to nrf_log_frontend.o(i.backend_id_assign) for backend_id_assign
    nrf_log_frontend.o(i.nrf_log_backend_add) refers to nrf_log_frontend.o(.bss) for m_log_data
    nrf_log_frontend.o(i.nrf_log_backend_remove) refers to nrf_log_frontend.o(.bss) for m_log_data
    nrf_log_frontend.o(i.nrf_log_frontend_dequeue) refers to nrf_log_frontend.o(i.buffer_is_empty) for buffer_is_empty
    nrf_log_frontend.o(i.nrf_log_frontend_dequeue) refers to nrf_memobj.o(i.nrf_memobj_alloc) for nrf_memobj_alloc
    nrf_log_frontend.o(i.nrf_log_frontend_dequeue) refers to nrf_memobj.o(i.nrf_memobj_get) for nrf_memobj_get
    nrf_log_frontend.o(i.nrf_log_frontend_dequeue) refers to nrf_memobj.o(i.nrf_memobj_write) for nrf_memobj_write
    nrf_log_frontend.o(i.nrf_log_frontend_dequeue) refers to nrf_memobj.o(i.nrf_memobj_put) for nrf_memobj_put
    nrf_log_frontend.o(i.nrf_log_frontend_dequeue) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    nrf_log_frontend.o(i.nrf_log_frontend_dequeue) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    nrf_log_frontend.o(i.nrf_log_frontend_dequeue) refers to nrf_log_frontend.o(.bss) for m_log_data
    nrf_log_frontend.o(i.nrf_log_frontend_dequeue) refers to nrf_log_frontend.o(.constdata) for mempool
    nrf_log_frontend.o(i.nrf_log_frontend_hexdump) refers to nrf_log_frontend.o(i.buf_prealloc) for buf_prealloc
    nrf_log_frontend.o(i.nrf_log_frontend_hexdump) refers to memcpya.o(.text) for __aeabi_memcpy
    nrf_log_frontend.o(i.nrf_log_frontend_hexdump) refers to nrf_log_frontend.o(i.nrf_log_frontend_dequeue) for nrf_log_frontend_dequeue
    nrf_log_frontend.o(i.nrf_log_frontend_hexdump) refers to nrf_log_frontend.o(.bss) for m_log_data
    nrf_log_frontend.o(i.nrf_log_frontend_std_0) refers to nrf_log_frontend.o(i.std_n) for std_n
    nrf_log_frontend.o(i.nrf_log_frontend_std_1) refers to nrf_log_frontend.o(i.std_n) for std_n
    nrf_log_frontend.o(i.nrf_log_frontend_std_2) refers to nrf_log_frontend.o(i.std_n) for std_n
    nrf_log_frontend.o(i.nrf_log_frontend_std_3) refers to nrf_log_frontend.o(i.std_n) for std_n
    nrf_log_frontend.o(i.nrf_log_frontend_std_4) refers to nrf_log_frontend.o(i.std_n) for std_n
    nrf_log_frontend.o(i.nrf_log_frontend_std_5) refers to nrf_log_frontend.o(i.std_n) for std_n
    nrf_log_frontend.o(i.nrf_log_frontend_std_6) refers to nrf_log_frontend.o(i.std_n) for std_n
    nrf_log_frontend.o(i.nrf_log_init) refers to nrf_memobj.o(i.nrf_memobj_pool_init) for nrf_memobj_pool_init
    nrf_log_frontend.o(i.nrf_log_init) refers to nrf_log_frontend.o(.bss) for m_log_data
    nrf_log_frontend.o(i.nrf_log_init) refers to nrf_log_frontend.o(.constdata) for mempool
    nrf_log_frontend.o(i.nrf_log_module_filter_get) refers to nrf_log_frontend.o(i.module_idx_get) for module_idx_get
    nrf_log_frontend.o(i.nrf_log_module_name_get) refers to nrf_log_frontend.o(i.module_idx_get) for module_idx_get
    nrf_log_frontend.o(i.nrf_log_panic) refers to nrf_log_frontend.o(.bss) for m_log_data
    nrf_log_frontend.o(i.nrf_log_push) refers to strlen.o(.text) for strlen
    nrf_log_frontend.o(i.nrf_log_push) refers to nrf_log_frontend.o(i.cont_buf_prealloc) for cont_buf_prealloc
    nrf_log_frontend.o(i.nrf_log_push) refers to memcpya.o(.text) for __aeabi_memcpy
    nrf_log_frontend.o(i.nrf_log_push) refers to nrf_log_frontend.o(.bss) for m_log_data
    nrf_log_frontend.o(i.std_header_set) refers to nrf_log_frontend.o(.bss) for m_log_data
    nrf_log_frontend.o(i.std_n) refers to nrf_log_frontend.o(i.buf_prealloc) for buf_prealloc
    nrf_log_frontend.o(i.std_n) refers to nrf_log_frontend.o(i.std_header_set) for std_header_set
    nrf_log_frontend.o(i.std_n) refers to nrf_log_frontend.o(i.nrf_log_frontend_dequeue) for nrf_log_frontend_dequeue
    nrf_log_frontend.o(i.std_n) refers to nrf_log_frontend.o(.bss) for m_log_data
    nrf_log_frontend.o(.constdata) refers to nrf_log_frontend.o(.data) for mempool_nrf_balloc_cb
    nrf_log_frontend.o(.constdata) refers to nrf_log_frontend.o(.bss) for mempool_nrf_balloc_pool_mem
    nrf_log_frontend.o(.data) refers to nrf_log_frontend.o(.conststring) for .conststring
    nrf_log_frontend.o(log_const_data) refers to nrf_log_frontend.o(.conststrlit) for .conststrlit
    nrf_log_str_formatter.o(i.nrf_log_hexdump_entry_process) refers to nrf_log_str_formatter.o(i.prefix_process) for prefix_process
    nrf_log_str_formatter.o(i.nrf_log_hexdump_entry_process) refers to nrf_fprintf.o(i.nrf_fprintf) for nrf_fprintf
    nrf_log_str_formatter.o(i.nrf_log_hexdump_entry_process) refers to ctype_o.o(.text) for __rt_ctype_table
    nrf_log_str_formatter.o(i.nrf_log_hexdump_entry_process) refers to nrf_log_str_formatter.o(i.postfix_process) for postfix_process
    nrf_log_str_formatter.o(i.nrf_log_std_entry_process) refers to nrf_log_str_formatter.o(i.prefix_process) for prefix_process
    nrf_log_str_formatter.o(i.nrf_log_std_entry_process) refers to nrf_fprintf.o(i.nrf_fprintf) for nrf_fprintf
    nrf_log_str_formatter.o(i.nrf_log_std_entry_process) refers to nrf_log_str_formatter.o(i.postfix_process) for postfix_process
    nrf_log_str_formatter.o(i.postfix_process) refers to nrf_fprintf.o(i.nrf_fprintf) for nrf_fprintf
    nrf_log_str_formatter.o(i.postfix_process) refers to nrf_fprintf.o(i.nrf_fprintf_buffer_flush) for nrf_fprintf_buffer_flush
    nrf_log_str_formatter.o(i.postfix_process) refers to nrf_log_str_formatter.o(.data) for m_colors
    nrf_log_str_formatter.o(i.prefix_process) refers to nrf_log_frontend.o(i.nrf_log_color_id_get) for nrf_log_color_id_get
    nrf_log_str_formatter.o(i.prefix_process) refers to nrf_fprintf.o(i.nrf_fprintf) for nrf_fprintf
    nrf_log_str_formatter.o(i.prefix_process) refers to nrf_log_frontend.o(i.nrf_log_module_name_get) for nrf_log_module_name_get
    nrf_log_str_formatter.o(i.prefix_process) refers to nrf_log_str_formatter.o(.data) for m_colors
    nrf_log_str_formatter.o(.data) refers to nrf_log_str_formatter.o(.conststring) for .conststring
    segger_rtt.o(i.SEGGER_RTT_AllocDownBuffer) refers to segger_rtt.o(i._DoInit) for _DoInit
    segger_rtt.o(i.SEGGER_RTT_AllocDownBuffer) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    segger_rtt.o(i.SEGGER_RTT_AllocDownBuffer) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    segger_rtt.o(i.SEGGER_RTT_AllocDownBuffer) refers to segger_rtt.o(.bss) for _SEGGER_RTT
    segger_rtt.o(i.SEGGER_RTT_AllocUpBuffer) refers to segger_rtt.o(i._DoInit) for _DoInit
    segger_rtt.o(i.SEGGER_RTT_AllocUpBuffer) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    segger_rtt.o(i.SEGGER_RTT_AllocUpBuffer) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    segger_rtt.o(i.SEGGER_RTT_AllocUpBuffer) refers to segger_rtt.o(.bss) for _SEGGER_RTT
    segger_rtt.o(i.SEGGER_RTT_ConfigDownBuffer) refers to segger_rtt.o(i._DoInit) for _DoInit
    segger_rtt.o(i.SEGGER_RTT_ConfigDownBuffer) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    segger_rtt.o(i.SEGGER_RTT_ConfigDownBuffer) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    segger_rtt.o(i.SEGGER_RTT_ConfigDownBuffer) refers to segger_rtt.o(.bss) for _SEGGER_RTT
    segger_rtt.o(i.SEGGER_RTT_ConfigUpBuffer) refers to segger_rtt.o(i._DoInit) for _DoInit
    segger_rtt.o(i.SEGGER_RTT_ConfigUpBuffer) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    segger_rtt.o(i.SEGGER_RTT_ConfigUpBuffer) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    segger_rtt.o(i.SEGGER_RTT_ConfigUpBuffer) refers to segger_rtt.o(.bss) for _SEGGER_RTT
    segger_rtt.o(i.SEGGER_RTT_GetKey) refers to segger_rtt.o(i.SEGGER_RTT_Read) for SEGGER_RTT_Read
    segger_rtt.o(i.SEGGER_RTT_HasData) refers to segger_rtt.o(.bss) for _SEGGER_RTT
    segger_rtt.o(i.SEGGER_RTT_HasKey) refers to segger_rtt.o(i._DoInit) for _DoInit
    segger_rtt.o(i.SEGGER_RTT_HasKey) refers to segger_rtt.o(.bss) for _SEGGER_RTT
    segger_rtt.o(i.SEGGER_RTT_Init) refers to segger_rtt.o(i._DoInit) for _DoInit
    segger_rtt.o(i.SEGGER_RTT_PutChar) refers to segger_rtt.o(i._DoInit) for _DoInit
    segger_rtt.o(i.SEGGER_RTT_PutChar) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    segger_rtt.o(i.SEGGER_RTT_PutChar) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    segger_rtt.o(i.SEGGER_RTT_PutChar) refers to segger_rtt.o(.bss) for _SEGGER_RTT
    segger_rtt.o(i.SEGGER_RTT_PutCharSkip) refers to segger_rtt.o(i._DoInit) for _DoInit
    segger_rtt.o(i.SEGGER_RTT_PutCharSkip) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    segger_rtt.o(i.SEGGER_RTT_PutCharSkip) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    segger_rtt.o(i.SEGGER_RTT_PutCharSkip) refers to segger_rtt.o(.bss) for _SEGGER_RTT
    segger_rtt.o(i.SEGGER_RTT_PutCharSkipNoLock) refers to segger_rtt.o(.bss) for _SEGGER_RTT
    segger_rtt.o(i.SEGGER_RTT_Read) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    segger_rtt.o(i.SEGGER_RTT_Read) refers to segger_rtt.o(i.SEGGER_RTT_ReadNoLock) for SEGGER_RTT_ReadNoLock
    segger_rtt.o(i.SEGGER_RTT_Read) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    segger_rtt.o(i.SEGGER_RTT_ReadNoLock) refers to segger_rtt.o(i._DoInit) for _DoInit
    segger_rtt.o(i.SEGGER_RTT_ReadNoLock) refers to memcpya.o(.text) for __aeabi_memcpy
    segger_rtt.o(i.SEGGER_RTT_ReadNoLock) refers to segger_rtt.o(.bss) for _SEGGER_RTT
    segger_rtt.o(i.SEGGER_RTT_SetFlagsDownBuffer) refers to segger_rtt.o(i._DoInit) for _DoInit
    segger_rtt.o(i.SEGGER_RTT_SetFlagsDownBuffer) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    segger_rtt.o(i.SEGGER_RTT_SetFlagsDownBuffer) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    segger_rtt.o(i.SEGGER_RTT_SetFlagsDownBuffer) refers to segger_rtt.o(.bss) for _SEGGER_RTT
    segger_rtt.o(i.SEGGER_RTT_SetFlagsUpBuffer) refers to segger_rtt.o(i._DoInit) for _DoInit
    segger_rtt.o(i.SEGGER_RTT_SetFlagsUpBuffer) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    segger_rtt.o(i.SEGGER_RTT_SetFlagsUpBuffer) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    segger_rtt.o(i.SEGGER_RTT_SetFlagsUpBuffer) refers to segger_rtt.o(.bss) for _SEGGER_RTT
    segger_rtt.o(i.SEGGER_RTT_SetNameDownBuffer) refers to segger_rtt.o(i._DoInit) for _DoInit
    segger_rtt.o(i.SEGGER_RTT_SetNameDownBuffer) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    segger_rtt.o(i.SEGGER_RTT_SetNameDownBuffer) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    segger_rtt.o(i.SEGGER_RTT_SetNameDownBuffer) refers to segger_rtt.o(.bss) for _SEGGER_RTT
    segger_rtt.o(i.SEGGER_RTT_SetNameUpBuffer) refers to segger_rtt.o(i._DoInit) for _DoInit
    segger_rtt.o(i.SEGGER_RTT_SetNameUpBuffer) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    segger_rtt.o(i.SEGGER_RTT_SetNameUpBuffer) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    segger_rtt.o(i.SEGGER_RTT_SetNameUpBuffer) refers to segger_rtt.o(.bss) for _SEGGER_RTT
    segger_rtt.o(i.SEGGER_RTT_SetTerminal) refers to segger_rtt.o(i._DoInit) for _DoInit
    segger_rtt.o(i.SEGGER_RTT_SetTerminal) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    segger_rtt.o(i.SEGGER_RTT_SetTerminal) refers to segger_rtt.o(i._WriteBlocking) for _WriteBlocking
    segger_rtt.o(i.SEGGER_RTT_SetTerminal) refers to segger_rtt.o(i._GetAvailWriteSpace) for _GetAvailWriteSpace
    segger_rtt.o(i.SEGGER_RTT_SetTerminal) refers to segger_rtt.o(i._WriteNoCheck) for _WriteNoCheck
    segger_rtt.o(i.SEGGER_RTT_SetTerminal) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    segger_rtt.o(i.SEGGER_RTT_SetTerminal) refers to segger_rtt.o(.bss) for _SEGGER_RTT
    segger_rtt.o(i.SEGGER_RTT_SetTerminal) refers to segger_rtt.o(.data) for _aTerminalId
    segger_rtt.o(i.SEGGER_RTT_TerminalOut) refers to segger_rtt.o(i._DoInit) for _DoInit
    segger_rtt.o(i.SEGGER_RTT_TerminalOut) refers to strlen.o(.text) for strlen
    segger_rtt.o(i.SEGGER_RTT_TerminalOut) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    segger_rtt.o(i.SEGGER_RTT_TerminalOut) refers to segger_rtt.o(i._GetAvailWriteSpace) for _GetAvailWriteSpace
    segger_rtt.o(i.SEGGER_RTT_TerminalOut) refers to segger_rtt.o(i._PostTerminalSwitch) for _PostTerminalSwitch
    segger_rtt.o(i.SEGGER_RTT_TerminalOut) refers to segger_rtt.o(i._WriteBlocking) for _WriteBlocking
    segger_rtt.o(i.SEGGER_RTT_TerminalOut) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    segger_rtt.o(i.SEGGER_RTT_TerminalOut) refers to segger_rtt.o(.bss) for _SEGGER_RTT
    segger_rtt.o(i.SEGGER_RTT_TerminalOut) refers to segger_rtt.o(.data) for _ActiveTerminal
    segger_rtt.o(i.SEGGER_RTT_WaitKey) refers to segger_rtt.o(i.SEGGER_RTT_GetKey) for SEGGER_RTT_GetKey
    segger_rtt.o(i.SEGGER_RTT_Write) refers to segger_rtt.o(i._DoInit) for _DoInit
    segger_rtt.o(i.SEGGER_RTT_Write) refers to app_util_platform.o(i.app_util_critical_region_enter) for app_util_critical_region_enter
    segger_rtt.o(i.SEGGER_RTT_Write) refers to segger_rtt.o(i.SEGGER_RTT_WriteNoLock) for SEGGER_RTT_WriteNoLock
    segger_rtt.o(i.SEGGER_RTT_Write) refers to app_util_platform.o(i.app_util_critical_region_exit) for app_util_critical_region_exit
    segger_rtt.o(i.SEGGER_RTT_Write) refers to segger_rtt.o(.bss) for _SEGGER_RTT
    segger_rtt.o(i.SEGGER_RTT_WriteNoLock) refers to segger_rtt.o(i._GetAvailWriteSpace) for _GetAvailWriteSpace
    segger_rtt.o(i.SEGGER_RTT_WriteNoLock) refers to segger_rtt.o(i._WriteNoCheck) for _WriteNoCheck
    segger_rtt.o(i.SEGGER_RTT_WriteNoLock) refers to segger_rtt.o(i._WriteBlocking) for _WriteBlocking
    segger_rtt.o(i.SEGGER_RTT_WriteNoLock) refers to segger_rtt.o(.bss) for _SEGGER_RTT
    segger_rtt.o(i.SEGGER_RTT_WriteSkipNoLock) refers to memcpya.o(.text) for __aeabi_memcpy
    segger_rtt.o(i.SEGGER_RTT_WriteSkipNoLock) refers to segger_rtt.o(.bss) for _SEGGER_RTT
    segger_rtt.o(i.SEGGER_RTT_WriteString) refers to strlen.o(.text) for strlen
    segger_rtt.o(i.SEGGER_RTT_WriteString) refers to segger_rtt.o(i.SEGGER_RTT_Write) for SEGGER_RTT_Write
    segger_rtt.o(i.SEGGER_RTT_WriteWithOverwriteNoLock) refers to memcpya.o(.text) for __aeabi_memcpy
    segger_rtt.o(i.SEGGER_RTT_WriteWithOverwriteNoLock) refers to segger_rtt.o(.bss) for _SEGGER_RTT
    segger_rtt.o(i._DoInit) refers to strcpy.o(.text) for strcpy
    segger_rtt.o(i._DoInit) refers to segger_rtt.o(.bss) for _SEGGER_RTT
    segger_rtt.o(i._PostTerminalSwitch) refers to segger_rtt.o(i._WriteBlocking) for _WriteBlocking
    segger_rtt.o(i._PostTerminalSwitch) refers to segger_rtt.o(.data) for _aTerminalId
    segger_rtt.o(i._WriteBlocking) refers to memcpya.o(.text) for __aeabi_memcpy
    segger_rtt.o(i._WriteNoCheck) refers to memcpya.o(.text) for __aeabi_memcpy
    segger_rtt_printf.o(i.SEGGER_RTT_printf) refers to segger_rtt_printf.o(i.SEGGER_RTT_vprintf) for SEGGER_RTT_vprintf
    segger_rtt_printf.o(i.SEGGER_RTT_vprintf) refers to segger_rtt_printf.o(i._StoreChar) for _StoreChar
    segger_rtt_printf.o(i.SEGGER_RTT_vprintf) refers to segger_rtt_printf.o(i._PrintInt) for _PrintInt
    segger_rtt_printf.o(i.SEGGER_RTT_vprintf) refers to segger_rtt_printf.o(i._PrintUnsigned) for _PrintUnsigned
    segger_rtt_printf.o(i.SEGGER_RTT_vprintf) refers to segger_rtt.o(i.SEGGER_RTT_Write) for SEGGER_RTT_Write
    segger_rtt_printf.o(i._PrintInt) refers to segger_rtt_printf.o(i._StoreChar) for _StoreChar
    segger_rtt_printf.o(i._PrintInt) refers to segger_rtt_printf.o(i._PrintUnsigned) for _PrintUnsigned
    segger_rtt_printf.o(i._PrintUnsigned) refers to segger_rtt_printf.o(i._StoreChar) for _StoreChar
    segger_rtt_printf.o(i._PrintUnsigned) refers to segger_rtt_printf.o(.constdata) for _aV2C
    segger_rtt_printf.o(i._StoreChar) refers to segger_rtt.o(i.SEGGER_RTT_Write) for SEGGER_RTT_Write
    nrf_sdh.o(i.SWI2_EGU2_IRQHandler) refers to nrf_sdh.o(i.nrf_sdh_evts_poll) for nrf_sdh_evts_poll
    nrf_sdh.o(i.nrf_sdh_disable_request) refers to nrf_sdh.o(i.sdh_request_observer_notify) for sdh_request_observer_notify
    nrf_sdh.o(i.nrf_sdh_disable_request) refers to nrf_sdh.o(i.sdh_state_observer_notify) for sdh_state_observer_notify
    nrf_sdh.o(i.nrf_sdh_disable_request) refers to nrf_sdh.o(i.softdevice_evt_irq_disable) for softdevice_evt_irq_disable
    nrf_sdh.o(i.nrf_sdh_disable_request) refers to nrf_sdh.o(.data) for m_nrf_sdh_enabled
    nrf_sdh.o(i.nrf_sdh_enable_request) refers to nrf_sdh.o(i.sdh_request_observer_notify) for sdh_request_observer_notify
    nrf_sdh.o(i.nrf_sdh_enable_request) refers to nrf_sdh.o(i.sdh_state_observer_notify) for sdh_state_observer_notify
    nrf_sdh.o(i.nrf_sdh_enable_request) refers to nrf_sdh.o(i.softdevices_evt_irq_enable) for softdevices_evt_irq_enable
    nrf_sdh.o(i.nrf_sdh_enable_request) refers to nrf_sdh.o(.data) for m_nrf_sdh_enabled
    nrf_sdh.o(i.nrf_sdh_enable_request) refers to nrf_sdh.o(.constdata) for .constdata
    nrf_sdh.o(i.nrf_sdh_enable_request) refers to app_error_weak.o(i.app_error_fault_handler) for app_error_fault_handler
    nrf_sdh.o(i.nrf_sdh_evts_poll) refers to nrf_section_iter.o(i.nrf_section_iter_init) for nrf_section_iter_init
    nrf_sdh.o(i.nrf_sdh_evts_poll) refers to nrf_sdh.o(i.nrf_section_iter_get) for nrf_section_iter_get
    nrf_sdh.o(i.nrf_sdh_evts_poll) refers to nrf_section_iter.o(i.nrf_section_iter_next) for nrf_section_iter_next
    nrf_sdh.o(i.nrf_sdh_evts_poll) refers to nrf_sdh.o(.constdata) for sdh_stack_observers
    nrf_sdh.o(i.nrf_sdh_is_enabled) refers to nrf_sdh.o(.data) for m_nrf_sdh_enabled
    nrf_sdh.o(i.nrf_sdh_is_suspended) refers to nrf_sdh.o(.data) for m_nrf_sdh_enabled
    nrf_sdh.o(i.nrf_sdh_request_continue) refers to nrf_sdh.o(i.nrf_sdh_disable_request) for nrf_sdh_disable_request
    nrf_sdh.o(i.nrf_sdh_request_continue) refers to nrf_sdh.o(i.nrf_sdh_enable_request) for nrf_sdh_enable_request
    nrf_sdh.o(i.nrf_sdh_request_continue) refers to nrf_sdh.o(.data) for m_nrf_sdh_continue
    nrf_sdh.o(i.nrf_sdh_resume) refers to nrf_sdh.o(i.__sd_nvic_app_accessible_irq) for __sd_nvic_app_accessible_irq
    nrf_sdh.o(i.nrf_sdh_resume) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    nrf_sdh.o(i.nrf_sdh_resume) refers to nrf_sdh.o(i.softdevices_evt_irq_enable) for softdevices_evt_irq_enable
    nrf_sdh.o(i.nrf_sdh_resume) refers to nrf_sdh.o(.data) for m_nrf_sdh_suspended
    nrf_sdh.o(i.nrf_sdh_suspend) refers to nrf_sdh.o(i.softdevice_evt_irq_disable) for softdevice_evt_irq_disable
    nrf_sdh.o(i.nrf_sdh_suspend) refers to nrf_sdh.o(.data) for m_nrf_sdh_enabled
    nrf_sdh.o(i.sd_nvic_EnableIRQ) refers to nrf_sdh.o(i.__sd_nvic_app_accessible_irq) for __sd_nvic_app_accessible_irq
    nrf_sdh.o(i.sd_nvic_EnableIRQ) refers to app_util_platform.o(.bss) for nrf_nvic_state
    nrf_sdh.o(i.sdh_request_observer_notify) refers to nrf_section_iter.o(i.nrf_section_iter_init) for nrf_section_iter_init
    nrf_sdh.o(i.sdh_request_observer_notify) refers to nrf_sdh.o(i.nrf_section_iter_get) for nrf_section_iter_get
    nrf_sdh.o(i.sdh_request_observer_notify) refers to nrf_section_iter.o(i.nrf_section_iter_next) for nrf_section_iter_next
    nrf_sdh.o(i.sdh_request_observer_notify) refers to nrf_sdh.o(.constdata) for sdh_req_observers
    nrf_sdh.o(i.sdh_state_observer_notify) refers to nrf_section_iter.o(i.nrf_section_iter_init) for nrf_section_iter_init
    nrf_sdh.o(i.sdh_state_observer_notify) refers to nrf_sdh.o(i.nrf_section_iter_get) for nrf_section_iter_get
    nrf_sdh.o(i.sdh_state_observer_notify) refers to nrf_section_iter.o(i.nrf_section_iter_next) for nrf_section_iter_next
    nrf_sdh.o(i.sdh_state_observer_notify) refers to nrf_sdh.o(.constdata) for sdh_state_observers
    nrf_sdh.o(i.softdevice_evt_irq_disable) refers to nrf_sdh.o(i.__sd_nvic_app_accessible_irq) for __sd_nvic_app_accessible_irq
    nrf_sdh.o(i.softdevice_evt_irq_disable) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    nrf_sdh.o(i.softdevice_evt_irq_disable) refers to app_util_platform.o(.bss) for nrf_nvic_state
    nrf_sdh.o(i.softdevices_evt_irq_enable) refers to nrf_sdh.o(i.sd_nvic_EnableIRQ) for sd_nvic_EnableIRQ
    nrf_sdh.o(i.softdevices_evt_irq_enable) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    nrf_sdh.o(log_const_data) refers to nrf_sdh.o(.conststrlit) for .conststrlit
    nrf_sdh_ble.o(i.nrf_sdh_ble_app_ram_start_get) refers to nrf_sdh_ble.o(.constdata) for m_ram_start
    nrf_sdh_ble.o(i.nrf_sdh_ble_default_cfg_set) refers to nrf_sdh_ble.o(i.nrf_sdh_ble_app_ram_start_get) for nrf_sdh_ble_app_ram_start_get
    nrf_sdh_ble.o(i.nrf_sdh_ble_default_cfg_set) refers to nrf_strerror.o(i.nrf_strerror_get) for nrf_strerror_get
    nrf_sdh_ble.o(i.nrf_sdh_ble_default_cfg_set) refers to nrf_log_frontend.o(i.nrf_log_frontend_std_1) for nrf_log_frontend_std_1
    nrf_sdh_ble.o(i.nrf_sdh_ble_default_cfg_set) refers to nrf_sdh_ble.o(log_dynamic_data) for m_nrf_log_nrf_sdh_ble_logs_data_dynamic
    nrf_sdh_ble.o(i.nrf_sdh_ble_default_cfg_set) refers to nrf_sdh_ble.o(.conststring) for .conststring
    nrf_sdh_ble.o(i.nrf_sdh_ble_enable) refers to nrf_log_frontend.o(i.nrf_log_frontend_std_2) for nrf_log_frontend_std_2
    nrf_sdh_ble.o(i.nrf_sdh_ble_enable) refers to nrf_sdh_ble.o(i.ram_end_address_get) for ram_end_address_get
    nrf_sdh_ble.o(i.nrf_sdh_ble_enable) refers to nrf_log_frontend.o(i.nrf_log_frontend_std_1) for nrf_log_frontend_std_1
    nrf_sdh_ble.o(i.nrf_sdh_ble_enable) refers to nrf_strerror.o(i.nrf_strerror_get) for nrf_strerror_get
    nrf_sdh_ble.o(i.nrf_sdh_ble_enable) refers to nrf_sdh_ble.o(log_dynamic_data) for m_nrf_log_nrf_sdh_ble_logs_data_dynamic
    nrf_sdh_ble.o(i.nrf_sdh_ble_evts_poll) refers to nrf_section_iter.o(i.nrf_section_iter_init) for nrf_section_iter_init
    nrf_sdh_ble.o(i.nrf_sdh_ble_evts_poll) refers to nrf_section_iter.o(i.nrf_section_iter_next) for nrf_section_iter_next
    nrf_sdh_ble.o(i.nrf_sdh_ble_evts_poll) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    nrf_sdh_ble.o(i.nrf_sdh_ble_evts_poll) refers to nrf_sdh_ble.o(.constdata) for sdh_ble_observers
    nrf_sdh_ble.o(log_const_data) refers to nrf_sdh_ble.o(.conststrlit) for .conststrlit
    nrf_sdh_ble.o(sdh_stack_observers0) refers to nrf_sdh_ble.o(i.nrf_sdh_ble_evts_poll) for nrf_sdh_ble_evts_poll
    nrf_sdh_soc.o(i.nrf_sdh_soc_evts_poll) refers to nrf_section_iter.o(i.nrf_section_iter_init) for nrf_section_iter_init
    nrf_sdh_soc.o(i.nrf_sdh_soc_evts_poll) refers to nrf_section_iter.o(i.nrf_section_iter_next) for nrf_section_iter_next
    nrf_sdh_soc.o(i.nrf_sdh_soc_evts_poll) refers to app_error.o(i.app_error_handler_bare) for app_error_handler_bare
    nrf_sdh_soc.o(i.nrf_sdh_soc_evts_poll) refers to nrf_sdh_soc.o(.constdata) for sdh_soc_observers
    nrf_sdh_soc.o(log_const_data) refers to nrf_sdh_soc.o(.conststrlit) for .conststrlit
    nrf_sdh_soc.o(sdh_stack_observers0) refers to nrf_sdh_soc.o(i.nrf_sdh_soc_evts_poll) for nrf_sdh_soc_evts_poll
    arm_startup_nrf52840.o(RESET) refers to arm_startup_nrf52840.o(STACK) for __initial_sp
    arm_startup_nrf52840.o(RESET) refers to arm_startup_nrf52840.o(.text) for Reset_Handler
    arm_startup_nrf52840.o(RESET) refers to nrf_drv_clock.o(i.POWER_CLOCK_IRQHandler) for POWER_CLOCK_IRQHandler
    arm_startup_nrf52840.o(RESET) refers to nrf_drv_uart.o(i.UARTE0_UART0_IRQHandler) for UARTE0_UART0_IRQHandler
    arm_startup_nrf52840.o(RESET) refers to nrf_drv_gpiote.o(i.GPIOTE_IRQHandler) for GPIOTE_IRQHandler
    arm_startup_nrf52840.o(RESET) refers to app_timer.o(i.RTC1_IRQHandler) for RTC1_IRQHandler
    arm_startup_nrf52840.o(RESET) refers to app_timer.o(i.SWI0_EGU0_IRQHandler) for SWI0_EGU0_IRQHandler
    arm_startup_nrf52840.o(RESET) refers to nrf_sdh.o(i.SWI2_EGU2_IRQHandler) for SWI2_EGU2_IRQHandler
    arm_startup_nrf52840.o(.text) refers to system_nrf52840.o(i.SystemInit) for SystemInit
    arm_startup_nrf52840.o(.text) refers to entry.o(.ARM.Collect$$$$00000000) for __main
    system_nrf52840.o(i.SystemCoreClockUpdate) refers to system_nrf52840.o(.data) for SystemCoreClock
    system_nrf52840.o(i.SystemInit) refers to system_nrf52840.o(i.errata_36) for errata_36
    system_nrf52840.o(i.SystemInit) refers to system_nrf52840.o(i.errata_66) for errata_66
    system_nrf52840.o(i.SystemInit) refers to system_nrf52840.o(i.errata_98) for errata_98
    system_nrf52840.o(i.SystemInit) refers to system_nrf52840.o(i.errata_103) for errata_103
    system_nrf52840.o(i.SystemInit) refers to system_nrf52840.o(i.errata_115) for errata_115
    system_nrf52840.o(i.SystemInit) refers to system_nrf52840.o(i.errata_120) for errata_120
    system_nrf52840.o(i.SystemInit) refers to system_nrf52840.o(i.errata_136) for errata_136
    system_nrf52840.o(i.SystemInit) refers to system_nrf52840.o(i.SystemCoreClockUpdate) for SystemCoreClockUpdate
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry10a.o(.ARM.Collect$$$$0000000D) for __rt_final_cpp
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry11a.o(.ARM.Collect$$$$0000000F) for __rt_final_exit
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry7b.o(.ARM.Collect$$$$00000008) for _main_clock
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry8b.o(.ARM.Collect$$$$0000000A) for _main_cpp_init
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry9a.o(.ARM.Collect$$$$0000000B) for _main_init
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry5.o(.ARM.Collect$$$$00000004) for _main_scatterload
    entry.o(.ARM.Collect$$$$00000000) refers (Special) to entry2.o(.ARM.Collect$$$$00000001) for _main_stk
    uldiv.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    uldiv.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    ctype_o.o(.text) refers to ctype_o.o(.constdata) for .constdata
    ctype_o.o(.constdata) refers to ctype_o.o(.constdata) for __ctype_table
    isalnum_o.o(.text) refers to ctype_o.o(.text) for __rt_ctype_table
    isalpha_o.o(.text) refers to ctype_o.o(.text) for __rt_ctype_table
    isblank_o.o(.text) refers to ctype_o.o(.constdata) for __ctype_table
    iscntrl_o.o(.text) refers to ctype_o.o(.text) for __rt_ctype_table
    isdigit_o.o(.text) refers to ctype_o.o(.text) for __rt_ctype_table
    isgraph_o.o(.text) refers to ctype_o.o(.text) for __rt_ctype_table
    islower_o.o(.text) refers to ctype_o.o(.text) for __rt_ctype_table
    isprint_o.o(.text) refers to ctype_o.o(.text) for __rt_ctype_table
    ispunct_o.o(.text) refers to ctype_o.o(.text) for __rt_ctype_table
    isspace_o.o(.text) refers to ctype_o.o(.text) for __rt_ctype_table
    isupper_o.o(.text) refers to ctype_o.o(.text) for __rt_ctype_table
    isxdigit_o.o(.text) refers to ctype_o.o(.text) for __rt_ctype_table
    printfb.o(i.__0fprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0fprintf$bare) refers to retarget.o(i.fputc) for fputc
    printfb.o(i.__0printf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0printf$bare) refers to retarget.o(i.fputc) for fputc
    printfb.o(i.__0printf$bare) refers to retarget.o(.data) for __stdout
    printfb.o(i.__0snprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0snprintf$bare) refers to printfb.o(i._snputc) for _snputc
    printfb.o(i.__0sprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0sprintf$bare) refers to printfb.o(i._sputc) for _sputc
    printfb.o(i.__0vfprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vfprintf$bare) refers to retarget.o(i.fputc) for fputc
    printfb.o(i.__0vprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vprintf$bare) refers to retarget.o(i.fputc) for fputc
    printfb.o(i.__0vprintf$bare) refers to retarget.o(.data) for __stdout
    printfb.o(i.__0vsnprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vsnprintf$bare) refers to printfb.o(i._snputc) for _snputc
    printfb.o(i.__0vsprintf$bare) refers to printfb.o(i._printf_core) for _printf_core
    printfb.o(i.__0vsprintf$bare) refers to printfb.o(i._sputc) for _sputc
    printf0.o(i.__0fprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0fprintf$0) refers to retarget.o(i.fputc) for fputc
    printf0.o(i.__0printf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0printf$0) refers to retarget.o(i.fputc) for fputc
    printf0.o(i.__0printf$0) refers to retarget.o(.data) for __stdout
    printf0.o(i.__0snprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0snprintf$0) refers to printf0.o(i._snputc) for _snputc
    printf0.o(i.__0sprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0sprintf$0) refers to printf0.o(i._sputc) for _sputc
    printf0.o(i.__0vfprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vfprintf$0) refers to retarget.o(i.fputc) for fputc
    printf0.o(i.__0vprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vprintf$0) refers to retarget.o(i.fputc) for fputc
    printf0.o(i.__0vprintf$0) refers to retarget.o(.data) for __stdout
    printf0.o(i.__0vsnprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vsnprintf$0) refers to printf0.o(i._snputc) for _snputc
    printf0.o(i.__0vsprintf$0) refers to printf0.o(i._printf_core) for _printf_core
    printf0.o(i.__0vsprintf$0) refers to printf0.o(i._sputc) for _sputc
    printf1.o(i.__0fprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0fprintf$1) refers to retarget.o(i.fputc) for fputc
    printf1.o(i.__0printf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0printf$1) refers to retarget.o(i.fputc) for fputc
    printf1.o(i.__0printf$1) refers to retarget.o(.data) for __stdout
    printf1.o(i.__0snprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0snprintf$1) refers to printf1.o(i._snputc) for _snputc
    printf1.o(i.__0sprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0sprintf$1) refers to printf1.o(i._sputc) for _sputc
    printf1.o(i.__0vfprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vfprintf$1) refers to retarget.o(i.fputc) for fputc
    printf1.o(i.__0vprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vprintf$1) refers to retarget.o(i.fputc) for fputc
    printf1.o(i.__0vprintf$1) refers to retarget.o(.data) for __stdout
    printf1.o(i.__0vsnprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vsnprintf$1) refers to printf1.o(i._snputc) for _snputc
    printf1.o(i.__0vsprintf$1) refers to printf1.o(i._printf_core) for _printf_core
    printf1.o(i.__0vsprintf$1) refers to printf1.o(i._sputc) for _sputc
    printf1.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf2.o(i.__0fprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0fprintf$2) refers to retarget.o(i.fputc) for fputc
    printf2.o(i.__0printf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0printf$2) refers to retarget.o(i.fputc) for fputc
    printf2.o(i.__0printf$2) refers to retarget.o(.data) for __stdout
    printf2.o(i.__0snprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0snprintf$2) refers to printf2.o(i._snputc) for _snputc
    printf2.o(i.__0sprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0sprintf$2) refers to printf2.o(i._sputc) for _sputc
    printf2.o(i.__0vfprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vfprintf$2) refers to retarget.o(i.fputc) for fputc
    printf2.o(i.__0vprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vprintf$2) refers to retarget.o(i.fputc) for fputc
    printf2.o(i.__0vprintf$2) refers to retarget.o(.data) for __stdout
    printf2.o(i.__0vsnprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vsnprintf$2) refers to printf2.o(i._snputc) for _snputc
    printf2.o(i.__0vsprintf$2) refers to printf2.o(i._printf_core) for _printf_core
    printf2.o(i.__0vsprintf$2) refers to printf2.o(i._sputc) for _sputc
    printf3.o(i.__0fprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0fprintf$3) refers to retarget.o(i.fputc) for fputc
    printf3.o(i.__0printf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0printf$3) refers to retarget.o(i.fputc) for fputc
    printf3.o(i.__0printf$3) refers to retarget.o(.data) for __stdout
    printf3.o(i.__0snprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0snprintf$3) refers to printf3.o(i._snputc) for _snputc
    printf3.o(i.__0sprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0sprintf$3) refers to printf3.o(i._sputc) for _sputc
    printf3.o(i.__0vfprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vfprintf$3) refers to retarget.o(i.fputc) for fputc
    printf3.o(i.__0vprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vprintf$3) refers to retarget.o(i.fputc) for fputc
    printf3.o(i.__0vprintf$3) refers to retarget.o(.data) for __stdout
    printf3.o(i.__0vsnprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vsnprintf$3) refers to printf3.o(i._snputc) for _snputc
    printf3.o(i.__0vsprintf$3) refers to printf3.o(i._printf_core) for _printf_core
    printf3.o(i.__0vsprintf$3) refers to printf3.o(i._sputc) for _sputc
    printf3.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf4.o(i.__0fprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0fprintf$4) refers to retarget.o(i.fputc) for fputc
    printf4.o(i.__0printf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0printf$4) refers to retarget.o(i.fputc) for fputc
    printf4.o(i.__0printf$4) refers to retarget.o(.data) for __stdout
    printf4.o(i.__0snprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0snprintf$4) refers to printf4.o(i._snputc) for _snputc
    printf4.o(i.__0sprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0sprintf$4) refers to printf4.o(i._sputc) for _sputc
    printf4.o(i.__0vfprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vfprintf$4) refers to retarget.o(i.fputc) for fputc
    printf4.o(i.__0vprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vprintf$4) refers to retarget.o(i.fputc) for fputc
    printf4.o(i.__0vprintf$4) refers to retarget.o(.data) for __stdout
    printf4.o(i.__0vsnprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vsnprintf$4) refers to printf4.o(i._snputc) for _snputc
    printf4.o(i.__0vsprintf$4) refers to printf4.o(i._printf_core) for _printf_core
    printf4.o(i.__0vsprintf$4) refers to printf4.o(i._sputc) for _sputc
    printf4.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf5.o(i.__0fprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0fprintf$5) refers to retarget.o(i.fputc) for fputc
    printf5.o(i.__0printf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0printf$5) refers to retarget.o(i.fputc) for fputc
    printf5.o(i.__0printf$5) refers to retarget.o(.data) for __stdout
    printf5.o(i.__0snprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0snprintf$5) refers to printf5.o(i._snputc) for _snputc
    printf5.o(i.__0sprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0sprintf$5) refers to printf5.o(i._sputc) for _sputc
    printf5.o(i.__0vfprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vfprintf$5) refers to retarget.o(i.fputc) for fputc
    printf5.o(i.__0vprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vprintf$5) refers to retarget.o(i.fputc) for fputc
    printf5.o(i.__0vprintf$5) refers to retarget.o(.data) for __stdout
    printf5.o(i.__0vsnprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vsnprintf$5) refers to printf5.o(i._snputc) for _snputc
    printf5.o(i.__0vsprintf$5) refers to printf5.o(i._printf_core) for _printf_core
    printf5.o(i.__0vsprintf$5) refers to printf5.o(i._sputc) for _sputc
    printf5.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf6.o(i.__0fprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0fprintf$6) refers to retarget.o(i.fputc) for fputc
    printf6.o(i.__0printf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0printf$6) refers to retarget.o(i.fputc) for fputc
    printf6.o(i.__0printf$6) refers to retarget.o(.data) for __stdout
    printf6.o(i.__0snprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0snprintf$6) refers to printf6.o(i._snputc) for _snputc
    printf6.o(i.__0sprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0sprintf$6) refers to printf6.o(i._sputc) for _sputc
    printf6.o(i.__0vfprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vfprintf$6) refers to retarget.o(i.fputc) for fputc
    printf6.o(i.__0vprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vprintf$6) refers to retarget.o(i.fputc) for fputc
    printf6.o(i.__0vprintf$6) refers to retarget.o(.data) for __stdout
    printf6.o(i.__0vsnprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vsnprintf$6) refers to printf6.o(i._snputc) for _snputc
    printf6.o(i.__0vsprintf$6) refers to printf6.o(i._printf_core) for _printf_core
    printf6.o(i.__0vsprintf$6) refers to printf6.o(i._sputc) for _sputc
    printf6.o(i._printf_core) refers to printf6.o(i._printf_pre_padding) for _printf_pre_padding
    printf6.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printf6.o(i._printf_core) refers to printf6.o(i._printf_post_padding) for _printf_post_padding
    printf7.o(i.__0fprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0fprintf$7) refers to retarget.o(i.fputc) for fputc
    printf7.o(i.__0printf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0printf$7) refers to retarget.o(i.fputc) for fputc
    printf7.o(i.__0printf$7) refers to retarget.o(.data) for __stdout
    printf7.o(i.__0snprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0snprintf$7) refers to printf7.o(i._snputc) for _snputc
    printf7.o(i.__0sprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0sprintf$7) refers to printf7.o(i._sputc) for _sputc
    printf7.o(i.__0vfprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vfprintf$7) refers to retarget.o(i.fputc) for fputc
    printf7.o(i.__0vprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vprintf$7) refers to retarget.o(i.fputc) for fputc
    printf7.o(i.__0vprintf$7) refers to retarget.o(.data) for __stdout
    printf7.o(i.__0vsnprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vsnprintf$7) refers to printf7.o(i._snputc) for _snputc
    printf7.o(i.__0vsprintf$7) refers to printf7.o(i._printf_core) for _printf_core
    printf7.o(i.__0vsprintf$7) refers to printf7.o(i._sputc) for _sputc
    printf7.o(i._printf_core) refers to printf7.o(i._printf_pre_padding) for _printf_pre_padding
    printf7.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf7.o(i._printf_core) refers to printf7.o(i._printf_post_padding) for _printf_post_padding
    printf8.o(i.__0fprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0fprintf$8) refers to retarget.o(i.fputc) for fputc
    printf8.o(i.__0printf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0printf$8) refers to retarget.o(i.fputc) for fputc
    printf8.o(i.__0printf$8) refers to retarget.o(.data) for __stdout
    printf8.o(i.__0snprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0snprintf$8) refers to printf8.o(i._snputc) for _snputc
    printf8.o(i.__0sprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0sprintf$8) refers to printf8.o(i._sputc) for _sputc
    printf8.o(i.__0vfprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vfprintf$8) refers to retarget.o(i.fputc) for fputc
    printf8.o(i.__0vprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vprintf$8) refers to retarget.o(i.fputc) for fputc
    printf8.o(i.__0vprintf$8) refers to retarget.o(.data) for __stdout
    printf8.o(i.__0vsnprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vsnprintf$8) refers to printf8.o(i._snputc) for _snputc
    printf8.o(i.__0vsprintf$8) refers to printf8.o(i._printf_core) for _printf_core
    printf8.o(i.__0vsprintf$8) refers to printf8.o(i._sputc) for _sputc
    printf8.o(i._printf_core) refers to printf8.o(i._printf_pre_padding) for _printf_pre_padding
    printf8.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printf8.o(i._printf_core) refers to printf8.o(i._printf_post_padding) for _printf_post_padding
    printfa.o(i.__0fprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0fprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0fprintf) refers to retarget.o(i.fputc) for fputc
    printfa.o(i.__0printf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0printf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0printf) refers to retarget.o(i.fputc) for fputc
    printfa.o(i.__0printf) refers to retarget.o(.data) for __stdout
    printfa.o(i.__0snprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0snprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0snprintf) refers to printfa.o(i._snputc) for _snputc
    printfa.o(i.__0sprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0sprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0sprintf) refers to printfa.o(i._sputc) for _sputc
    printfa.o(i.__0vfprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vfprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vfprintf) refers to retarget.o(i.fputc) for fputc
    printfa.o(i.__0vprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vprintf) refers to retarget.o(i.fputc) for fputc
    printfa.o(i.__0vprintf) refers to retarget.o(.data) for __stdout
    printfa.o(i.__0vsnprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vsnprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vsnprintf) refers to printfa.o(i._snputc) for _snputc
    printfa.o(i.__0vsprintf) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i.__0vsprintf) refers to printfa.o(i._printf_core) for _printf_core
    printfa.o(i.__0vsprintf) refers to printfa.o(i._sputc) for _sputc
    printfa.o(i._fp_digits) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._fp_digits) refers to dmul.o(.text) for __aeabi_dmul
    printfa.o(i._fp_digits) refers to ddiv.o(.text) for __aeabi_ddiv
    printfa.o(i._fp_digits) refers to cdrcmple.o(.text) for __aeabi_cdrcmple
    printfa.o(i._fp_digits) refers to dadd.o(.text) for __aeabi_dadd
    printfa.o(i._fp_digits) refers to dfixul.o(.text) for __aeabi_d2ulz
    printfa.o(i._fp_digits) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i._printf_core) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._printf_core) refers to printfa.o(i._printf_pre_padding) for _printf_pre_padding
    printfa.o(i._printf_core) refers to uldiv.o(.text) for __aeabi_uldivmod
    printfa.o(i._printf_core) refers to printfa.o(i._printf_post_padding) for _printf_post_padding
    printfa.o(i._printf_core) refers to printfa.o(i._fp_digits) for _fp_digits
    printfa.o(i._printf_core) refers to uidiv.o(.text) for __aeabi_uidivmod
    printfa.o(i._printf_post_padding) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._printf_pre_padding) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._snputc) refers (Special) to iusefp.o(.text) for __I$use$fp
    printfa.o(i._sputc) refers (Special) to iusefp.o(.text) for __I$use$fp
    entry2.o(.ARM.Collect$$$$00000001) refers to entry2.o(.ARM.Collect$$$$00002712) for __lit__00000000
    entry2.o(.ARM.Collect$$$$00002712) refers to arm_startup_nrf52840.o(STACK) for __initial_sp
    entry2.o(__vectab_stack_and_reset_area) refers to arm_startup_nrf52840.o(STACK) for __initial_sp
    entry2.o(__vectab_stack_and_reset_area) refers to entry.o(.ARM.Collect$$$$00000000) for __main
    entry5.o(.ARM.Collect$$$$00000004) refers to init.o(.text) for __scatterload
    entry9a.o(.ARM.Collect$$$$0000000B) refers to main.o(i.main) for main
    entry9b.o(.ARM.Collect$$$$0000000C) refers to main.o(i.main) for main
    dadd.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    dadd.o(.text) refers to llsshr.o(.text) for __aeabi_lasr
    dadd.o(.text) refers to depilogue.o(.text) for _double_epilogue
    dmul.o(.text) refers to depilogue.o(.text) for _double_epilogue
    ddiv.o(.text) refers to depilogue.o(.text) for _double_round
    dfixul.o(.text) refers to llushr.o(.text) for __aeabi_llsr
    dfixul.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    init.o(.text) refers to entry5.o(.ARM.Collect$$$$00000004) for __main_after_scatterload
    depilogue.o(.text) refers to llshl.o(.text) for __aeabi_llsl
    depilogue.o(.text) refers to llushr.o(.text) for __aeabi_llsr


==============================================================================

Removing Unused input sections from the image.

    Removing main.o(.rev16_text), (4 bytes).
    Removing main.o(.revsh_text), (4 bytes).
    Removing main.o(.rrx_text), (6 bytes).
    Removing main.o(i.assert_nrf_callback), (24 bytes).
    Removing boards.o(.rev16_text), (4 bytes).
    Removing boards.o(.revsh_text), (4 bytes).
    Removing boards.o(.rrx_text), (6 bytes).
    Removing boards.o(i.bsp_board_buttons_init), (44 bytes).
    Removing boards.o(i.bsp_board_led_idx_to_pin), (12 bytes).
    Removing boards.o(i.bsp_board_pin_to_led_idx), (36 bytes).
    Removing bsp.o(.rev16_text), (4 bytes).
    Removing bsp.o(.revsh_text), (4 bytes).
    Removing bsp.o(.rrx_text), (6 bytes).
    Removing bsp.o(i.bsp_buttons_disable), (8 bytes).
    Removing bsp.o(i.bsp_buttons_enable), (8 bytes).
    Removing bsp.o(i.bsp_wakeup_button_disable), (22 bytes).
    Removing bsp_btn_ble.o(.rev16_text), (4 bytes).
    Removing bsp_btn_ble.o(.revsh_text), (4 bytes).
    Removing bsp_btn_ble.o(.rrx_text), (6 bytes).
    Removing bsp_nfc.o(.rev16_text), (4 bytes).
    Removing bsp_nfc.o(.revsh_text), (4 bytes).
    Removing bsp_nfc.o(.rrx_text), (6 bytes).
    Removing bsp_nfc.o(i.bsp_nfc_btn_deinit), (20 bytes).
    Removing bsp_nfc.o(i.bsp_nfc_btn_init), (20 bytes).
    Removing bsp_nfc.o(i.bsp_nfc_sleep_mode_prepare), (48 bytes).
    Removing ble_advdata.o(.rev16_text), (4 bytes).
    Removing ble_advdata.o(.revsh_text), (4 bytes).
    Removing ble_advdata.o(.rrx_text), (6 bytes).
    Removing ble_advdata.o(i.advdata_check), (18 bytes).
    Removing ble_advdata.o(i.appearance_encode), (82 bytes).
    Removing ble_advdata.o(i.ble_advdata_encode), (364 bytes).
    Removing ble_advdata.o(i.ble_advdata_set), (148 bytes).
    Removing ble_advdata.o(i.ble_device_addr_encode), (118 bytes).
    Removing ble_advdata.o(i.conn_int_check), (90 bytes).
    Removing ble_advdata.o(i.conn_int_encode), (104 bytes).
    Removing ble_advdata.o(i.flags_encode), (54 bytes).
    Removing ble_advdata.o(i.manuf_specific_data_encode), (118 bytes).
    Removing ble_advdata.o(i.name_encode), (194 bytes).
    Removing ble_advdata.o(i.service_data_encode), (150 bytes).
    Removing ble_advdata.o(i.srdata_check), (14 bytes).
    Removing ble_advdata.o(i.tx_power_level_encode), (54 bytes).
    Removing ble_advdata.o(i.uint16_encode), (12 bytes).
    Removing ble_advdata.o(i.uuid_list_encode), (78 bytes).
    Removing ble_advdata.o(i.uuid_list_sized_encode), (220 bytes).
    Removing ble_db_discovery.o(.rev16_text), (4 bytes).
    Removing ble_db_discovery.o(.revsh_text), (4 bytes).
    Removing ble_db_discovery.o(.rrx_text), (6 bytes).
    Removing ble_db_discovery.o(i.ble_db_discovery_close), (28 bytes).
    Removing ble_srv_common.o(.rev16_text), (4 bytes).
    Removing ble_srv_common.o(.revsh_text), (4 bytes).
    Removing ble_srv_common.o(.rrx_text), (6 bytes).
    Removing ble_srv_common.o(i.ble_srv_ascii_to_utf8), (18 bytes).
    Removing ble_srv_common.o(i.ble_srv_is_indication_enabled), (18 bytes).
    Removing ble_srv_common.o(i.ble_srv_is_notification_enabled), (18 bytes).
    Removing ble_srv_common.o(i.ble_srv_report_ref_encode), (60 bytes).
    Removing ble_srv_common.o(i.characteristic_add), (456 bytes).
    Removing ble_srv_common.o(i.descriptor_add), (190 bytes).
    Removing ble_srv_common.o(i.set_security_req), (190 bytes).
    Removing ble_srv_common.o(i.uint16_decode), (12 bytes).
    Removing nrf_ble_gatt.o(.rev16_text), (4 bytes).
    Removing nrf_ble_gatt.o(.revsh_text), (4 bytes).
    Removing nrf_ble_gatt.o(.rrx_text), (6 bytes).
    Removing nrf_ble_gatt.o(i.nrf_ble_gatt_att_mtu_periph_set), (30 bytes).
    Removing nrf_ble_gatt.o(i.nrf_ble_gatt_data_length_get), (48 bytes).
    Removing nrf_ble_gatt.o(i.nrf_ble_gatt_data_length_set), (86 bytes).
    Removing nrf_ble_gatt.o(i.nrf_ble_gatt_eff_mtu_get), (22 bytes).
    Removing ble_nus_c.o(.rev16_text), (4 bytes).
    Removing ble_nus_c.o(.revsh_text), (4 bytes).
    Removing ble_nus_c.o(.rrx_text), (6 bytes).
    Removing nrf_drv_clock.o(.rev16_text), (4 bytes).
    Removing nrf_drv_clock.o(.revsh_text), (4 bytes).
    Removing nrf_drv_clock.o(.rrx_text), (6 bytes).
    Removing nrf_drv_clock.o(i.hfclk_start), (36 bytes).
    Removing nrf_drv_clock.o(i.hfclk_stop), (44 bytes).
    Removing nrf_drv_clock.o(i.item_enqueue), (34 bytes).
    Removing nrf_drv_clock.o(i.lfclk_start), (24 bytes).
    Removing nrf_drv_clock.o(i.nrf_clock_hf_is_running), (32 bytes).
    Removing nrf_drv_clock.o(i.nrf_clock_int_enable), (12 bytes).
    Removing nrf_drv_clock.o(i.nrf_drv_clock_calibration_abort), (6 bytes).
    Removing nrf_drv_clock.o(i.nrf_drv_clock_calibration_start), (8 bytes).
    Removing nrf_drv_clock.o(i.nrf_drv_clock_hfclk_is_running), (32 bytes).
    Removing nrf_drv_clock.o(i.nrf_drv_clock_hfclk_release), (48 bytes).
    Removing nrf_drv_clock.o(i.nrf_drv_clock_hfclk_request), (108 bytes).
    Removing nrf_drv_clock.o(i.nrf_drv_clock_init_check), (12 bytes).
    Removing nrf_drv_clock.o(i.nrf_drv_clock_is_calibrating), (8 bytes).
    Removing nrf_drv_clock.o(i.nrf_drv_clock_lfclk_is_running), (18 bytes).
    Removing nrf_drv_clock.o(i.nrf_drv_clock_lfclk_request), (108 bytes).
    Removing nrf_drv_clock.o(i.nrf_drv_clock_uninit), (36 bytes).
    Removing nrf_drv_clock.o(.constdata), (112 bytes).
    Removing nrf_drv_common.o(.rev16_text), (4 bytes).
    Removing nrf_drv_common.o(.revsh_text), (4 bytes).
    Removing nrf_drv_common.o(.rrx_text), (6 bytes).
    Removing nrf_drv_common.o(i.nrf_drv_common_clock_irq_disable), (28 bytes).
    Removing nrf_drv_gpiote.o(.rev16_text), (4 bytes).
    Removing nrf_drv_gpiote.o(.revsh_text), (4 bytes).
    Removing nrf_drv_gpiote.o(.rrx_text), (6 bytes).
    Removing nrf_drv_gpiote.o(i.nrf_drv_gpiote_clr_task_addr_get), (24 bytes).
    Removing nrf_drv_gpiote.o(i.nrf_drv_gpiote_clr_task_trigger), (32 bytes).
    Removing nrf_drv_gpiote.o(i.nrf_drv_gpiote_in_event_addr_get), (38 bytes).
    Removing nrf_drv_gpiote.o(i.nrf_drv_gpiote_in_event_disable), (84 bytes).
    Removing nrf_drv_gpiote.o(i.nrf_drv_gpiote_in_uninit), (58 bytes).
    Removing nrf_drv_gpiote.o(i.nrf_drv_gpiote_out_clear), (12 bytes).
    Removing nrf_drv_gpiote.o(i.nrf_drv_gpiote_out_init), (204 bytes).
    Removing nrf_drv_gpiote.o(i.nrf_drv_gpiote_out_set), (12 bytes).
    Removing nrf_drv_gpiote.o(i.nrf_drv_gpiote_out_task_addr_get), (22 bytes).
    Removing nrf_drv_gpiote.o(i.nrf_drv_gpiote_out_task_disable), (36 bytes).
    Removing nrf_drv_gpiote.o(i.nrf_drv_gpiote_out_task_enable), (44 bytes).
    Removing nrf_drv_gpiote.o(i.nrf_drv_gpiote_out_task_force), (48 bytes).
    Removing nrf_drv_gpiote.o(i.nrf_drv_gpiote_out_task_trigger), (32 bytes).
    Removing nrf_drv_gpiote.o(i.nrf_drv_gpiote_out_toggle), (46 bytes).
    Removing nrf_drv_gpiote.o(i.nrf_drv_gpiote_out_uninit), (52 bytes).
    Removing nrf_drv_gpiote.o(i.nrf_drv_gpiote_set_task_addr_get), (24 bytes).
    Removing nrf_drv_gpiote.o(i.nrf_drv_gpiote_set_task_trigger), (32 bytes).
    Removing nrf_drv_gpiote.o(i.nrf_drv_gpiote_uninit), (68 bytes).
    Removing nrf_drv_gpiote.o(i.nrf_gpio_cfg_default), (24 bytes).
    Removing nrf_drv_gpiote.o(i.nrf_gpio_pin_clear), (26 bytes).
    Removing nrf_drv_gpiote.o(i.nrf_gpio_pin_set), (26 bytes).
    Removing nrf_drv_gpiote.o(i.nrf_gpiote_task_addr_get), (12 bytes).
    Removing nrf_drv_gpiote.o(i.nrf_gpiote_te_default), (16 bytes).
    Removing nrf_drv_uart.o(.rev16_text), (4 bytes).
    Removing nrf_drv_uart.o(.revsh_text), (4 bytes).
    Removing nrf_drv_uart.o(.rrx_text), (6 bytes).
    Removing nrf_drv_uart.o(i.nrf_drv_common_irq_disable), (28 bytes).
    Removing nrf_drv_uart.o(i.nrf_drv_uart_errorsrc_get), (64 bytes).
    Removing nrf_drv_uart.o(i.nrf_drv_uart_rx_abort), (52 bytes).
    Removing nrf_drv_uart.o(i.nrf_drv_uart_rx_disable), (44 bytes).
    Removing nrf_drv_uart.o(i.nrf_drv_uart_rx_ready), (44 bytes).
    Removing nrf_drv_uart.o(i.nrf_drv_uart_tx_abort), (100 bytes).
    Removing nrf_drv_uart.o(i.nrf_drv_uart_uninit), (140 bytes).
    Removing nrf_drv_uart.o(i.nrf_gpio_cfg_default), (24 bytes).
    Removing nrf_drv_uart.o(i.pins_to_default), (216 bytes).
    Removing app_button.o(.rev16_text), (4 bytes).
    Removing app_button.o(.revsh_text), (4 bytes).
    Removing app_button.o(.rrx_text), (6 bytes).
    Removing app_button.o(i.app_button_disable), (52 bytes).
    Removing app_button.o(i.app_button_is_pushed), (44 bytes).
    Removing app_error.o(.rev16_text), (4 bytes).
    Removing app_error.o(.revsh_text), (4 bytes).
    Removing app_error.o(.rrx_text), (6 bytes).
    Removing app_error.o(i.app_error_handler), (32 bytes).
    Removing app_error.o(i.app_error_save_and_stop), (136 bytes).
    Removing app_error.o(.bss), (32 bytes).
    Removing app_error_weak.o(.rev16_text), (4 bytes).
    Removing app_error_weak.o(.revsh_text), (4 bytes).
    Removing app_error_weak.o(.rrx_text), (6 bytes).
    Removing app_fifo.o(.rev16_text), (4 bytes).
    Removing app_fifo.o(.revsh_text), (4 bytes).
    Removing app_fifo.o(.rrx_text), (6 bytes).
    Removing app_fifo.o(i.app_fifo_flush), (10 bytes).
    Removing app_fifo.o(i.app_fifo_peek), (36 bytes).
    Removing app_fifo.o(i.app_fifo_read), (102 bytes).
    Removing app_fifo.o(i.app_fifo_write), (106 bytes).
    Removing app_scheduler.o(.rev16_text), (4 bytes).
    Removing app_scheduler.o(.revsh_text), (4 bytes).
    Removing app_scheduler.o(.rrx_text), (6 bytes).
    Removing app_scheduler.o(i.app_sched_event_put), (184 bytes).
    Removing app_scheduler.o(i.app_sched_execute), (116 bytes).
    Removing app_scheduler.o(i.app_sched_init), (92 bytes).
    Removing app_scheduler.o(i.app_sched_queue_space_get), (52 bytes).
    Removing app_scheduler.o(i.next_index), (24 bytes).
    Removing app_scheduler.o(.data), (14 bytes).
    Removing app_timer.o(.rev16_text), (4 bytes).
    Removing app_timer.o(.revsh_text), (4 bytes).
    Removing app_timer.o(.rrx_text), (6 bytes).
    Removing app_timer.o(i.app_timer_cnt_diff_compute), (16 bytes).
    Removing app_timer.o(i.app_timer_cnt_get), (8 bytes).
    Removing app_timer.o(i.app_timer_pause), (12 bytes).
    Removing app_timer.o(i.app_timer_resume), (12 bytes).
    Removing app_timer.o(i.app_timer_stop_all), (32 bytes).
    Removing app_uart_fifo.o(.rev16_text), (4 bytes).
    Removing app_uart_fifo.o(.revsh_text), (4 bytes).
    Removing app_uart_fifo.o(.rrx_text), (6 bytes).
    Removing app_uart_fifo.o(i.app_uart_close), (16 bytes).
    Removing app_uart_fifo.o(i.app_uart_flush), (52 bytes).
    Removing app_util_platform.o(.rev16_text), (4 bytes).
    Removing app_util_platform.o(.revsh_text), (4 bytes).
    Removing app_util_platform.o(.rrx_text), (6 bytes).
    Removing app_util_platform.o(i.app_util_disable_irq), (20 bytes).
    Removing app_util_platform.o(i.app_util_enable_irq), (24 bytes).
    Removing app_util_platform.o(i.current_int_priority_get), (60 bytes).
    Removing app_util_platform.o(i.privilege_level_get), (34 bytes).
    Removing app_util_platform.o(.data), (4 bytes).
    Removing hardfault_implementation.o(.rev16_text), (4 bytes).
    Removing hardfault_implementation.o(.revsh_text), (4 bytes).
    Removing hardfault_implementation.o(.rrx_text), (6 bytes).
    Removing nrf_assert.o(.rev16_text), (4 bytes).
    Removing nrf_assert.o(.revsh_text), (4 bytes).
    Removing nrf_assert.o(.rrx_text), (6 bytes).
    Removing nrf_assert.o(i.assert_nrf_callback), (26 bytes).
    Removing nrf_atfifo.o(.rev16_text), (4 bytes).
    Removing nrf_atfifo.o(.revsh_text), (4 bytes).
    Removing nrf_atfifo.o(.rrx_text), (6 bytes).
    Removing nrf_atfifo.o(.emb_text), (200 bytes).
    Removing nrf_atfifo.o(i.nrf_atfifo_alloc_put), (58 bytes).
    Removing nrf_atfifo.o(i.nrf_atfifo_clear), (22 bytes).
    Removing nrf_atfifo.o(i.nrf_atfifo_get_free), (58 bytes).
    Removing nrf_atfifo.o(i.nrf_atfifo_init), (40 bytes).
    Removing nrf_atfifo.o(i.nrf_atfifo_item_alloc), (28 bytes).
    Removing nrf_atfifo.o(i.nrf_atfifo_item_free), (28 bytes).
    Removing nrf_atfifo.o(i.nrf_atfifo_item_get), (28 bytes).
    Removing nrf_atfifo.o(i.nrf_atfifo_item_put), (28 bytes).
    Removing nrf_balloc.o(.rev16_text), (4 bytes).
    Removing nrf_balloc.o(.revsh_text), (4 bytes).
    Removing nrf_balloc.o(.rrx_text), (6 bytes).
    Removing nrf_fprintf.o(.rev16_text), (4 bytes).
    Removing nrf_fprintf.o(.revsh_text), (4 bytes).
    Removing nrf_fprintf.o(.rrx_text), (6 bytes).
    Removing nrf_fprintf_format.o(.rev16_text), (4 bytes).
    Removing nrf_fprintf_format.o(.revsh_text), (4 bytes).
    Removing nrf_fprintf_format.o(.rrx_text), (6 bytes).
    Removing nrf_memobj.o(.rev16_text), (4 bytes).
    Removing nrf_memobj.o(.revsh_text), (4 bytes).
    Removing nrf_memobj.o(.rrx_text), (6 bytes).
    Removing nrf_pwr_mgmt.o(.rev16_text), (4 bytes).
    Removing nrf_pwr_mgmt.o(.revsh_text), (4 bytes).
    Removing nrf_pwr_mgmt.o(.rrx_text), (6 bytes).
    Removing nrf_pwr_mgmt.o(i.nrf_pwr_mgmt_feed), (2 bytes).
    Removing nrf_section_iter.o(.rev16_text), (4 bytes).
    Removing nrf_section_iter.o(.revsh_text), (4 bytes).
    Removing nrf_section_iter.o(.rrx_text), (6 bytes).
    Removing nrf_strerror.o(.rev16_text), (4 bytes).
    Removing nrf_strerror.o(.revsh_text), (4 bytes).
    Removing nrf_strerror.o(.rrx_text), (6 bytes).
    Removing retarget.o(.rev16_text), (4 bytes).
    Removing retarget.o(.revsh_text), (4 bytes).
    Removing retarget.o(.rrx_text), (6 bytes).
    Removing retarget.o(i.fgetc), (22 bytes).
    Removing nrf_log_backend_rtt.o(.rev16_text), (4 bytes).
    Removing nrf_log_backend_rtt.o(.revsh_text), (4 bytes).
    Removing nrf_log_backend_rtt.o(.rrx_text), (6 bytes).
    Removing nrf_log_backend_serial.o(.rev16_text), (4 bytes).
    Removing nrf_log_backend_serial.o(.revsh_text), (4 bytes).
    Removing nrf_log_backend_serial.o(.rrx_text), (6 bytes).
    Removing nrf_log_default_backends.o(.rev16_text), (4 bytes).
    Removing nrf_log_default_backends.o(.revsh_text), (4 bytes).
    Removing nrf_log_default_backends.o(.rrx_text), (6 bytes).
    Removing nrf_log_frontend.o(.rev16_text), (4 bytes).
    Removing nrf_log_frontend.o(.revsh_text), (4 bytes).
    Removing nrf_log_frontend.o(.rrx_text), (6 bytes).
    Removing nrf_log_frontend.o(i.cont_buf_prealloc), (172 bytes).
    Removing nrf_log_frontend.o(i.higher_lvl_get), (34 bytes).
    Removing nrf_log_frontend.o(i.nrf_log_backend_remove), (44 bytes).
    Removing nrf_log_frontend.o(i.nrf_log_frontend_hexdump), (224 bytes).
    Removing nrf_log_frontend.o(i.nrf_log_frontend_std_3), (40 bytes).
    Removing nrf_log_frontend.o(i.nrf_log_frontend_std_4), (44 bytes).
    Removing nrf_log_frontend.o(i.nrf_log_frontend_std_5), (56 bytes).
    Removing nrf_log_frontend.o(i.nrf_log_module_filter_get), (52 bytes).
    Removing nrf_log_frontend.o(i.nrf_log_module_filter_set), (2 bytes).
    Removing nrf_log_frontend.o(i.nrf_log_push), (120 bytes).
    Removing nrf_log_str_formatter.o(.rev16_text), (4 bytes).
    Removing nrf_log_str_formatter.o(.revsh_text), (4 bytes).
    Removing nrf_log_str_formatter.o(.rrx_text), (6 bytes).
    Removing segger_rtt.o(.rev16_text), (4 bytes).
    Removing segger_rtt.o(.revsh_text), (4 bytes).
    Removing segger_rtt.o(.rrx_text), (6 bytes).
    Removing segger_rtt.o(i.SEGGER_RTT_AllocDownBuffer), (184 bytes).
    Removing segger_rtt.o(i.SEGGER_RTT_AllocUpBuffer), (184 bytes).
    Removing segger_rtt.o(i.SEGGER_RTT_ConfigDownBuffer), (160 bytes).
    Removing segger_rtt.o(i.SEGGER_RTT_ConfigUpBuffer), (160 bytes).
    Removing segger_rtt.o(i.SEGGER_RTT_GetKey), (32 bytes).
    Removing segger_rtt.o(i.SEGGER_RTT_HasData), (28 bytes).
    Removing segger_rtt.o(i.SEGGER_RTT_HasKey), (40 bytes).
    Removing segger_rtt.o(i.SEGGER_RTT_PutChar), (112 bytes).
    Removing segger_rtt.o(i.SEGGER_RTT_PutCharSkip), (96 bytes).
    Removing segger_rtt.o(i.SEGGER_RTT_PutCharSkipNoLock), (56 bytes).
    Removing segger_rtt.o(i.SEGGER_RTT_Read), (42 bytes).
    Removing segger_rtt.o(i.SEGGER_RTT_ReadNoLock), (152 bytes).
    Removing segger_rtt.o(i.SEGGER_RTT_SetFlagsDownBuffer), (76 bytes).
    Removing segger_rtt.o(i.SEGGER_RTT_SetFlagsUpBuffer), (76 bytes).
    Removing segger_rtt.o(i.SEGGER_RTT_SetNameDownBuffer), (76 bytes).
    Removing segger_rtt.o(i.SEGGER_RTT_SetNameUpBuffer), (76 bytes).
    Removing segger_rtt.o(i.SEGGER_RTT_SetTerminal), (144 bytes).
    Removing segger_rtt.o(i.SEGGER_RTT_TerminalOut), (244 bytes).
    Removing segger_rtt.o(i.SEGGER_RTT_WaitKey), (14 bytes).
    Removing segger_rtt.o(i.SEGGER_RTT_Write), (60 bytes).
    Removing segger_rtt.o(i.SEGGER_RTT_WriteSkipNoLock), (176 bytes).
    Removing segger_rtt.o(i.SEGGER_RTT_WriteString), (26 bytes).
    Removing segger_rtt.o(i.SEGGER_RTT_WriteWithOverwriteNoLock), (172 bytes).
    Removing segger_rtt.o(i._PostTerminalSwitch), (36 bytes).
    Removing segger_rtt.o(.data), (17 bytes).
    Removing segger_rtt_printf.o(.rev16_text), (4 bytes).
    Removing segger_rtt_printf.o(.revsh_text), (4 bytes).
    Removing segger_rtt_printf.o(.rrx_text), (6 bytes).
    Removing segger_rtt_printf.o(i.SEGGER_RTT_printf), (34 bytes).
    Removing segger_rtt_printf.o(i.SEGGER_RTT_vprintf), (522 bytes).
    Removing segger_rtt_printf.o(i._PrintInt), (236 bytes).
    Removing segger_rtt_printf.o(i._PrintUnsigned), (236 bytes).
    Removing segger_rtt_printf.o(i._StoreChar), (68 bytes).
    Removing segger_rtt_printf.o(.constdata), (16 bytes).
    Removing nrf_sdh.o(.rev16_text), (4 bytes).
    Removing nrf_sdh.o(.revsh_text), (4 bytes).
    Removing nrf_sdh.o(.rrx_text), (6 bytes).
    Removing nrf_sdh.o(i.nrf_sdh_disable_request), (80 bytes).
    Removing nrf_sdh.o(i.nrf_sdh_is_suspended), (28 bytes).
    Removing nrf_sdh.o(i.nrf_sdh_request_continue), (40 bytes).
    Removing nrf_sdh.o(i.nrf_sdh_resume), (100 bytes).
    Removing nrf_sdh.o(i.nrf_sdh_suspend), (32 bytes).
    Removing nrf_sdh.o(i.softdevice_evt_irq_disable), (108 bytes).
    Removing nrf_sdh_ble.o(.rev16_text), (4 bytes).
    Removing nrf_sdh_ble.o(.revsh_text), (4 bytes).
    Removing nrf_sdh_ble.o(.rrx_text), (6 bytes).
    Removing nrf_sdh_soc.o(.rev16_text), (4 bytes).
    Removing nrf_sdh_soc.o(.revsh_text), (4 bytes).
    Removing nrf_sdh_soc.o(.rrx_text), (6 bytes).
    Removing arm_startup_nrf52840.o(HEAP), (8192 bytes).
    Removing system_nrf52840.o(.rev16_text), (4 bytes).
    Removing system_nrf52840.o(.revsh_text), (4 bytes).
    Removing system_nrf52840.o(.rrx_text), (6 bytes).
    Removing dadd.o(.text), (334 bytes).
    Removing dmul.o(.text), (228 bytes).
    Removing ddiv.o(.text), (222 bytes).
    Removing dfixul.o(.text), (48 bytes).
    Removing cdrcmple.o(.text), (48 bytes).
    Removing depilogue.o(.text), (186 bytes).

314 unused section(s) (total 22089 bytes) removed from the image.

==============================================================================

Image Symbol Table

    Local Symbols

    Symbol Name                              Value     Ov Type        Size  Object(Section)

    ../clib/../cmprslib/zerorunl2.c          0x00000000   Number         0  __dczerorl2.o ABSOLUTE
    ../clib/microlib/ctype/ctype.c           0x00000000   Number         0  isblank_o.o ABSOLUTE
    ../clib/microlib/ctype/ctype.c           0x00000000   Number         0  isalpha_o.o ABSOLUTE
    ../clib/microlib/ctype/ctype.c           0x00000000   Number         0  isalnum_o.o ABSOLUTE
    ../clib/microlib/ctype/ctype.c           0x00000000   Number         0  isprint_o.o ABSOLUTE
    ../clib/microlib/ctype/ctype.c           0x00000000   Number         0  iscntrl_o.o ABSOLUTE
    ../clib/microlib/ctype/ctype.c           0x00000000   Number         0  isdigit_o.o ABSOLUTE
    ../clib/microlib/ctype/ctype.c           0x00000000   Number         0  isgraph_o.o ABSOLUTE
    ../clib/microlib/ctype/ctype.c           0x00000000   Number         0  islower_o.o ABSOLUTE
    ../clib/microlib/ctype/ctype.c           0x00000000   Number         0  isspace_o.o ABSOLUTE
    ../clib/microlib/ctype/ctype.c           0x00000000   Number         0  ispunct_o.o ABSOLUTE
    ../clib/microlib/ctype/ctype.c           0x00000000   Number         0  ctype_o.o ABSOLUTE
    ../clib/microlib/ctype/ctype.c           0x00000000   Number         0  isxdigit_o.o ABSOLUTE
    ../clib/microlib/ctype/ctype.c           0x00000000   Number         0  isupper_o.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  uidiv.o ABSOLUTE
    ../clib/microlib/division.c              0x00000000   Number         0  uldiv.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry11b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry10b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry11a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry10a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry9b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry9a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry7a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry8b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry8a.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry2.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry5.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry7b.o ABSOLUTE
    ../clib/microlib/init/entry.s            0x00000000   Number         0  entry.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llushr.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llsshr.o ABSOLUTE
    ../clib/microlib/longlong.c              0x00000000   Number         0  llshl.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printfa.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf5.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf4.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf3.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf0.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printfb.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf7.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf2.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf6.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf8.o ABSOLUTE
    ../clib/microlib/printf/printf.c         0x00000000   Number         0  printf1.o ABSOLUTE
    ../clib/microlib/string/memcpy.c         0x00000000   Number         0  memcpyb.o ABSOLUTE
    ../clib/microlib/string/memcpy.c         0x00000000   Number         0  memcpya.o ABSOLUTE
    ../clib/microlib/string/memset.c         0x00000000   Number         0  memseta.o ABSOLUTE
    ../clib/microlib/string/strcpy.c         0x00000000   Number         0  strcpy.o ABSOLUTE
    ../clib/microlib/string/strlen.c         0x00000000   Number         0  strlen.o ABSOLUTE
    ../clib/microlib/stubs.s                 0x00000000   Number         0  iusefp.o ABSOLUTE
    ../fplib/microlib/fpadd.c                0x00000000   Number         0  dadd.o ABSOLUTE
    ../fplib/microlib/fpdiv.c                0x00000000   Number         0  ddiv.o ABSOLUTE
    ../fplib/microlib/fpepilogue.c           0x00000000   Number         0  depilogue.o ABSOLUTE
    ../fplib/microlib/fpfix.c                0x00000000   Number         0  dfixul.o ABSOLUTE
    ../fplib/microlib/fpmul.c                0x00000000   Number         0  dmul.o ABSOLUTE
    ..\..\..\..\..\..\components\ble\ble_db_discovery\ble_db_discovery.c 0x00000000   Number         0  ble_db_discovery.o ABSOLUTE
    ..\..\..\..\..\..\components\ble\ble_services\ble_nus_c\ble_nus_c.c 0x00000000   Number         0  ble_nus_c.o ABSOLUTE
    ..\..\..\..\..\..\components\ble\common\ble_advdata.c 0x00000000   Number         0  ble_advdata.o ABSOLUTE
    ..\..\..\..\..\..\components\ble\common\ble_srv_common.c 0x00000000   Number         0  ble_srv_common.o ABSOLUTE
    ..\..\..\..\..\..\components\ble\nrf_ble_gatt\nrf_ble_gatt.c 0x00000000   Number         0  nrf_ble_gatt.o ABSOLUTE
    ..\..\..\..\..\..\components\boards\boards.c 0x00000000   Number         0  boards.o ABSOLUTE
    ..\..\..\..\..\..\components\drivers_nrf\clock\nrf_drv_clock.c 0x00000000   Number         0  nrf_drv_clock.o ABSOLUTE
    ..\..\..\..\..\..\components\drivers_nrf\common\nrf_drv_common.c 0x00000000   Number         0  nrf_drv_common.o ABSOLUTE
    ..\..\..\..\..\..\components\drivers_nrf\gpiote\nrf_drv_gpiote.c 0x00000000   Number         0  nrf_drv_gpiote.o ABSOLUTE
    ..\..\..\..\..\..\components\drivers_nrf\uart\nrf_drv_uart.c 0x00000000   Number         0  nrf_drv_uart.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\atomic_fifo\nrf_atfifo.c 0x00000000   Number         0  nrf_atfifo.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\balloc\nrf_balloc.c 0x00000000   Number         0  nrf_balloc.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\bsp\bsp.c 0x00000000   Number         0  bsp.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\bsp\bsp_btn_ble.c 0x00000000   Number         0  bsp_btn_ble.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\bsp\bsp_nfc.c 0x00000000   Number         0  bsp_nfc.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\button\app_button.c 0x00000000   Number         0  app_button.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\experimental_log\src\nrf_log_backend_rtt.c 0x00000000   Number         0  nrf_log_backend_rtt.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\experimental_log\src\nrf_log_backend_serial.c 0x00000000   Number         0  nrf_log_backend_serial.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\experimental_log\src\nrf_log_default_backends.c 0x00000000   Number         0  nrf_log_default_backends.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\experimental_log\src\nrf_log_frontend.c 0x00000000   Number         0  nrf_log_frontend.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\experimental_log\src\nrf_log_str_formatter.c 0x00000000   Number         0  nrf_log_str_formatter.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\experimental_memobj\nrf_memobj.c 0x00000000   Number         0  nrf_memobj.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\experimental_section_vars\nrf_section_iter.c 0x00000000   Number         0  nrf_section_iter.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\fifo\app_fifo.c 0x00000000   Number         0  app_fifo.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\hardfault\hardfault_implementation.c 0x00000000   Number         0  hardfault_implementation.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\pwr_mgmt\nrf_pwr_mgmt.c 0x00000000   Number         0  nrf_pwr_mgmt.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\scheduler\app_scheduler.c 0x00000000   Number         0  app_scheduler.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\strerror\nrf_strerror.c 0x00000000   Number         0  nrf_strerror.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\timer\app_timer.c 0x00000000   Number         0  app_timer.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\uart\app_uart_fifo.c 0x00000000   Number         0  app_uart_fifo.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\uart\retarget.c 0x00000000   Number         0  retarget.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\util\app_error.c 0x00000000   Number         0  app_error.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\util\app_error_weak.c 0x00000000   Number         0  app_error_weak.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\util\app_util_platform.c 0x00000000   Number         0  app_util_platform.o ABSOLUTE
    ..\..\..\..\..\..\components\libraries\util\nrf_assert.c 0x00000000   Number         0  nrf_assert.o ABSOLUTE
    ..\..\..\..\..\..\components\softdevice\common\nrf_sdh.c 0x00000000   Number         0  nrf_sdh.o ABSOLUTE
    ..\..\..\..\..\..\components\softdevice\common\nrf_sdh_ble.c 0x00000000   Number         0  nrf_sdh_ble.o ABSOLUTE
    ..\..\..\..\..\..\components\softdevice\common\nrf_sdh_soc.c 0x00000000   Number         0  nrf_sdh_soc.o ABSOLUTE
    ..\..\..\..\..\..\external\fprintf\nrf_fprintf.c 0x00000000   Number         0  nrf_fprintf.o ABSOLUTE
    ..\..\..\..\..\..\external\fprintf\nrf_fprintf_format.c 0x00000000   Number         0  nrf_fprintf_format.o ABSOLUTE
    ..\..\..\..\..\..\external\segger_rtt\SEGGER_RTT.c 0x00000000   Number         0  segger_rtt.o ABSOLUTE
    ..\..\..\..\..\..\external\segger_rtt\SEGGER_RTT_Syscalls_KEIL.c 0x00000000   Number         0  segger_rtt_syscalls_keil.o ABSOLUTE
    ..\..\..\..\..\..\external\segger_rtt\SEGGER_RTT_printf.c 0x00000000   Number         0  segger_rtt_printf.o ABSOLUTE
    ..\..\..\main.c                          0x00000000   Number         0  main.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\ble\\ble_db_discovery\\ble_db_discovery.c 0x00000000   Number         0  ble_db_discovery.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\ble\\ble_services\\ble_nus_c\\ble_nus_c.c 0x00000000   Number         0  ble_nus_c.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\ble\\common\\ble_advdata.c 0x00000000   Number         0  ble_advdata.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\ble\\common\\ble_srv_common.c 0x00000000   Number         0  ble_srv_common.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\ble\\nrf_ble_gatt\\nrf_ble_gatt.c 0x00000000   Number         0  nrf_ble_gatt.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\boards\\boards.c 0x00000000   Number         0  boards.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\drivers_nrf\\clock\\nrf_drv_clock.c 0x00000000   Number         0  nrf_drv_clock.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\drivers_nrf\\common\\nrf_drv_common.c 0x00000000   Number         0  nrf_drv_common.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\drivers_nrf\\gpiote\\nrf_drv_gpiote.c 0x00000000   Number         0  nrf_drv_gpiote.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\drivers_nrf\\uart\\nrf_drv_uart.c 0x00000000   Number         0  nrf_drv_uart.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\atomic_fifo\\nrf_atfifo.c 0x00000000   Number         0  nrf_atfifo.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\balloc\\nrf_balloc.c 0x00000000   Number         0  nrf_balloc.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\bsp\\bsp.c 0x00000000   Number         0  bsp.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\bsp\\bsp_btn_ble.c 0x00000000   Number         0  bsp_btn_ble.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\bsp\\bsp_nfc.c 0x00000000   Number         0  bsp_nfc.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\button\\app_button.c 0x00000000   Number         0  app_button.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\experimental_log\\src\\nrf_log_backend_rtt.c 0x00000000   Number         0  nrf_log_backend_rtt.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\experimental_log\\src\\nrf_log_backend_serial.c 0x00000000   Number         0  nrf_log_backend_serial.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\experimental_log\\src\\nrf_log_default_backends.c 0x00000000   Number         0  nrf_log_default_backends.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\experimental_log\\src\\nrf_log_frontend.c 0x00000000   Number         0  nrf_log_frontend.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\experimental_log\\src\\nrf_log_str_formatter.c 0x00000000   Number         0  nrf_log_str_formatter.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\experimental_memobj\\nrf_memobj.c 0x00000000   Number         0  nrf_memobj.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\experimental_section_vars\\nrf_section_iter.c 0x00000000   Number         0  nrf_section_iter.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\fifo\\app_fifo.c 0x00000000   Number         0  app_fifo.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\hardfault\\hardfault_implementation.c 0x00000000   Number         0  hardfault_implementation.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\pwr_mgmt\\nrf_pwr_mgmt.c 0x00000000   Number         0  nrf_pwr_mgmt.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\scheduler\\app_scheduler.c 0x00000000   Number         0  app_scheduler.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\strerror\\nrf_strerror.c 0x00000000   Number         0  nrf_strerror.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\timer\\app_timer.c 0x00000000   Number         0  app_timer.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\uart\\app_uart_fifo.c 0x00000000   Number         0  app_uart_fifo.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\uart\\retarget.c 0x00000000   Number         0  retarget.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\util\\app_error.c 0x00000000   Number         0  app_error.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\util\\app_error_weak.c 0x00000000   Number         0  app_error_weak.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\util\\app_util_platform.c 0x00000000   Number         0  app_util_platform.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\libraries\\util\\nrf_assert.c 0x00000000   Number         0  nrf_assert.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\softdevice\\common\\nrf_sdh.c 0x00000000   Number         0  nrf_sdh.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\softdevice\\common\\nrf_sdh_ble.c 0x00000000   Number         0  nrf_sdh_ble.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\components\\softdevice\\common\\nrf_sdh_soc.c 0x00000000   Number         0  nrf_sdh_soc.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\external\\fprintf\\nrf_fprintf.c 0x00000000   Number         0  nrf_fprintf.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\external\\fprintf\\nrf_fprintf_format.c 0x00000000   Number         0  nrf_fprintf_format.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\external\\segger_rtt\\SEGGER_RTT.c 0x00000000   Number         0  segger_rtt.o ABSOLUTE
    ..\\..\\..\\..\\..\\..\\external\\segger_rtt\\SEGGER_RTT_printf.c 0x00000000   Number         0  segger_rtt_printf.o ABSOLUTE
    ..\\..\\..\\main.c                       0x00000000   Number         0  main.o ABSOLUTE
    RTE\Device\nRF52840_xxAA\arm_startup_nrf52840.s 0x00000000   Number         0  arm_startup_nrf52840.o ABSOLUTE
    RTE\Device\nRF52840_xxAA\system_nrf52840.c 0x00000000   Number         0  system_nrf52840.o ABSOLUTE
    RTE\\Device\\nRF52840_xxAA\\system_nrf52840.c 0x00000000   Number         0  system_nrf52840.o ABSOLUTE
    cdrcmple.s                               0x00000000   Number         0  cdrcmple.o ABSOLUTE
    dc.s                                     0x00000000   Number         0  dc.o ABSOLUTE
    handlers.s                               0x00000000   Number         0  handlers.o ABSOLUTE
    init.s                                   0x00000000   Number         0  init.o ABSOLUTE
    RESET                                    0x00022000   Section      512  arm_startup_nrf52840.o(RESET)
    .ARM.Collect$$$$00000000                 0x00022200   Section        0  entry.o(.ARM.Collect$$$$00000000)
    .ARM.Collect$$$$00000001                 0x00022200   Section        4  entry2.o(.ARM.Collect$$$$00000001)
    .ARM.Collect$$$$00000004                 0x00022204   Section        4  entry5.o(.ARM.Collect$$$$00000004)
    .ARM.Collect$$$$00000008                 0x00022208   Section        0  entry7b.o(.ARM.Collect$$$$00000008)
    .ARM.Collect$$$$0000000A                 0x00022208   Section        0  entry8b.o(.ARM.Collect$$$$0000000A)
    .ARM.Collect$$$$0000000B                 0x00022208   Section        8  entry9a.o(.ARM.Collect$$$$0000000B)
    .ARM.Collect$$$$0000000D                 0x00022210   Section        0  entry10a.o(.ARM.Collect$$$$0000000D)
    .ARM.Collect$$$$0000000F                 0x00022210   Section        0  entry11a.o(.ARM.Collect$$$$0000000F)
    .ARM.Collect$$$$00002712                 0x00022210   Section        4  entry2.o(.ARM.Collect$$$$00002712)
    __lit__00000000                          0x00022210   Data           4  entry2.o(.ARM.Collect$$$$00002712)
    .emb_text                                0x00022214   Section      154  nrf_memobj.o(.emb_text)
    $v0                                      0x00022214   Number         0  nrf_memobj.o(.emb_text)
    .emb_text                                0x000222b0   Section      154  nrf_pwr_mgmt.o(.emb_text)
    $v0                                      0x000222b0   Number         0  nrf_pwr_mgmt.o(.emb_text)
    .emb_text                                0x0002234c   Section      154  nrf_log_frontend.o(.emb_text)
    $v0                                      0x0002234c   Number         0  nrf_log_frontend.o(.emb_text)
    .text                                    0x000223e8   Section       36  arm_startup_nrf52840.o(.text)
    $v0                                      0x000223e8   Number         0  arm_startup_nrf52840.o(.text)
    .text                                    0x0002240c   Section        0  uldiv.o(.text)
    .text                                    0x00022470   Section        0  ctype_o.o(.text)
    .text                                    0x00022478   Section        0  memcpya.o(.text)
    .text                                    0x0002249c   Section        0  memseta.o(.text)
    .text                                    0x000224c0   Section        0  strlen.o(.text)
    .text                                    0x000224ce   Section        0  strcpy.o(.text)
    .text                                    0x000224e0   Section        0  llshl.o(.text)
    .text                                    0x000224fe   Section        0  llushr.o(.text)
    .text                                    0x00022520   Section       36  init.o(.text)
    .text                                    0x00022544   Section        0  __dczerorl2.o(.text)
    i.GPIOTE_IRQHandler                      0x0002259c   Section        0  nrf_drv_gpiote.o(i.GPIOTE_IRQHandler)
    i.NVIC_ClearPendingIRQ                   0x000227dc   Section        0  app_timer.o(i.NVIC_ClearPendingIRQ)
    NVIC_ClearPendingIRQ                     0x000227dd   Thumb Code    18  app_timer.o(i.NVIC_ClearPendingIRQ)
    i.NVIC_EnableIRQ                         0x000227f4   Section        0  app_timer.o(i.NVIC_EnableIRQ)
    NVIC_EnableIRQ                           0x000227f5   Thumb Code    22  app_timer.o(i.NVIC_EnableIRQ)
    i.NVIC_SetPendingIRQ                     0x0002280c   Section        0  app_timer.o(i.NVIC_SetPendingIRQ)
    NVIC_SetPendingIRQ                       0x0002280d   Thumb Code    18  app_timer.o(i.NVIC_SetPendingIRQ)
    i.NVIC_SetPriority                       0x00022824   Section        0  app_timer.o(i.NVIC_SetPriority)
    NVIC_SetPriority                         0x00022825   Thumb Code    32  app_timer.o(i.NVIC_SetPriority)
    i.POWER_CLOCK_IRQHandler                 0x0002284c   Section        0  nrf_drv_clock.o(i.POWER_CLOCK_IRQHandler)
    i.RTC1_IRQHandler                        0x0002289c   Section        0  app_timer.o(i.RTC1_IRQHandler)
    i.SEGGER_RTT_Init                        0x000228d0   Section        0  segger_rtt.o(i.SEGGER_RTT_Init)
    i.SEGGER_RTT_WriteNoLock                 0x000228d8   Section        0  segger_rtt.o(i.SEGGER_RTT_WriteNoLock)
    i.SWI0_EGU0_IRQHandler                   0x0002295c   Section        0  app_timer.o(i.SWI0_EGU0_IRQHandler)
    i.SWI2_EGU2_IRQHandler                   0x00022964   Section        0  nrf_sdh.o(i.SWI2_EGU2_IRQHandler)
    i.SystemCoreClockUpdate                  0x0002296c   Section        0  system_nrf52840.o(i.SystemCoreClockUpdate)
    i.SystemInit                             0x0002297c   Section        0  system_nrf52840.o(i.SystemInit)
    i.UARTE0_UART0_IRQHandler                0x00022bac   Section        0  nrf_drv_uart.o(i.UARTE0_UART0_IRQHandler)
    i._DoInit                                0x00022bd0   Section        0  segger_rtt.o(i._DoInit)
    _DoInit                                  0x00022bd1   Thumb Code    74  segger_rtt.o(i._DoInit)
    i._GetAvailWriteSpace                    0x00022c40   Section        0  segger_rtt.o(i._GetAvailWriteSpace)
    _GetAvailWriteSpace                      0x00022c41   Thumb Code    28  segger_rtt.o(i._GetAvailWriteSpace)
    i._WriteBlocking                         0x00022c5c   Section        0  segger_rtt.o(i._WriteBlocking)
    _WriteBlocking                           0x00022c5d   Thumb Code   114  segger_rtt.o(i._WriteBlocking)
    i._WriteNoCheck                          0x00022cce   Section        0  segger_rtt.o(i._WriteNoCheck)
    _WriteNoCheck                            0x00022ccf   Thumb Code    76  segger_rtt.o(i._WriteNoCheck)
    i.__0printf$bare                         0x00022d1c   Section        0  printfb.o(i.__0printf$bare)
    i.__scatterload_copy                     0x00022d2c   Section       14  handlers.o(i.__scatterload_copy)
    i.__scatterload_null                     0x00022d3a   Section        2  handlers.o(i.__scatterload_null)
    i.__scatterload_zeroinit                 0x00022d3c   Section       14  handlers.o(i.__scatterload_zeroinit)
    i.__sd_nvic_app_accessible_irq           0x00022d4c   Section        0  nrf_sdh.o(i.__sd_nvic_app_accessible_irq)
    __sd_nvic_app_accessible_irq             0x00022d4d   Thumb Code    52  nrf_sdh.o(i.__sd_nvic_app_accessible_irq)
    i.__sd_nvic_irq_disable                  0x00022d84   Section        0  app_util_platform.o(i.__sd_nvic_irq_disable)
    __sd_nvic_irq_disable                    0x00022d85   Thumb Code    12  app_util_platform.o(i.__sd_nvic_irq_disable)
    i._printf_core                           0x00022d90   Section        0  printfb.o(i._printf_core)
    _printf_core                             0x00022d91   Thumb Code    34  printfb.o(i._printf_core)
    i.advertising_buttons_configure          0x00022db2   Section        0  bsp_btn_ble.o(i.advertising_buttons_configure)
    advertising_buttons_configure            0x00022db3   Thumb Code    84  bsp_btn_ble.o(i.advertising_buttons_configure)
    i.alert_timer_handler                    0x00022e06   Section        0  bsp.o(i.alert_timer_handler)
    alert_timer_handler                      0x00022e07   Thumb Code    12  bsp.o(i.alert_timer_handler)
    i.app_button_enable                      0x00022e14   Section        0  app_button.o(i.app_button_enable)
    i.app_button_init                        0x00022e40   Section        0  app_button.o(i.app_button_init)
    i.app_error_fault_handler                0x00022ee8   Section        0  app_error_weak.o(i.app_error_fault_handler)
    i.app_error_handler_bare                 0x00022f98   Section        0  app_error.o(i.app_error_handler_bare)
    i.app_fifo_get                           0x00022fb4   Section        0  app_fifo.o(i.app_fifo_get)
    i.app_fifo_init                          0x00022fd2   Section        0  app_fifo.o(i.app_fifo_init)
    i.app_fifo_put                           0x00022ff6   Section        0  app_fifo.o(i.app_fifo_put)
    i.app_timer_create                       0x00023018   Section        0  app_timer.o(i.app_timer_create)
    i.app_timer_init                         0x00023054   Section        0  app_timer.o(i.app_timer_init)
    i.app_timer_start                        0x000230b0   Section        0  app_timer.o(i.app_timer_start)
    i.app_timer_stop                         0x00023104   Section        0  app_timer.o(i.app_timer_stop)
    i.app_uart_get                           0x00023134   Section        0  app_uart_fifo.o(i.app_uart_get)
    i.app_uart_init                          0x00023188   Section        0  app_uart_fifo.o(i.app_uart_init)
    i.app_uart_put                           0x00023270   Section        0  app_uart_fifo.o(i.app_uart_put)
    i.app_util_critical_region_enter         0x000232b0   Section        0  app_util_platform.o(i.app_util_critical_region_enter)
    i.app_util_critical_region_exit          0x000232bc   Section        0  app_util_platform.o(i.app_util_critical_region_exit)
    i.apply_config                           0x00023304   Section        0  nrf_drv_uart.o(i.apply_config)
    apply_config                             0x00023305   Thumb Code   222  nrf_drv_uart.o(i.apply_config)
    i.backend_id_assign                      0x000233e8   Section        0  nrf_log_frontend.o(i.backend_id_assign)
    backend_id_assign                        0x000233e9   Thumb Code    52  nrf_log_frontend.o(i.backend_id_assign)
    i.ble_db_discovery_evt_register          0x00023420   Section        0  ble_db_discovery.o(i.ble_db_discovery_evt_register)
    i.ble_db_discovery_init                  0x00023454   Section        0  ble_db_discovery.o(i.ble_db_discovery_init)
    i.ble_db_discovery_on_ble_evt            0x0002348c   Section        0  ble_db_discovery.o(i.ble_db_discovery_on_ble_evt)
    i.ble_db_discovery_start                 0x00023520   Section        0  ble_db_discovery.o(i.ble_db_discovery_start)
    i.ble_evt_handler                        0x00023568   Section        0  main.o(i.ble_evt_handler)
    ble_evt_handler                          0x00023569   Thumb Code   430  main.o(i.ble_evt_handler)
    i.ble_evt_handler                        0x000237a4   Section        0  bsp_btn_ble.o(i.ble_evt_handler)
    ble_evt_handler                          0x000237a5   Thumb Code   112  bsp_btn_ble.o(i.ble_evt_handler)
    i.ble_nus_c_evt_handler                  0x0002381c   Section        0  main.o(i.ble_nus_c_evt_handler)
    ble_nus_c_evt_handler                    0x0002381d   Thumb Code   152  main.o(i.ble_nus_c_evt_handler)
    i.ble_nus_c_handles_assign               0x0002390c   Section        0  ble_nus_c.o(i.ble_nus_c_handles_assign)
    i.ble_nus_c_init                         0x00023930   Section        0  ble_nus_c.o(i.ble_nus_c_init)
    i.ble_nus_c_on_ble_evt                   0x00023994   Section        0  ble_nus_c.o(i.ble_nus_c_on_ble_evt)
    i.ble_nus_c_on_db_disc_evt               0x000239fa   Section        0  ble_nus_c.o(i.ble_nus_c_on_db_disc_evt)
    i.ble_nus_c_string_send                  0x00023a90   Section        0  ble_nus_c.o(i.ble_nus_c_string_send)
    i.ble_nus_c_tx_notif_enable              0x00023b2c   Section        0  ble_nus_c.o(i.ble_nus_c_tx_notif_enable)
    i.ble_nus_chars_received_uart_print      0x00023b58   Section        0  main.o(i.ble_nus_chars_received_uart_print)
    ble_nus_chars_received_uart_print        0x00023b59   Thumb Code   162  main.o(i.ble_nus_chars_received_uart_print)
    i.ble_stack_init                         0x00023c58   Section        0  main.o(i.ble_stack_init)
    ble_stack_init                           0x00023c59   Thumb Code    86  main.o(i.ble_stack_init)
    i.bsp_board_button_idx_to_pin            0x00023cb0   Section        0  boards.o(i.bsp_board_button_idx_to_pin)
    i.bsp_board_button_state_get             0x00023cbc   Section        0  boards.o(i.bsp_board_button_state_get)
    i.bsp_board_led_invert                   0x00023cf0   Section        0  boards.o(i.bsp_board_led_invert)
    i.bsp_board_led_off                      0x00023d28   Section        0  boards.o(i.bsp_board_led_off)
    i.bsp_board_led_on                       0x00023d3c   Section        0  boards.o(i.bsp_board_led_on)
    i.bsp_board_led_state_get                0x00023d50   Section        0  boards.o(i.bsp_board_led_state_get)
    i.bsp_board_leds_init                    0x00023d84   Section        0  boards.o(i.bsp_board_leds_init)
    i.bsp_board_leds_off                     0x00023db4   Section        0  boards.o(i.bsp_board_leds_off)
    i.bsp_board_leds_on                      0x00023dc8   Section        0  boards.o(i.bsp_board_leds_on)
    i.bsp_board_pin_to_button_idx            0x00023ddc   Section        0  boards.o(i.bsp_board_pin_to_button_idx)
    i.bsp_btn_ble_init                       0x00023e00   Section        0  bsp_btn_ble.o(i.bsp_btn_ble_init)
    i.bsp_btn_ble_sleep_mode_prepare         0x00023e2c   Section        0  bsp_btn_ble.o(i.bsp_btn_ble_sleep_mode_prepare)
    i.bsp_button_event_handler               0x00023e60   Section        0  bsp.o(i.bsp_button_event_handler)
    bsp_button_event_handler                 0x00023e61   Thumb Code   176  bsp.o(i.bsp_button_event_handler)
    i.bsp_button_is_pressed                  0x00023f24   Section        0  bsp.o(i.bsp_button_is_pressed)
    i.bsp_event_handler                      0x00023f30   Section        0  main.o(i.bsp_event_handler)
    i.bsp_event_to_button_action_assign      0x00023f70   Section        0  bsp.o(i.bsp_event_to_button_action_assign)
    i.bsp_indication_set                     0x00023fcc   Section        0  bsp.o(i.bsp_indication_set)
    i.bsp_init                               0x00023fec   Section        0  bsp.o(i.bsp_init)
    i.bsp_led_indication                     0x00024098   Section        0  bsp.o(i.bsp_led_indication)
    bsp_led_indication                       0x00024099   Thumb Code   872  bsp.o(i.bsp_led_indication)
    i.bsp_wakeup_button_enable               0x00024414   Section        0  bsp.o(i.bsp_wakeup_button_enable)
    i.buf_prealloc                           0x0002442c   Section        0  nrf_log_frontend.o(i.buf_prealloc)
    buf_prealloc                             0x0002442d   Thumb Code   140  nrf_log_frontend.o(i.buf_prealloc)
    i.buffer_add                             0x000244bc   Section        0  nrf_fprintf_format.o(i.buffer_add)
    buffer_add                               0x000244bd   Thumb Code    32  nrf_fprintf_format.o(i.buffer_add)
    i.buffer_is_empty                        0x000244dc   Section        0  nrf_log_frontend.o(i.buffer_is_empty)
    i.button_timer_handler                   0x000244f4   Section        0  bsp.o(i.button_timer_handler)
    button_timer_handler                     0x000244f5   Thumb Code    14  bsp.o(i.button_timer_handler)
    i.buttons_leds_init                      0x00024504   Section        0  main.o(i.buttons_leds_init)
    buttons_leds_init                        0x00024505   Thumb Code    60  main.o(i.buttons_leds_init)
    i.cccd_configure                         0x00024544   Section        0  ble_nus_c.o(i.cccd_configure)
    cccd_configure                           0x00024545   Thumb Code    44  ble_nus_c.o(i.cccd_configure)
    i.channel_free                           0x00024574   Section        0  nrf_drv_gpiote.o(i.channel_free)
    channel_free                             0x00024575   Thumb Code    26  nrf_drv_gpiote.o(i.channel_free)
    i.channel_handler_get                    0x00024594   Section        0  nrf_drv_gpiote.o(i.channel_handler_get)
    channel_handler_get                      0x00024595   Thumb Code    10  nrf_drv_gpiote.o(i.channel_handler_get)
    i.channel_port_alloc                     0x000245a4   Section        0  nrf_drv_gpiote.o(i.channel_port_alloc)
    channel_port_alloc                       0x000245a5   Thumb Code   122  nrf_drv_gpiote.o(i.channel_port_alloc)
    i.channel_port_get                       0x00024624   Section        0  nrf_drv_gpiote.o(i.channel_port_get)
    channel_port_get                         0x00024625   Thumb Code     8  nrf_drv_gpiote.o(i.channel_port_get)
    i.characteristics_discover               0x00024630   Section        0  ble_db_discovery.o(i.characteristics_discover)
    characteristics_discover                 0x00024631   Thumb Code    96  ble_db_discovery.o(i.characteristics_discover)
    i.clock_clk_started_notify               0x00024690   Section        0  nrf_drv_clock.o(i.clock_clk_started_notify)
    clock_clk_started_notify                 0x00024691   Thumb Code    42  nrf_drv_clock.o(i.clock_clk_started_notify)
    i.compare_reg_update                     0x000246c0   Section        0  app_timer.o(i.compare_reg_update)
    compare_reg_update                       0x000246c1   Thumb Code   132  app_timer.o(i.compare_reg_update)
    i.connection_buttons_configure           0x00024750   Section        0  bsp_btn_ble.o(i.connection_buttons_configure)
    connection_buttons_configure             0x00024751   Thumb Code    84  bsp_btn_ble.o(i.connection_buttons_configure)
    i.data_length_update                     0x000247a4   Section        0  nrf_ble_gatt.o(i.data_length_update)
    data_length_update                       0x000247a5   Thumb Code    70  nrf_ble_gatt.o(i.data_length_update)
    i.db_disc_handler                        0x000247f4   Section        0  main.o(i.db_disc_handler)
    db_disc_handler                          0x000247f5   Thumb Code    14  main.o(i.db_disc_handler)
    i.db_discovery_init                      0x00024808   Section        0  main.o(i.db_discovery_init)
    db_discovery_init                        0x00024809   Thumb Code    30  main.o(i.db_discovery_init)
    i.descriptors_discover                   0x0002482c   Section        0  ble_db_discovery.o(i.descriptors_discover)
    descriptors_discover                     0x0002482d   Thumb Code   182  ble_db_discovery.o(i.descriptors_discover)
    i.detection_delay_timeout_handler        0x000248e4   Section        0  app_button.o(i.detection_delay_timeout_handler)
    detection_delay_timeout_handler          0x000248e5   Thumb Code   124  app_button.o(i.detection_delay_timeout_handler)
    i.discovery_complete_evt_trigger         0x00024970   Section        0  ble_db_discovery.o(i.discovery_complete_evt_trigger)
    discovery_complete_evt_trigger           0x00024971   Thumb Code   150  ble_db_discovery.o(i.discovery_complete_evt_trigger)
    i.discovery_error_evt_trigger            0x00024a14   Section        0  ble_db_discovery.o(i.discovery_error_evt_trigger)
    discovery_error_evt_trigger              0x00024a15   Thumb Code    66  ble_db_discovery.o(i.discovery_error_evt_trigger)
    i.discovery_start                        0x00024a5c   Section        0  ble_db_discovery.o(i.discovery_start)
    discovery_start                          0x00024a5d   Thumb Code   124  ble_db_discovery.o(i.discovery_start)
    i.elapsed_ticks_acquire                  0x00024ae0   Section        0  app_timer.o(i.elapsed_ticks_acquire)
    elapsed_ticks_acquire                    0x00024ae1   Thumb Code    82  app_timer.o(i.elapsed_ticks_acquire)
    i.errata_103                             0x00024b44   Section        0  system_nrf52840.o(i.errata_103)
    errata_103                               0x00024b45   Thumb Code    24  system_nrf52840.o(i.errata_103)
    i.errata_115                             0x00024b60   Section        0  system_nrf52840.o(i.errata_115)
    errata_115                               0x00024b61   Thumb Code    24  system_nrf52840.o(i.errata_115)
    i.errata_120                             0x00024b7c   Section        0  system_nrf52840.o(i.errata_120)
    errata_120                               0x00024b7d   Thumb Code    24  system_nrf52840.o(i.errata_120)
    i.errata_136                             0x00024b98   Section        0  system_nrf52840.o(i.errata_136)
    errata_136                               0x00024b99   Thumb Code    24  system_nrf52840.o(i.errata_136)
    i.errata_36                              0x00024bb4   Section        0  system_nrf52840.o(i.errata_36)
    errata_36                                0x00024bb5   Thumb Code    24  system_nrf52840.o(i.errata_36)
    i.errata_66                              0x00024bd0   Section        0  system_nrf52840.o(i.errata_66)
    errata_66                                0x00024bd1   Thumb Code    24  system_nrf52840.o(i.errata_66)
    i.errata_98                              0x00024bec   Section        0  system_nrf52840.o(i.errata_98)
    errata_98                                0x00024bed   Thumb Code    24  system_nrf52840.o(i.errata_98)
    i.expired_timers_handler                 0x00024c08   Section        0  app_timer.o(i.expired_timers_handler)
    expired_timers_handler                   0x00024c09   Thumb Code    84  app_timer.o(i.expired_timers_handler)
    i.fifo_get                               0x00024c60   Section        0  app_fifo.o(i.fifo_get)
    fifo_get                                 0x00024c61   Thumb Code    24  app_fifo.o(i.fifo_get)
    i.fifo_length                            0x00024c78   Section        0  app_fifo.o(i.fifo_length)
    fifo_length                              0x00024c79   Thumb Code    10  app_fifo.o(i.fifo_length)
    i.fifo_length                            0x00024c82   Section        0  app_uart_fifo.o(i.fifo_length)
    fifo_length                              0x00024c83   Thumb Code    10  app_uart_fifo.o(i.fifo_length)
    i.fifo_peek                              0x00024c8c   Section        0  app_fifo.o(i.fifo_peek)
    fifo_peek                                0x00024c8d   Thumb Code    18  app_fifo.o(i.fifo_peek)
    i.fifo_put                               0x00024c9e   Section        0  app_fifo.o(i.fifo_put)
    fifo_put                                 0x00024c9f   Thumb Code    18  app_fifo.o(i.fifo_put)
    i.fputc                                  0x00024cb0   Section        0  retarget.o(i.fputc)
    i.gatt_evt_handler                       0x00024cc0   Section        0  main.o(i.gatt_evt_handler)
    i.gatt_init                              0x00024d4c   Section        0  main.o(i.gatt_init)
    i.gpiote_event_handler                   0x00024d90   Section        0  app_button.o(i.gpiote_event_handler)
    gpiote_event_handler                     0x00024d91   Thumb Code   110  app_button.o(i.gpiote_event_handler)
    i.int_print                              0x00024e10   Section        0  nrf_fprintf_format.o(i.int_print)
    int_print                                0x00024e11   Thumb Code   190  nrf_fprintf_format.o(i.int_print)
    i.interrupts_enable                      0x00024ed0   Section        0  nrf_drv_uart.o(i.interrupts_enable)
    interrupts_enable                        0x00024ed1   Thumb Code   126  nrf_drv_uart.o(i.interrupts_enable)
    i.is_char_discovery_reqd                 0x00024f5c   Section        0  ble_db_discovery.o(i.is_char_discovery_reqd)
    is_char_discovery_reqd                   0x00024f5d   Thumb Code    36  ble_db_discovery.o(i.is_char_discovery_reqd)
    i.is_desc_discovery_reqd                 0x00024f80   Section        0  ble_db_discovery.o(i.is_desc_discovery_reqd)
    is_desc_discovery_reqd                   0x00024f81   Thumb Code    94  ble_db_discovery.o(i.is_desc_discovery_reqd)
    i.is_uuid_present                        0x00024fde   Section        0  main.o(i.is_uuid_present)
    is_uuid_present                          0x00024fdf   Thumb Code   250  main.o(i.is_uuid_present)
    i.item_dequeue                           0x000250d8   Section        0  nrf_drv_clock.o(i.item_dequeue)
    item_dequeue                             0x000250d9   Thumb Code    12  nrf_drv_clock.o(i.item_dequeue)
    i.leds_off                               0x000250e4   Section        0  bsp.o(i.leds_off)
    leds_off                                 0x000250e5   Thumb Code    36  bsp.o(i.leds_off)
    i.leds_timer_handler                     0x0002510c   Section        0  bsp.o(i.leds_timer_handler)
    leds_timer_handler                       0x0002510d   Thumb Code    24  bsp.o(i.leds_timer_handler)
    i.lfclk_stop                             0x0002512c   Section        0  nrf_drv_clock.o(i.lfclk_stop)
    lfclk_stop                               0x0002512d   Thumb Code    24  nrf_drv_clock.o(i.lfclk_stop)
    i.link_init                              0x00025148   Section        0  nrf_ble_gatt.o(i.link_init)
    link_init                                0x00025149   Thumb Code    24  nrf_ble_gatt.o(i.link_init)
    i.list_insertions_handler                0x00025160   Section        0  app_timer.o(i.list_insertions_handler)
    list_insertions_handler                  0x00025161   Thumb Code   294  app_timer.o(i.list_insertions_handler)
    i.log_init                               0x0002529c   Section        0  main.o(i.log_init)
    log_init                                 0x0002529d   Thumb Code    34  main.o(i.log_init)
    i.log_skip                               0x000252c0   Section        0  nrf_log_frontend.o(i.log_skip)
    log_skip                                 0x000252c1   Thumb Code   196  nrf_log_frontend.o(i.log_skip)
    i.main                                   0x0002538c   Section        0  main.o(i.main)
    i.memobj_op                              0x00025428   Section        0  nrf_memobj.o(i.memobj_op)
    memobj_op                                0x00025429   Thumb Code   174  nrf_memobj.o(i.memobj_op)
    i.module_idx_get                         0x000254d8   Section        0  nrf_log_frontend.o(i.module_idx_get)
    module_idx_get                           0x000254d9   Thumb Code    56  nrf_log_frontend.o(i.module_idx_get)
    i.nrf_atomic_flag_set                    0x00025514   Section        0  nrf_log_frontend.o(i.nrf_atomic_flag_set)
    nrf_atomic_flag_set                      0x00025515   Thumb Code    22  nrf_log_frontend.o(i.nrf_atomic_flag_set)
    i.nrf_balloc_alloc                       0x0002552a   Section        0  nrf_balloc.o(i.nrf_balloc_alloc)
    i.nrf_balloc_block2idx                   0x0002557c   Section        0  nrf_balloc.o(i.nrf_balloc_block2idx)
    nrf_balloc_block2idx                     0x0002557d   Thumb Code    16  nrf_balloc.o(i.nrf_balloc_block2idx)
    i.nrf_balloc_free                        0x0002558c   Section        0  nrf_balloc.o(i.nrf_balloc_free)
    i.nrf_balloc_idx2block                   0x000255bc   Section        0  nrf_balloc.o(i.nrf_balloc_idx2block)
    nrf_balloc_idx2block                     0x000255bd   Thumb Code    12  nrf_balloc.o(i.nrf_balloc_idx2block)
    i.nrf_balloc_init                        0x000255c8   Section        0  nrf_balloc.o(i.nrf_balloc_init)
    i.nrf_bitmask_bit_is_set                 0x00025604   Section        0  nrf_drv_gpiote.o(i.nrf_bitmask_bit_is_set)
    nrf_bitmask_bit_is_set                   0x00025605   Thumb Code    22  nrf_drv_gpiote.o(i.nrf_bitmask_bit_is_set)
    i.nrf_ble_gatt_att_mtu_central_set       0x0002561a   Section        0  nrf_ble_gatt.o(i.nrf_ble_gatt_att_mtu_central_set)
    i.nrf_ble_gatt_init                      0x00025638   Section        0  nrf_ble_gatt.o(i.nrf_ble_gatt_init)
    i.nrf_ble_gatt_on_ble_evt                0x0002566c   Section        0  nrf_ble_gatt.o(i.nrf_ble_gatt_on_ble_evt)
    i.nrf_clock_event_check                  0x00025734   Section        0  nrf_drv_clock.o(i.nrf_clock_event_check)
    nrf_clock_event_check                    0x00025735   Thumb Code    18  nrf_drv_clock.o(i.nrf_clock_event_check)
    i.nrf_clock_event_clear                  0x00025746   Section        0  nrf_drv_clock.o(i.nrf_clock_event_clear)
    nrf_clock_event_clear                    0x00025747   Thumb Code    18  nrf_drv_clock.o(i.nrf_clock_event_clear)
    i.nrf_clock_int_disable                  0x00025758   Section        0  nrf_drv_clock.o(i.nrf_clock_int_disable)
    nrf_clock_int_disable                    0x00025759   Thumb Code     6  nrf_drv_clock.o(i.nrf_clock_int_disable)
    i.nrf_clock_lf_is_running                0x00025764   Section        0  nrf_drv_clock.o(i.nrf_clock_lf_is_running)
    nrf_clock_lf_is_running                  0x00025765   Thumb Code    10  nrf_drv_clock.o(i.nrf_clock_lf_is_running)
    i.nrf_clock_task_trigger                 0x00025774   Section        0  nrf_drv_clock.o(i.nrf_clock_task_trigger)
    nrf_clock_task_trigger                   0x00025775   Thumb Code     8  nrf_drv_clock.o(i.nrf_clock_task_trigger)
    i.nrf_delay_us                           0x0002577c   Section        0  app_timer.o(i.nrf_delay_us)
    nrf_delay_us                             0x0002577d   Thumb Code   146  app_timer.o(i.nrf_delay_us)
    i.nrf_drv_clock_init                     0x00025818   Section        0  nrf_drv_clock.o(i.nrf_drv_clock_init)
    i.nrf_drv_clock_lfclk_release            0x00025880   Section        0  nrf_drv_clock.o(i.nrf_drv_clock_lfclk_release)
    i.nrf_drv_common_irq_enable              0x000258b0   Section        0  nrf_drv_common.o(i.nrf_drv_common_irq_enable)
    i.nrf_drv_get_IRQn                       0x00025910   Section        0  nrf_drv_uart.o(i.nrf_drv_get_IRQn)
    nrf_drv_get_IRQn                         0x00025911   Thumb Code    10  nrf_drv_uart.o(i.nrf_drv_get_IRQn)
    i.nrf_drv_gpiote_in_event_enable         0x0002591c   Section        0  nrf_drv_gpiote.o(i.nrf_drv_gpiote_in_event_enable)
    i.nrf_drv_gpiote_in_init                 0x000259c8   Section        0  nrf_drv_gpiote.o(i.nrf_drv_gpiote_in_init)
    i.nrf_drv_gpiote_in_is_set               0x00025aa8   Section        0  nrf_drv_gpiote.o(i.nrf_drv_gpiote_in_is_set)
    i.nrf_drv_gpiote_init                    0x00025abc   Section        0  nrf_drv_gpiote.o(i.nrf_drv_gpiote_init)
    i.nrf_drv_gpiote_is_init                 0x00025b1c   Section        0  nrf_drv_gpiote.o(i.nrf_drv_gpiote_is_init)
    i.nrf_drv_is_in_RAM                      0x00025b30   Section        0  nrf_drv_uart.o(i.nrf_drv_is_in_RAM)
    nrf_drv_is_in_RAM                        0x00025b31   Thumb Code    20  nrf_drv_uart.o(i.nrf_drv_is_in_RAM)
    i.nrf_drv_uart_init                      0x00025b44   Section        0  nrf_drv_uart.o(i.nrf_drv_uart_init)
    i.nrf_drv_uart_rx                        0x00025bc8   Section        0  nrf_drv_uart.o(i.nrf_drv_uart_rx)
    i.nrf_drv_uart_rx_enable                 0x00025c9c   Section        0  nrf_drv_uart.o(i.nrf_drv_uart_rx_enable)
    i.nrf_drv_uart_rx_for_uart               0x00025cd0   Section        0  nrf_drv_uart.o(i.nrf_drv_uart_rx_for_uart)
    nrf_drv_uart_rx_for_uart                 0x00025cd1   Thumb Code   198  nrf_drv_uart.o(i.nrf_drv_uart_rx_for_uart)
    i.nrf_drv_uart_rx_for_uarte              0x00025d9c   Section        0  nrf_drv_uart.o(i.nrf_drv_uart_rx_for_uarte)
    nrf_drv_uart_rx_for_uarte                0x00025d9d   Thumb Code   196  nrf_drv_uart.o(i.nrf_drv_uart_rx_for_uarte)
    i.nrf_drv_uart_tx                        0x00025e64   Section        0  nrf_drv_uart.o(i.nrf_drv_uart_tx)
    i.nrf_drv_uart_tx_for_uart               0x00025ec8   Section        0  nrf_drv_uart.o(i.nrf_drv_uart_tx_for_uart)
    nrf_drv_uart_tx_for_uart                 0x00025ec9   Thumb Code   136  nrf_drv_uart.o(i.nrf_drv_uart_tx_for_uart)
    i.nrf_drv_uart_tx_for_uarte              0x00025f54   Section        0  nrf_drv_uart.o(i.nrf_drv_uart_tx_for_uarte)
    nrf_drv_uart_tx_for_uarte                0x00025f55   Thumb Code   118  nrf_drv_uart.o(i.nrf_drv_uart_tx_for_uarte)
    i.nrf_drv_uart_tx_in_progress            0x00025fd0   Section        0  nrf_drv_uart.o(i.nrf_drv_uart_tx_in_progress)
    i.nrf_fprintf                            0x00025fec   Section        0  nrf_fprintf.o(i.nrf_fprintf)
    i.nrf_fprintf_buffer_flush               0x00026016   Section        0  nrf_fprintf.o(i.nrf_fprintf_buffer_flush)
    i.nrf_fprintf_fmt                        0x00026032   Section        0  nrf_fprintf_format.o(i.nrf_fprintf_fmt)
    i.nrf_gpio_cfg                           0x00026222   Section        0  boards.o(i.nrf_gpio_cfg)
    nrf_gpio_cfg                             0x00026223   Thumb Code    52  boards.o(i.nrf_gpio_cfg)
    i.nrf_gpio_cfg                           0x00026256   Section        0  nrf_drv_gpiote.o(i.nrf_gpio_cfg)
    nrf_gpio_cfg                             0x00026257   Thumb Code    52  nrf_drv_gpiote.o(i.nrf_gpio_cfg)
    i.nrf_gpio_cfg                           0x0002628a   Section        0  nrf_drv_uart.o(i.nrf_gpio_cfg)
    nrf_gpio_cfg                             0x0002628b   Thumb Code    52  nrf_drv_uart.o(i.nrf_gpio_cfg)
    i.nrf_gpio_cfg_input                     0x000262be   Section        0  nrf_drv_uart.o(i.nrf_gpio_cfg_input)
    nrf_gpio_cfg_input                       0x000262bf   Thumb Code    26  nrf_drv_uart.o(i.nrf_gpio_cfg_input)
    i.nrf_gpio_cfg_output                    0x000262d8   Section        0  nrf_drv_uart.o(i.nrf_gpio_cfg_output)
    nrf_gpio_cfg_output                      0x000262d9   Thumb Code    24  nrf_drv_uart.o(i.nrf_gpio_cfg_output)
    i.nrf_gpio_cfg_sense_set                 0x000262f0   Section        0  bsp.o(i.nrf_gpio_cfg_sense_set)
    nrf_gpio_cfg_sense_set                   0x000262f1   Thumb Code    62  bsp.o(i.nrf_gpio_cfg_sense_set)
    i.nrf_gpio_cfg_sense_set                 0x00026334   Section        0  nrf_drv_gpiote.o(i.nrf_gpio_cfg_sense_set)
    nrf_gpio_cfg_sense_set                   0x00026335   Thumb Code    58  nrf_drv_gpiote.o(i.nrf_gpio_cfg_sense_set)
    i.nrf_gpio_pin_port_decode               0x00026370   Section        0  boards.o(i.nrf_gpio_pin_port_decode)
    nrf_gpio_pin_port_decode                 0x00026371   Thumb Code    26  boards.o(i.nrf_gpio_pin_port_decode)
    i.nrf_gpio_pin_port_decode               0x00026390   Section        0  nrf_drv_gpiote.o(i.nrf_gpio_pin_port_decode)
    nrf_gpio_pin_port_decode                 0x00026391   Thumb Code    26  nrf_drv_gpiote.o(i.nrf_gpio_pin_port_decode)
    i.nrf_gpio_pin_port_decode               0x000263b0   Section        0  nrf_drv_uart.o(i.nrf_gpio_pin_port_decode)
    nrf_gpio_pin_port_decode                 0x000263b1   Thumb Code    26  nrf_drv_uart.o(i.nrf_gpio_pin_port_decode)
    i.nrf_gpio_pin_read                      0x000263d0   Section        0  nrf_drv_gpiote.o(i.nrf_gpio_pin_read)
    nrf_gpio_pin_read                        0x000263d1   Thumb Code    26  nrf_drv_gpiote.o(i.nrf_gpio_pin_read)
    i.nrf_gpio_pin_set                       0x000263ea   Section        0  nrf_drv_uart.o(i.nrf_gpio_pin_set)
    nrf_gpio_pin_set                         0x000263eb   Thumb Code    26  nrf_drv_uart.o(i.nrf_gpio_pin_set)
    i.nrf_gpio_pin_write                     0x00026404   Section        0  boards.o(i.nrf_gpio_pin_write)
    nrf_gpio_pin_write                       0x00026405   Thumb Code    66  boards.o(i.nrf_gpio_pin_write)
    i.nrf_gpio_ports_read                    0x00026448   Section        0  nrf_drv_gpiote.o(i.nrf_gpio_ports_read)
    nrf_gpio_ports_read                      0x00026449   Thumb Code    38  nrf_drv_gpiote.o(i.nrf_gpio_ports_read)
    i.nrf_gpiote_event_addr_get              0x00026474   Section        0  nrf_drv_gpiote.o(i.nrf_gpiote_event_addr_get)
    nrf_gpiote_event_addr_get                0x00026475   Thumb Code     8  nrf_drv_gpiote.o(i.nrf_gpiote_event_addr_get)
    i.nrf_gpiote_event_clear                 0x00026480   Section        0  nrf_drv_gpiote.o(i.nrf_gpiote_event_clear)
    nrf_gpiote_event_clear                   0x00026481   Thumb Code    28  nrf_drv_gpiote.o(i.nrf_gpiote_event_clear)
    i.nrf_gpiote_event_is_set                0x0002649c   Section        0  nrf_drv_gpiote.o(i.nrf_gpiote_event_is_set)
    nrf_gpiote_event_is_set                  0x0002649d   Thumb Code    22  nrf_drv_gpiote.o(i.nrf_gpiote_event_is_set)
    i.nrf_gpiote_int_enable                  0x000264b4   Section        0  nrf_drv_gpiote.o(i.nrf_gpiote_int_enable)
    nrf_gpiote_int_enable                    0x000264b5   Thumb Code     6  nrf_drv_gpiote.o(i.nrf_gpiote_int_enable)
    i.nrf_log_backend_add                    0x000264c0   Section        0  nrf_log_frontend.o(i.nrf_log_backend_add)
    i.nrf_log_backend_rtt_flush              0x00026508   Section        0  nrf_log_backend_rtt.o(i.nrf_log_backend_rtt_flush)
    nrf_log_backend_rtt_flush                0x00026509   Thumb Code     2  nrf_log_backend_rtt.o(i.nrf_log_backend_rtt_flush)
    i.nrf_log_backend_rtt_init               0x0002650a   Section        0  nrf_log_backend_rtt.o(i.nrf_log_backend_rtt_init)
    i.nrf_log_backend_rtt_panic_set          0x00026512   Section        0  nrf_log_backend_rtt.o(i.nrf_log_backend_rtt_panic_set)
    nrf_log_backend_rtt_panic_set            0x00026513   Thumb Code     2  nrf_log_backend_rtt.o(i.nrf_log_backend_rtt_panic_set)
    i.nrf_log_backend_rtt_put                0x00026514   Section        0  nrf_log_backend_rtt.o(i.nrf_log_backend_rtt_put)
    nrf_log_backend_rtt_put                  0x00026515   Thumb Code    24  nrf_log_backend_rtt.o(i.nrf_log_backend_rtt_put)
    i.nrf_log_backend_serial_put             0x00026534   Section        0  nrf_log_backend_serial.o(i.nrf_log_backend_serial_put)
    i.nrf_log_color_id_get                   0x00026634   Section        0  nrf_log_frontend.o(i.nrf_log_color_id_get)
    i.nrf_log_default_backends_init          0x0002666c   Section        0  nrf_log_default_backends.o(i.nrf_log_default_backends_init)
    i.nrf_log_frontend_dequeue               0x00026690   Section        0  nrf_log_frontend.o(i.nrf_log_frontend_dequeue)
    i.nrf_log_frontend_std_0                 0x00026950   Section        0  nrf_log_frontend.o(i.nrf_log_frontend_std_0)
    i.nrf_log_frontend_std_1                 0x00026964   Section        0  nrf_log_frontend.o(i.nrf_log_frontend_std_1)
    i.nrf_log_frontend_std_2                 0x0002697c   Section        0  nrf_log_frontend.o(i.nrf_log_frontend_std_2)
    i.nrf_log_frontend_std_6                 0x0002699c   Section        0  nrf_log_frontend.o(i.nrf_log_frontend_std_6)
    i.nrf_log_hexdump_entry_process          0x000269d8   Section        0  nrf_log_str_formatter.o(i.nrf_log_hexdump_entry_process)
    i.nrf_log_init                           0x00026a90   Section        0  nrf_log_frontend.o(i.nrf_log_init)
    i.nrf_log_module_cnt_get                 0x00026af8   Section        0  nrf_log_frontend.o(i.nrf_log_module_cnt_get)
    i.nrf_log_module_name_get                0x00026b0c   Section        0  nrf_log_frontend.o(i.nrf_log_module_name_get)
    i.nrf_log_panic                          0x00026b30   Section        0  nrf_log_frontend.o(i.nrf_log_panic)
    i.nrf_log_std_entry_process              0x00026b64   Section        0  nrf_log_str_formatter.o(i.nrf_log_std_entry_process)
    i.nrf_memobj_alloc                       0x00026c2c   Section        0  nrf_memobj.o(i.nrf_memobj_alloc)
    i.nrf_memobj_free                        0x00026ca6   Section        0  nrf_memobj.o(i.nrf_memobj_free)
    i.nrf_memobj_get                         0x00026ce6   Section        0  nrf_memobj.o(i.nrf_memobj_get)
    i.nrf_memobj_pool_init                   0x00026d04   Section        0  nrf_memobj.o(i.nrf_memobj_pool_init)
    i.nrf_memobj_put                         0x00026d10   Section        0  nrf_memobj.o(i.nrf_memobj_put)
    i.nrf_memobj_read                        0x00026d40   Section        0  nrf_memobj.o(i.nrf_memobj_read)
    i.nrf_memobj_write                       0x00026d5c   Section        0  nrf_memobj.o(i.nrf_memobj_write)
    i.nrf_mtx_unlock                         0x00026d78   Section        0  nrf_pwr_mgmt.o(i.nrf_mtx_unlock)
    nrf_mtx_unlock                           0x00026d79   Thumb Code    22  nrf_pwr_mgmt.o(i.nrf_mtx_unlock)
    i.nrf_pwr_mgmt_init                      0x00026d90   Section        0  nrf_pwr_mgmt.o(i.nrf_pwr_mgmt_init)
    i.nrf_pwr_mgmt_run                       0x00026dd0   Section        0  nrf_pwr_mgmt.o(i.nrf_pwr_mgmt_run)
    i.nrf_pwr_mgmt_shutdown                  0x00026e38   Section        0  nrf_pwr_mgmt.o(i.nrf_pwr_mgmt_shutdown)
    i.nrf_sdh_ble_app_ram_start_get          0x00026ea8   Section        0  nrf_sdh_ble.o(i.nrf_sdh_ble_app_ram_start_get)
    i.nrf_sdh_ble_default_cfg_set            0x00026ec0   Section        0  nrf_sdh_ble.o(i.nrf_sdh_ble_default_cfg_set)
    i.nrf_sdh_ble_enable                     0x00027040   Section        0  nrf_sdh_ble.o(i.nrf_sdh_ble_enable)
    i.nrf_sdh_ble_evts_poll                  0x0002711c   Section        0  nrf_sdh_ble.o(i.nrf_sdh_ble_evts_poll)
    nrf_sdh_ble_evts_poll                    0x0002711d   Thumb Code    94  nrf_sdh_ble.o(i.nrf_sdh_ble_evts_poll)
    i.nrf_sdh_enable_request                 0x00027180   Section        0  nrf_sdh.o(i.nrf_sdh_enable_request)
    i.nrf_sdh_evts_poll                      0x000271ec   Section        0  nrf_sdh.o(i.nrf_sdh_evts_poll)
    i.nrf_sdh_is_enabled                     0x0002721c   Section        0  nrf_sdh.o(i.nrf_sdh_is_enabled)
    i.nrf_sdh_soc_evts_poll                  0x00027228   Section        0  nrf_sdh_soc.o(i.nrf_sdh_soc_evts_poll)
    nrf_sdh_soc_evts_poll                    0x00027229   Thumb Code    80  nrf_sdh_soc.o(i.nrf_sdh_soc_evts_poll)
    i.nrf_section_iter_get                   0x0002727c   Section        0  nrf_sdh.o(i.nrf_section_iter_get)
    nrf_section_iter_get                     0x0002727d   Thumb Code     6  nrf_sdh.o(i.nrf_section_iter_get)
    i.nrf_section_iter_init                  0x00027282   Section        0  nrf_section_iter.o(i.nrf_section_iter_init)
    i.nrf_section_iter_item_set              0x00027296   Section        0  nrf_section_iter.o(i.nrf_section_iter_item_set)
    nrf_section_iter_item_set                0x00027297   Thumb Code    46  nrf_section_iter.o(i.nrf_section_iter_item_set)
    i.nrf_section_iter_next                  0x000272c4   Section        0  nrf_section_iter.o(i.nrf_section_iter_next)
    i.nrf_strerror_find                      0x000272f4   Section        0  nrf_strerror.o(i.nrf_strerror_find)
    i.nrf_strerror_get                       0x00027334   Section        0  nrf_strerror.o(i.nrf_strerror_get)
    i.nrf_uart_errorsrc_get_and_clear        0x00027350   Section        0  nrf_drv_uart.o(i.nrf_uart_errorsrc_get_and_clear)
    nrf_uart_errorsrc_get_and_clear          0x00027351   Thumb Code    12  nrf_drv_uart.o(i.nrf_uart_errorsrc_get_and_clear)
    i.nrf_uart_event_check                   0x0002735c   Section        0  nrf_drv_uart.o(i.nrf_uart_event_check)
    nrf_uart_event_check                     0x0002735d   Thumb Code    14  nrf_drv_uart.o(i.nrf_uart_event_check)
    i.nrf_uart_event_clear                   0x0002736a   Section        0  nrf_drv_uart.o(i.nrf_uart_event_clear)
    nrf_uart_event_clear                     0x0002736b   Thumb Code    14  nrf_drv_uart.o(i.nrf_uart_event_clear)
    i.nrf_uart_hwfc_pins_set                 0x00027378   Section        0  nrf_drv_uart.o(i.nrf_uart_hwfc_pins_set)
    nrf_uart_hwfc_pins_set                   0x00027379   Thumb Code    12  nrf_drv_uart.o(i.nrf_uart_hwfc_pins_set)
    i.nrf_uart_int_disable                   0x00027384   Section        0  nrf_drv_uart.o(i.nrf_uart_int_disable)
    nrf_uart_int_disable                     0x00027385   Thumb Code     6  nrf_drv_uart.o(i.nrf_uart_int_disable)
    i.nrf_uart_int_enable                    0x0002738a   Section        0  nrf_drv_uart.o(i.nrf_uart_int_enable)
    nrf_uart_int_enable                      0x0002738b   Thumb Code     6  nrf_drv_uart.o(i.nrf_uart_int_enable)
    i.nrf_uart_int_enable_check              0x00027390   Section        0  nrf_drv_uart.o(i.nrf_uart_int_enable_check)
    nrf_uart_int_enable_check                0x00027391   Thumb Code    18  nrf_drv_uart.o(i.nrf_uart_int_enable_check)
    i.nrf_uart_task_trigger                  0x000273a2   Section        0  nrf_drv_uart.o(i.nrf_uart_task_trigger)
    nrf_uart_task_trigger                    0x000273a3   Thumb Code     6  nrf_drv_uart.o(i.nrf_uart_task_trigger)
    i.nrf_uart_txrx_pins_set                 0x000273a8   Section        0  nrf_drv_uart.o(i.nrf_uart_txrx_pins_set)
    nrf_uart_txrx_pins_set                   0x000273a9   Thumb Code    14  nrf_drv_uart.o(i.nrf_uart_txrx_pins_set)
    i.nrf_uarte_errorsrc_get_and_clear       0x000273b6   Section        0  nrf_drv_uart.o(i.nrf_uarte_errorsrc_get_and_clear)
    nrf_uarte_errorsrc_get_and_clear         0x000273b7   Thumb Code    12  nrf_drv_uart.o(i.nrf_uarte_errorsrc_get_and_clear)
    i.nrf_uarte_event_check                  0x000273c2   Section        0  nrf_drv_uart.o(i.nrf_uarte_event_check)
    nrf_uarte_event_check                    0x000273c3   Thumb Code    14  nrf_drv_uart.o(i.nrf_uarte_event_check)
    i.nrf_uarte_event_clear                  0x000273d0   Section        0  nrf_drv_uart.o(i.nrf_uarte_event_clear)
    nrf_uarte_event_clear                    0x000273d1   Thumb Code    14  nrf_drv_uart.o(i.nrf_uarte_event_clear)
    i.nrf_uarte_hwfc_pins_set                0x000273de   Section        0  nrf_drv_uart.o(i.nrf_uarte_hwfc_pins_set)
    nrf_uarte_hwfc_pins_set                  0x000273df   Thumb Code    12  nrf_drv_uart.o(i.nrf_uarte_hwfc_pins_set)
    i.nrf_uarte_int_disable                  0x000273ea   Section        0  nrf_drv_uart.o(i.nrf_uarte_int_disable)
    nrf_uarte_int_disable                    0x000273eb   Thumb Code     6  nrf_drv_uart.o(i.nrf_uarte_int_disable)
    i.nrf_uarte_int_enable                   0x000273f0   Section        0  nrf_drv_uart.o(i.nrf_uarte_int_enable)
    nrf_uarte_int_enable                     0x000273f1   Thumb Code     6  nrf_drv_uart.o(i.nrf_uarte_int_enable)
    i.nrf_uarte_rx_amount_get                0x000273f6   Section        0  nrf_drv_uart.o(i.nrf_uarte_rx_amount_get)
    nrf_uarte_rx_amount_get                  0x000273f7   Thumb Code    10  nrf_drv_uart.o(i.nrf_uarte_rx_amount_get)
    i.nrf_uarte_task_trigger                 0x00027400   Section        0  nrf_drv_uart.o(i.nrf_uarte_task_trigger)
    nrf_uarte_task_trigger                   0x00027401   Thumb Code     6  nrf_drv_uart.o(i.nrf_uarte_task_trigger)
    i.nrf_uarte_txrx_pins_set                0x00027406   Section        0  nrf_drv_uart.o(i.nrf_uarte_txrx_pins_set)
    nrf_uarte_txrx_pins_set                  0x00027407   Thumb Code    14  nrf_drv_uart.o(i.nrf_uarte_txrx_pins_set)
    i.nus_c_init                             0x00027414   Section        0  main.o(i.nus_c_init)
    nus_c_init                               0x00027415   Thumb Code    36  main.o(i.nus_c_init)
    i.on_characteristic_discovery_rsp        0x00027440   Section        0  ble_db_discovery.o(i.on_characteristic_discovery_rsp)
    on_characteristic_discovery_rsp          0x00027441   Thumb Code   380  ble_db_discovery.o(i.on_characteristic_discovery_rsp)
    i.on_connected_evt                       0x000275c0   Section        0  nrf_ble_gatt.o(i.on_connected_evt)
    on_connected_evt                         0x000275c1   Thumb Code   122  nrf_ble_gatt.o(i.on_connected_evt)
    i.on_data_length_update_evt              0x00027644   Section        0  nrf_ble_gatt.o(i.on_data_length_update_evt)
    on_data_length_update_evt                0x00027645   Thumb Code    78  nrf_ble_gatt.o(i.on_data_length_update_evt)
    i.on_data_length_update_request_evt      0x00027698   Section        0  nrf_ble_gatt.o(i.on_data_length_update_request_evt)
    on_data_length_update_request_evt        0x00027699   Thumb Code    88  nrf_ble_gatt.o(i.on_data_length_update_request_evt)
    i.on_descriptor_discovery_rsp            0x000276f8   Section        0  ble_db_discovery.o(i.on_descriptor_discovery_rsp)
    on_descriptor_discovery_rsp              0x000276f9   Thumb Code   298  ble_db_discovery.o(i.on_descriptor_discovery_rsp)
    i.on_disconnected                        0x00027828   Section        0  ble_db_discovery.o(i.on_disconnected)
    on_disconnected                          0x00027829   Thumb Code    30  ble_db_discovery.o(i.on_disconnected)
    i.on_disconnected_evt                    0x00027846   Section        0  nrf_ble_gatt.o(i.on_disconnected_evt)
    on_disconnected_evt                      0x00027847   Thumb Code    20  nrf_ble_gatt.o(i.on_disconnected_evt)
    i.on_exchange_mtu_request_evt            0x0002785c   Section        0  nrf_ble_gatt.o(i.on_exchange_mtu_request_evt)
    on_exchange_mtu_request_evt              0x0002785d   Thumb Code   126  nrf_ble_gatt.o(i.on_exchange_mtu_request_evt)
    i.on_exchange_mtu_rsp_evt                0x000278e8   Section        0  nrf_ble_gatt.o(i.on_exchange_mtu_rsp_evt)
    on_exchange_mtu_rsp_evt                  0x000278e9   Thumb Code    94  nrf_ble_gatt.o(i.on_exchange_mtu_rsp_evt)
    i.on_hvx                                 0x0002794c   Section        0  ble_nus_c.o(i.on_hvx)
    on_hvx                                   0x0002794d   Thumb Code    56  ble_nus_c.o(i.on_hvx)
    i.on_primary_srv_discovery_rsp           0x00027984   Section        0  ble_db_discovery.o(i.on_primary_srv_discovery_rsp)
    on_primary_srv_discovery_rsp             0x00027985   Thumb Code   122  ble_db_discovery.o(i.on_primary_srv_discovery_rsp)
    i.on_srv_disc_completion                 0x00027a04   Section        0  ble_db_discovery.o(i.on_srv_disc_completion)
    on_srv_disc_completion                   0x00027a05   Thumb Code   144  ble_db_discovery.o(i.on_srv_disc_completion)
    i.pending_user_evts_send                 0x00027aa0   Section        0  ble_db_discovery.o(i.pending_user_evts_send)
    pending_user_evts_send                   0x00027aa1   Thumb Code    38  ble_db_discovery.o(i.pending_user_evts_send)
    i.pin_in_use_by_gpiote                   0x00027ad4   Section        0  nrf_drv_gpiote.o(i.pin_in_use_by_gpiote)
    pin_in_use_by_gpiote                     0x00027ad5   Thumb Code    22  nrf_drv_gpiote.o(i.pin_in_use_by_gpiote)
    i.pin_in_use_by_port                     0x00027af0   Section        0  nrf_drv_gpiote.o(i.pin_in_use_by_port)
    pin_in_use_by_port                       0x00027af1   Thumb Code    18  nrf_drv_gpiote.o(i.pin_in_use_by_port)
    i.pin_in_use_by_te                       0x00027b08   Section        0  nrf_drv_gpiote.o(i.pin_in_use_by_te)
    pin_in_use_by_te                         0x00027b09   Thumb Code    26  nrf_drv_gpiote.o(i.pin_in_use_by_te)
    i.pin_in_use_clear                       0x00027b28   Section        0  nrf_drv_gpiote.o(i.pin_in_use_clear)
    pin_in_use_clear                         0x00027b29   Thumb Code     8  nrf_drv_gpiote.o(i.pin_in_use_clear)
    i.postfix_process                        0x00027b34   Section        0  nrf_log_str_formatter.o(i.postfix_process)
    postfix_process                          0x00027b35   Thumb Code    56  nrf_log_str_formatter.o(i.postfix_process)
    i.power_init                             0x00027b78   Section        0  main.o(i.power_init)
    power_init                               0x00027b79   Thumb Code    28  main.o(i.power_init)
    i.prefix_process                         0x00027b94   Section        0  nrf_log_str_formatter.o(i.prefix_process)
    prefix_process                           0x00027b95   Thumb Code    68  nrf_log_str_formatter.o(i.prefix_process)
    i.ram_end_address_get                    0x00027bf0   Section        0  nrf_sdh_ble.o(i.ram_end_address_get)
    ram_end_address_get                      0x00027bf1   Thumb Code    12  nrf_sdh_ble.o(i.ram_end_address_get)
    i.registered_handler_get                 0x00027c00   Section        0  ble_db_discovery.o(i.registered_handler_get)
    registered_handler_get                   0x00027c01   Thumb Code    52  ble_db_discovery.o(i.registered_handler_get)
    i.registered_handler_set                 0x00027c40   Section        0  ble_db_discovery.o(i.registered_handler_set)
    registered_handler_set                   0x00027c41   Thumb Code    58  ble_db_discovery.o(i.registered_handler_set)
    i.rtc1_compare0_set                      0x00027c84   Section        0  app_timer.o(i.rtc1_compare0_set)
    rtc1_compare0_set                        0x00027c85   Thumb Code     6  app_timer.o(i.rtc1_compare0_set)
    i.rtc1_counter_get                       0x00027c90   Section        0  app_timer.o(i.rtc1_counter_get)
    rtc1_counter_get                         0x00027c91   Thumb Code     6  app_timer.o(i.rtc1_counter_get)
    i.rtc1_init                              0x00027c9c   Section        0  app_timer.o(i.rtc1_init)
    rtc1_init                                0x00027c9d   Thumb Code    18  app_timer.o(i.rtc1_init)
    i.rtc1_start                             0x00027cb4   Section        0  app_timer.o(i.rtc1_start)
    rtc1_start                               0x00027cb5   Thumb Code    48  app_timer.o(i.rtc1_start)
    i.rtc1_stop                              0x00027cf0   Section        0  app_timer.o(i.rtc1_stop)
    rtc1_stop                                0x00027cf1   Thumb Code    68  app_timer.o(i.rtc1_stop)
    i.rx_byte                                0x00027d48   Section        0  nrf_drv_uart.o(i.rx_byte)
    rx_byte                                  0x00027d49   Thumb Code    62  nrf_drv_uart.o(i.rx_byte)
    i.rx_done_event                          0x00027d86   Section        0  nrf_drv_uart.o(i.rx_done_event)
    rx_done_event                            0x00027d87   Thumb Code    30  nrf_drv_uart.o(i.rx_done_event)
    i.rx_enable                              0x00027da4   Section        0  nrf_drv_uart.o(i.rx_enable)
    rx_enable                                0x00027da5   Thumb Code    34  nrf_drv_uart.o(i.rx_enable)
    i.scan_start                             0x00027dc8   Section        0  main.o(i.scan_start)
    scan_start                               0x00027dc9   Thumb Code    54  main.o(i.scan_start)
    i.sd_nvic_EnableIRQ                      0x00027e04   Section        0  nrf_sdh.o(i.sd_nvic_EnableIRQ)
    sd_nvic_EnableIRQ                        0x00027e05   Thumb Code   146  nrf_sdh.o(i.sd_nvic_EnableIRQ)
    i.sd_nvic_critical_region_enter          0x00027ea4   Section        0  app_util_platform.o(i.sd_nvic_critical_region_enter)
    sd_nvic_critical_region_enter            0x00027ea5   Thumb Code    90  app_util_platform.o(i.sd_nvic_critical_region_enter)
    i.sd_state_evt_handler                   0x00027f0c   Section        0  nrf_drv_clock.o(i.sd_state_evt_handler)
    sd_state_evt_handler                     0x00027f0d   Thumb Code   100  nrf_drv_clock.o(i.sd_state_evt_handler)
    i.sdh_request_observer_notify            0x00027f78   Section        0  nrf_sdh.o(i.sdh_request_observer_notify)
    sdh_request_observer_notify              0x00027f79   Thumb Code    56  nrf_sdh.o(i.sdh_request_observer_notify)
    i.sdh_state_observer_notify              0x00027fb4   Section        0  nrf_sdh.o(i.sdh_state_observer_notify)
    sdh_state_observer_notify                0x00027fb5   Thumb Code    48  nrf_sdh.o(i.sdh_state_observer_notify)
    i.serial_tx                              0x00027fe8   Section        0  nrf_log_backend_rtt.o(i.serial_tx)
    serial_tx                                0x00027fe9   Thumb Code    62  nrf_log_backend_rtt.o(i.serial_tx)
    i.shutdown_handler                       0x00028026   Section        0  main.o(i.shutdown_handler)
    shutdown_handler                         0x00028027   Thumb Code    66  main.o(i.shutdown_handler)
    i.shutdown_process                       0x00028068   Section        0  nrf_pwr_mgmt.o(i.shutdown_process)
    shutdown_process                         0x00028069   Thumb Code   182  nrf_pwr_mgmt.o(i.shutdown_process)
    i.soc_evt_handler                        0x00028134   Section        0  nrf_drv_clock.o(i.soc_evt_handler)
    soc_evt_handler                          0x00028135   Thumb Code    16  nrf_drv_clock.o(i.soc_evt_handler)
    i.softdevices_evt_irq_enable             0x00028144   Section        0  nrf_sdh.o(i.softdevices_evt_irq_enable)
    softdevices_evt_irq_enable               0x00028145   Thumb Code    30  nrf_sdh.o(i.softdevices_evt_irq_enable)
    i.startup_event_extract                  0x00028162   Section        0  bsp_btn_ble.o(i.startup_event_extract)
    startup_event_extract                    0x00028163   Thumb Code    38  bsp_btn_ble.o(i.startup_event_extract)
    i.std_header_set                         0x00028188   Section        0  nrf_log_frontend.o(i.std_header_set)
    std_header_set                           0x00028189   Thumb Code    76  nrf_log_frontend.o(i.std_header_set)
    i.std_n                                  0x000281d8   Section        0  nrf_log_frontend.o(i.std_n)
    std_n                                    0x000281d9   Thumb Code   104  nrf_log_frontend.o(i.std_n)
    i.string_print                           0x00028244   Section        0  nrf_fprintf_format.o(i.string_print)
    string_print                             0x00028245   Thumb Code   116  nrf_fprintf_format.o(i.string_print)
    i.ticks_diff_get                         0x000282b8   Section        0  app_timer.o(i.ticks_diff_get)
    ticks_diff_get                           0x000282b9   Thumb Code    10  app_timer.o(i.ticks_diff_get)
    i.timeout_handler_exec                   0x000282c2   Section        0  app_timer.o(i.timeout_handler_exec)
    timeout_handler_exec                     0x000282c3   Thumb Code    12  app_timer.o(i.timeout_handler_exec)
    i.timer_init                             0x000282ce   Section        0  main.o(i.timer_init)
    timer_init                               0x000282cf   Thumb Code    28  main.o(i.timer_init)
    i.timer_list_handler                     0x000282ec   Section        0  app_timer.o(i.timer_list_handler)
    timer_list_handler                       0x000282ed   Thumb Code    68  app_timer.o(i.timer_list_handler)
    i.timer_list_handler_sched               0x0002833c   Section        0  app_timer.o(i.timer_list_handler_sched)
    timer_list_handler_sched                 0x0002833d   Thumb Code    10  app_timer.o(i.timer_list_handler_sched)
    i.timer_list_insert                      0x00028348   Section        0  app_timer.o(i.timer_list_insert)
    timer_list_insert                        0x00028349   Thumb Code    98  app_timer.o(i.timer_list_insert)
    i.timer_list_remove                      0x000283b0   Section        0  app_timer.o(i.timer_list_remove)
    timer_list_remove                        0x000283b1   Thumb Code   118  app_timer.o(i.timer_list_remove)
    i.timer_start_op_schedule                0x00028438   Section        0  app_timer.o(i.timer_start_op_schedule)
    timer_start_op_schedule                  0x00028439   Thumb Code    94  app_timer.o(i.timer_start_op_schedule)
    i.timer_stop_op_schedule                 0x00028496   Section        0  app_timer.o(i.timer_stop_op_schedule)
    timer_stop_op_schedule                   0x00028497   Thumb Code    66  app_timer.o(i.timer_stop_op_schedule)
    i.timer_timeouts_check                   0x000284d8   Section        0  app_timer.o(i.timer_timeouts_check)
    timer_timeouts_check                     0x000284d9   Thumb Code   130  app_timer.o(i.timer_timeouts_check)
    i.timer_timeouts_check_sched             0x00028570   Section        0  app_timer.o(i.timer_timeouts_check_sched)
    timer_timeouts_check_sched               0x00028571   Thumb Code    10  app_timer.o(i.timer_timeouts_check_sched)
    i.tx_byte                                0x0002857a   Section        0  nrf_drv_uart.o(i.tx_byte)
    tx_byte                                  0x0002857b   Thumb Code    38  nrf_drv_uart.o(i.tx_byte)
    i.tx_done_event                          0x000285a0   Section        0  nrf_drv_uart.o(i.tx_done_event)
    tx_done_event                            0x000285a1   Thumb Code    34  nrf_drv_uart.o(i.tx_done_event)
    i.uart_event_handle                      0x000285c4   Section        0  main.o(i.uart_event_handle)
    i.uart_event_handler                     0x000286f0   Section        0  app_uart_fifo.o(i.uart_event_handler)
    uart_event_handler                       0x000286f1   Thumb Code   184  app_uart_fifo.o(i.uart_event_handler)
    i.uart_init                              0x000287c4   Section        0  main.o(i.uart_init)
    uart_init                                0x000287c5   Thumb Code    74  main.o(i.uart_init)
    i.uart_irq_handler                       0x00028820   Section        0  nrf_drv_uart.o(i.uart_irq_handler)
    uart_irq_handler                         0x00028821   Thumb Code   322  nrf_drv_uart.o(i.uart_irq_handler)
    i.uarte_irq_handler                      0x00028962   Section        0  nrf_drv_uart.o(i.uarte_irq_handler)
    uarte_irq_handler                        0x00028963   Thumb Code   268  nrf_drv_uart.o(i.uarte_irq_handler)
    i.unsigned_print                         0x00028a70   Section        0  nrf_fprintf_format.o(i.unsigned_print)
    unsigned_print                           0x00028a71   Thumb Code   178  nrf_fprintf_format.o(i.unsigned_print)
    i.user_op_alloc                          0x00028b28   Section        0  app_timer.o(i.user_op_alloc)
    user_op_alloc                            0x00028b29   Thumb Code    56  app_timer.o(i.user_op_alloc)
    i.user_op_enque                          0x00028b64   Section        0  app_timer.o(i.user_op_enque)
    user_op_enque                            0x00028b65   Thumb Code     6  app_timer.o(i.user_op_enque)
    .constdata                               0x00028b70   Section       44  main.o(.constdata)
    m_connection_param                       0x00028b70   Data           8  main.o(.constdata)
    m_scan_params                            0x00028b78   Data           8  main.o(.constdata)
    m_nus_uuid                               0x00028b80   Data           4  main.o(.constdata)
    .constdata                               0x00028b9c   Section        8  boards.o(.constdata)
    m_board_led_list                         0x00028b9c   Data           4  boards.o(.constdata)
    m_board_btn_list                         0x00028ba0   Data           4  boards.o(.constdata)
    .constdata                               0x00028ba4   Section       44  bsp.o(.constdata)
    m_leds_timer_id                          0x00028ba4   Data           4  bsp.o(.constdata)
    m_alert_timer_id                         0x00028ba8   Data           4  bsp.o(.constdata)
    m_button_timer_id                        0x00028bac   Data           4  bsp.o(.constdata)
    app_buttons                              0x00028bb0   Data          32  bsp.o(.constdata)
    .constdata                               0x00028bd0   Section      124  ble_db_discovery.o(.constdata)
    .constdata                               0x00028c4c   Section       22  nrf_ble_gatt.o(.constdata)
    .constdata                               0x00028c64   Section       40  ble_nus_c.o(.constdata)
    .constdata                               0x00028c8c   Section       75  nrf_drv_gpiote.o(.constdata)
    __func__                                 0x00028c94   Data          20  nrf_drv_gpiote.o(.constdata)
    __func__                                 0x00028ca8   Data          24  nrf_drv_gpiote.o(.constdata)
    __func__                                 0x00028cc0   Data          23  nrf_drv_gpiote.o(.constdata)
    .constdata                               0x00028cd8   Section        8  app_button.o(.constdata)
    m_detection_delay_timer_id               0x00028cd8   Data           4  app_button.o(.constdata)
    .constdata                               0x00028ce0   Section       32  app_uart_fifo.o(.constdata)
    .constdata                               0x00028d00   Section       16  nrf_fprintf_format.o(.constdata)
    _aV2C                                    0x00028d00   Data          16  nrf_fprintf_format.o(.constdata)
    .constdata                               0x00028d10   Section       36  nrf_pwr_mgmt.o(.constdata)
    pwr_mgmt_data_array                      0x00028d10   Data          24  nrf_pwr_mgmt.o(.constdata)
    pwr_mgmt_data                            0x00028d28   Data          12  nrf_pwr_mgmt.o(.constdata)
    .constdata                               0x00028d34   Section      260  nrf_strerror.o(.constdata)
    m_unknown_str                            0x00028d34   Data          19  nrf_strerror.o(.constdata)
    nrf_strerror_array                       0x00028d48   Data         240  nrf_strerror.o(.constdata)
    .constdata                               0x00028e38   Section       12  nrf_log_backend_rtt.o(.constdata)
    .constdata                               0x00028e44   Section       20  nrf_log_frontend.o(.constdata)
    mempool                                  0x00028e44   Data          20  nrf_log_frontend.o(.constdata)
    .constdata                               0x00028e58   Section       88  nrf_sdh.o(.constdata)
    sdh_req_observers_array                  0x00028e58   Data          16  nrf_sdh.o(.constdata)
    sdh_req_observers                        0x00028e68   Data          12  nrf_sdh.o(.constdata)
    sdh_state_observers_array                0x00028e74   Data          16  nrf_sdh.o(.constdata)
    sdh_state_observers                      0x00028e84   Data          12  nrf_sdh.o(.constdata)
    sdh_stack_observers_array                0x00028e90   Data          16  nrf_sdh.o(.constdata)
    sdh_stack_observers                      0x00028ea0   Data          12  nrf_sdh.o(.constdata)
    .constdata                               0x00028eb0   Section       48  nrf_sdh_ble.o(.constdata)
    sdh_ble_observers_array                  0x00028eb0   Data          32  nrf_sdh_ble.o(.constdata)
    sdh_ble_observers                        0x00028ed0   Data          12  nrf_sdh_ble.o(.constdata)
    .constdata                               0x00028ee0   Section       28  nrf_sdh_soc.o(.constdata)
    sdh_soc_observers_array                  0x00028ee0   Data          16  nrf_sdh_soc.o(.constdata)
    sdh_soc_observers                        0x00028ef0   Data          12  nrf_sdh_soc.o(.constdata)
    .constdata                               0x00028efc   Section      129  ctype_o.o(.constdata)
    .constdata                               0x00028f80   Section        4  ctype_o.o(.constdata)
    table                                    0x00028f80   Data           4  ctype_o.o(.constdata)
    .conststring                             0x00028f84   Section      301  nrf_ble_gatt.o(.conststring)
    .conststring                             0x000290b4   Section      775  nrf_strerror.o(.conststring)
    .conststring                             0x000293bc   Section        9  nrf_log_frontend.o(.conststring)
    .conststring                             0x000293c8   Section      102  nrf_log_str_formatter.o(.conststring)
    .conststring                             0x00029430   Section      463  nrf_sdh_ble.o(.conststring)
    .conststrlit                             0x00029600   Section       12  ble_db_discovery.o(.conststrlit)
    .conststrlit                             0x0002960c   Section        9  nrf_ble_gatt.o(.conststrlit)
    .conststrlit                             0x00029618   Section        8  ble_nus_c.o(.conststrlit)
    .conststrlit                             0x00029620   Section        6  nrf_drv_clock.o(.conststrlit)
    .conststrlit                             0x00029628   Section        7  nrf_drv_gpiote.o(.conststrlit)
    .conststrlit                             0x00029630   Section        5  nrf_drv_uart.o(.conststrlit)
    .conststrlit                             0x00029638   Section        7  nrf_balloc.o(.conststrlit)
    .conststrlit                             0x00029640   Section        9  nrf_pwr_mgmt.o(.conststrlit)
    .conststrlit                             0x0002964c   Section        4  nrf_log_frontend.o(.conststrlit)
    .conststrlit                             0x00029650   Section        8  nrf_sdh.o(.conststrlit)
    .conststrlit                             0x00029658   Section       12  nrf_sdh_ble.o(.conststrlit)
    .conststrlit                             0x00029664   Section       12  nrf_sdh_soc.o(.conststrlit)
    log_const_data                           0x00029690   Section        8  ble_db_discovery.o(log_const_data)
    __tagsym$$used                           0x00029690   Number         0  ble_db_discovery.o(log_const_data)
    log_const_data                           0x00029698   Section        8  nrf_ble_gatt.o(log_const_data)
    __tagsym$$used                           0x00029698   Number         0  nrf_ble_gatt.o(log_const_data)
    log_const_data                           0x000296a0   Section        8  ble_nus_c.o(log_const_data)
    __tagsym$$used                           0x000296a0   Number         0  ble_nus_c.o(log_const_data)
    log_const_data                           0x000296a8   Section        8  nrf_drv_clock.o(log_const_data)
    __tagsym$$used                           0x000296a8   Number         0  nrf_drv_clock.o(log_const_data)
    log_const_data                           0x000296b0   Section        8  nrf_drv_gpiote.o(log_const_data)
    __tagsym$$used                           0x000296b0   Number         0  nrf_drv_gpiote.o(log_const_data)
    log_const_data                           0x000296b8   Section        8  nrf_drv_uart.o(log_const_data)
    __tagsym$$used                           0x000296b8   Number         0  nrf_drv_uart.o(log_const_data)
    log_const_data                           0x000296c0   Section        8  nrf_balloc.o(log_const_data)
    __tagsym$$used                           0x000296c0   Number         0  nrf_balloc.o(log_const_data)
    log_const_data                           0x000296c8   Section        8  nrf_pwr_mgmt.o(log_const_data)
    __tagsym$$used                           0x000296c8   Number         0  nrf_pwr_mgmt.o(log_const_data)
    log_const_data                           0x000296d0   Section        8  nrf_log_frontend.o(log_const_data)
    __tagsym$$used                           0x000296d0   Number         0  nrf_log_frontend.o(log_const_data)
    log_const_data                           0x000296d8   Section        8  nrf_sdh.o(log_const_data)
    __tagsym$$used                           0x000296d8   Number         0  nrf_sdh.o(log_const_data)
    log_const_data                           0x000296e0   Section        8  nrf_sdh_ble.o(log_const_data)
    __tagsym$$used                           0x000296e0   Number         0  nrf_sdh_ble.o(log_const_data)
    log_const_data                           0x000296e8   Section        8  nrf_sdh_soc.o(log_const_data)
    __tagsym$$used                           0x000296e8   Number         0  nrf_sdh_soc.o(log_const_data)
    pwr_mgmt_data1                           0x000296f0   Section        4  main.o(pwr_mgmt_data1)
    __tagsym$$used                           0x000296f0   Number         0  main.o(pwr_mgmt_data1)
    shutdown_handler_handler_function        0x000296f0   Data           4  main.o(pwr_mgmt_data1)
    sdh_ble_observers1                       0x000296f4   Section       16  main.o(sdh_ble_observers1)
    __tagsym$$used                           0x000296f4   Number         0  main.o(sdh_ble_observers1)
    m_gatt_obs                               0x000296f4   Data           8  main.o(sdh_ble_observers1)
    __tagsym$$used                           0x000296fc   Number         0  main.o(sdh_ble_observers1)
    m_db_disc_obs                            0x000296fc   Data           8  main.o(sdh_ble_observers1)
    sdh_ble_observers1                       0x00029704   Section        8  bsp_btn_ble.o(sdh_ble_observers1)
    __tagsym$$used                           0x00029704   Number         0  bsp_btn_ble.o(sdh_ble_observers1)
    m_ble_observer                           0x00029704   Data           8  bsp_btn_ble.o(sdh_ble_observers1)
    sdh_ble_observers2                       0x0002970c   Section        8  main.o(sdh_ble_observers2)
    __tagsym$$used                           0x0002970c   Number         0  main.o(sdh_ble_observers2)
    m_ble_nus_c_obs                          0x0002970c   Data           8  main.o(sdh_ble_observers2)
    sdh_ble_observers3                       0x00029714   Section        8  main.o(sdh_ble_observers3)
    __tagsym$$used                           0x00029714   Number         0  main.o(sdh_ble_observers3)
    m_ble_observer                           0x00029714   Data           8  main.o(sdh_ble_observers3)
    sdh_soc_observers0                       0x0002971c   Section        8  nrf_drv_clock.o(sdh_soc_observers0)
    __tagsym$$used                           0x0002971c   Number         0  nrf_drv_clock.o(sdh_soc_observers0)
    m_soc_evt_observer                       0x0002971c   Data           8  nrf_drv_clock.o(sdh_soc_observers0)
    sdh_stack_observers0                     0x00029724   Section        8  nrf_sdh_ble.o(sdh_stack_observers0)
    __tagsym$$used                           0x00029724   Number         0  nrf_sdh_ble.o(sdh_stack_observers0)
    m_nrf_sdh_ble_evts_poll                  0x00029724   Data           8  nrf_sdh_ble.o(sdh_stack_observers0)
    sdh_stack_observers0                     0x0002972c   Section        8  nrf_sdh_soc.o(sdh_stack_observers0)
    __tagsym$$used                           0x0002972c   Number         0  nrf_sdh_soc.o(sdh_stack_observers0)
    m_nrf_sdh_soc_evts_poll                  0x0002972c   Data           8  nrf_sdh_soc.o(sdh_stack_observers0)
    sdh_state_observers0                     0x00029734   Section        8  nrf_drv_clock.o(sdh_state_observers0)
    __tagsym$$used                           0x00029734   Number         0  nrf_drv_clock.o(sdh_state_observers0)
    m_sd_state_observer                      0x00029734   Data           8  nrf_drv_clock.o(sdh_state_observers0)
    .data                                    0x20002978   Section      720  main.o(.data)
    m_db_disc                                0x20002978   Data         716  main.o(.data)
    m_ble_nus_max_data_len                   0x20002c44   Data           2  main.o(.data)
    index                                    0x20002c46   Data           2  main.o(.data)
    .data                                    0x20002c48   Section       21  bsp.o(.data)
    m_stable_state                           0x20002c48   Data           1  bsp.o(.data)
    m_leds_clear                             0x20002c49   Data           1  bsp.o(.data)
    m_indication_type                        0x20002c4c   Data           4  bsp.o(.data)
    m_alert_on                               0x20002c50   Data           1  bsp.o(.data)
    m_registered_callback                    0x20002c54   Data           4  bsp.o(.data)
    current_long_push_pin_no                 0x20002c58   Data           1  bsp.o(.data)
    release_event_at_push                    0x20002c59   Data           4  bsp.o(.data)
    .data                                    0x20002c60   Section        8  bsp_btn_ble.o(.data)
    m_error_handler                          0x20002c60   Data           4  bsp_btn_ble.o(.data)
    m_num_connections                        0x20002c64   Data           4  bsp_btn_ble.o(.data)
    .data                                    0x20002c68   Section       13  ble_db_discovery.o(.data)
    m_evt_handler                            0x20002c68   Data           4  ble_db_discovery.o(.data)
    m_pending_usr_evt_index                  0x20002c6c   Data           4  ble_db_discovery.o(.data)
    m_num_of_handlers_reg                    0x20002c70   Data           4  ble_db_discovery.o(.data)
    m_initialized                            0x20002c74   Data           1  ble_db_discovery.o(.data)
    .data                                    0x20002c78   Section       20  app_button.o(.data)
    mp_buttons                               0x20002c78   Data           4  app_button.o(.data)
    m_button_count                           0x20002c7c   Data           1  app_button.o(.data)
    m_detection_delay                        0x20002c80   Data           4  app_button.o(.data)
    m_pin_state                              0x20002c84   Data           4  app_button.o(.data)
    m_pin_transition                         0x20002c88   Data           4  app_button.o(.data)
    .data                                    0x20002c8c   Section       20  app_timer.o(.data)
    mp_timer_id_head                         0x20002c8c   Data           4  app_timer.o(.data)
    m_ticks_latest                           0x20002c90   Data           4  app_timer.o(.data)
    m_ticks_elapsed                          0x20002c94   Data           8  app_timer.o(.data)
    m_ticks_elapsed_q_read_ind               0x20002c9c   Data           1  app_timer.o(.data)
    m_ticks_elapsed_q_write_ind              0x20002c9d   Data           1  app_timer.o(.data)
    m_rtc1_running                           0x20002c9e   Data           1  app_timer.o(.data)
    m_rtc1_reset                             0x20002c9f   Data           1  app_timer.o(.data)
    .data                                    0x20002ca0   Section       15  app_uart_fifo.o(.data)
    app_uart_inst                            0x20002ca0   Data           8  app_uart_fifo.o(.data)
    m_event_handler                          0x20002ca8   Data           4  app_uart_fifo.o(.data)
    tx_buffer                                0x20002cac   Data           1  app_uart_fifo.o(.data)
    rx_buffer                                0x20002cad   Data           1  app_uart_fifo.o(.data)
    m_rx_ovf                                 0x20002cae   Data           1  app_uart_fifo.o(.data)
    .data                                    0x20002cb0   Section        9  nrf_pwr_mgmt.o(.data)
    m_pwr_mgmt_evt                           0x20002cb0   Data           1  nrf_pwr_mgmt.o(.data)
    m_sysoff_mtx                             0x20002cb4   Data           4  nrf_pwr_mgmt.o(.data)
    m_shutdown_started                       0x20002cb8   Data           1  nrf_pwr_mgmt.o(.data)
    .data                                    0x20002cbc   Section        8  retarget.o(.data)
    .data                                    0x20002cc4   Section       12  nrf_log_default_backends.o(.data)
    rtt_log_backend                          0x20002cc4   Data          12  nrf_log_default_backends.o(.data)
    .data                                    0x20002cd0   Section       20  nrf_log_frontend.o(.data)
    mempool_nrf_balloc_pool_stack            0x20002cd0   Data           8  nrf_log_frontend.o(.data)
    mempool_nrf_balloc_cb                    0x20002cd8   Data           8  nrf_log_frontend.o(.data)
    m_overflow_info                          0x20002ce0   Data           4  nrf_log_frontend.o(.data)
    .data                                    0x20002ce4   Section       56  nrf_log_str_formatter.o(.data)
    severity_names                           0x20002ce4   Data          20  nrf_log_str_formatter.o(.data)
    m_colors                                 0x20002cf8   Data          36  nrf_log_str_formatter.o(.data)
    .data                                    0x20002d1c   Section        3  nrf_sdh.o(.data)
    m_nrf_sdh_enabled                        0x20002d1c   Data           1  nrf_sdh.o(.data)
    m_nrf_sdh_suspended                      0x20002d1d   Data           1  nrf_sdh.o(.data)
    m_nrf_sdh_continue                       0x20002d1e   Data           1  nrf_sdh.o(.data)
    .data                                    0x20002d20   Section        4  system_nrf52840.o(.data)
    __tagsym$$used                           0x20002d20   Number         0  system_nrf52840.o(.data)
    log_dynamic_data                         0x20002d24   Section       12  ble_db_discovery.o(log_dynamic_data)
    __tagsym$$used                           0x20002d24   Number         0  ble_db_discovery.o(log_dynamic_data)
    log_dynamic_data                         0x20002d30   Section       12  nrf_ble_gatt.o(log_dynamic_data)
    __tagsym$$used                           0x20002d30   Number         0  nrf_ble_gatt.o(log_dynamic_data)
    log_dynamic_data                         0x20002d3c   Section       12  ble_nus_c.o(log_dynamic_data)
    __tagsym$$used                           0x20002d3c   Number         0  ble_nus_c.o(log_dynamic_data)
    log_dynamic_data                         0x20002d48   Section       12  nrf_drv_clock.o(log_dynamic_data)
    __tagsym$$used                           0x20002d48   Number         0  nrf_drv_clock.o(log_dynamic_data)
    log_dynamic_data                         0x20002d54   Section       12  nrf_drv_gpiote.o(log_dynamic_data)
    __tagsym$$used                           0x20002d54   Number         0  nrf_drv_gpiote.o(log_dynamic_data)
    log_dynamic_data                         0x20002d60   Section       12  nrf_drv_uart.o(log_dynamic_data)
    __tagsym$$used                           0x20002d60   Number         0  nrf_drv_uart.o(log_dynamic_data)
    log_dynamic_data                         0x20002d6c   Section       12  nrf_balloc.o(log_dynamic_data)
    __tagsym$$used                           0x20002d6c   Number         0  nrf_balloc.o(log_dynamic_data)
    log_dynamic_data                         0x20002d78   Section       12  nrf_pwr_mgmt.o(log_dynamic_data)
    __tagsym$$used                           0x20002d78   Number         0  nrf_pwr_mgmt.o(log_dynamic_data)
    log_dynamic_data                         0x20002d84   Section       12  nrf_log_frontend.o(log_dynamic_data)
    __tagsym$$used                           0x20002d84   Number         0  nrf_log_frontend.o(log_dynamic_data)
    log_dynamic_data                         0x20002d90   Section       12  nrf_sdh.o(log_dynamic_data)
    __tagsym$$used                           0x20002d90   Number         0  nrf_sdh.o(log_dynamic_data)
    log_dynamic_data                         0x20002d9c   Section       12  nrf_sdh_ble.o(log_dynamic_data)
    __tagsym$$used                           0x20002d9c   Number         0  nrf_sdh_ble.o(log_dynamic_data)
    log_dynamic_data                         0x20002da8   Section       12  nrf_sdh_soc.o(log_dynamic_data)
    __tagsym$$used                           0x20002da8   Number         0  nrf_sdh_soc.o(log_dynamic_data)
    .bss                                     0x20002db4   Section      792  main.o(.bss)
    m_ble_nus_c                              0x20002db4   Data          16  main.o(.bss)
    m_gatt                                   0x20002dc4   Data          20  main.o(.bss)
    data_array                               0x20002dd8   Data         244  main.o(.bss)
    rx_buf                                   0x20002ecc   Data         256  main.o(.bss)
    tx_buf                                   0x20002fcc   Data         256  main.o(.bss)
    .bss                                     0x200030cc   Section      108  bsp.o(.bss)
    m_leds_timer_id_data                     0x200030cc   Data          32  bsp.o(.bss)
    m_alert_timer_id_data                    0x200030ec   Data          32  bsp.o(.bss)
    m_events_list                            0x2000310c   Data          12  bsp.o(.bss)
    m_button_timer_id_data                   0x20003118   Data          32  bsp.o(.bss)
    .bss                                     0x20003138   Section      792  ble_db_discovery.o(.bss)
    m_registered_handlers                    0x20003138   Data          24  ble_db_discovery.o(.bss)
    m_pending_user_evts                      0x20003150   Data         768  ble_db_discovery.o(.bss)
    .bss                                     0x20003450   Section       20  nrf_drv_clock.o(.bss)
    m_clock_cb                               0x20003450   Data          20  nrf_drv_clock.o(.bss)
    .bss                                     0x20003464   Section      104  nrf_drv_gpiote.o(.bss)
    m_cb                                     0x20003464   Data         104  nrf_drv_gpiote.o(.bss)
    .bss                                     0x200034cc   Section       32  nrf_drv_uart.o(.bss)
    m_cb                                     0x200034cc   Data          32  nrf_drv_uart.o(.bss)
    .bss                                     0x200034ec   Section       32  app_button.o(.bss)
    m_detection_delay_timer_id_data          0x200034ec   Data          32  app_button.o(.bss)
    .bss                                     0x2000350c   Section      268  app_timer.o(.bss)
    m_op_queue                               0x2000350c   Data         268  app_timer.o(.bss)
    .bss                                     0x20003618   Section       32  app_uart_fifo.o(.bss)
    m_rx_fifo                                0x20003618   Data          16  app_uart_fifo.o(.bss)
    m_tx_fifo                                0x20003628   Data          16  app_uart_fifo.o(.bss)
    .bss                                     0x20003638   Section       12  app_util_platform.o(.bss)
    .bss                                     0x20003644   Section       12  nrf_pwr_mgmt.o(.bss)
    m_handlers_iter                          0x20003644   Data          12  nrf_pwr_mgmt.o(.bss)
    .bss                                     0x20003650   Section       64  nrf_log_backend_rtt.o(.bss)
    m_string_buff                            0x20003650   Data          64  nrf_log_backend_rtt.o(.bss)
    .bss                                     0x20003690   Section     1248  nrf_log_frontend.o(.bss)
    mempool_nrf_balloc_pool_mem              0x20003690   Data         192  nrf_log_frontend.o(.bss)
    m_log_data                               0x20003750   Data        1056  nrf_log_frontend.o(.bss)
    .bss                                     0x20003b70   Section      648  segger_rtt.o(.bss)
    _acUpBuffer                              0x20003be8   Data         512  segger_rtt.o(.bss)
    _acDownBuffer                            0x20003de8   Data          16  segger_rtt.o(.bss)
    STACK                                    0x20003df8   Section     8192  arm_startup_nrf52840.o(STACK)

    Global Symbols

    Symbol Name                              Value     Ov Type        Size  Object(Section)

    BuildAttributes$$THM_ISAv4$E$P$D$K$B$S$7EM$VFPi3$EXTD16$VFPS$VFMA$PE$A:L22UL41UL21$X:L11$S22US41US21$IEEE1$IW$USESV6$~STKCKD$USESV7$~SHL$OSPACE$ROPI$EBA8$MICROLIB$REQ8$PRES8$EABIv2 0x00000000   Number         0  anon$$obj.o ABSOLUTE
    __ARM_use_no_argv                        0x00000000   Number         0  main.o ABSOLUTE
    __cpp_initialize__aeabi_                  - Undefined Weak Reference
    __cxa_finalize                            - Undefined Weak Reference
    _clock_init                               - Undefined Weak Reference
    _microlib_exit                            - Undefined Weak Reference
    pwr_mgmt_data0$$Base                      - Undefined Reference
    pwr_mgmt_data0$$Limit                     - Undefined Reference
    pwr_mgmt_data2$$Base                      - Undefined Reference
    pwr_mgmt_data2$$Limit                     - Undefined Reference
    sdh_ble_observers0$$Base                  - Undefined Reference
    sdh_ble_observers0$$Limit                 - Undefined Reference
    sdh_req_observers0$$Base                  - Undefined Reference
    sdh_req_observers0$$Limit                 - Undefined Reference
    sdh_req_observers1$$Base                  - Undefined Reference
    sdh_req_observers1$$Limit                 - Undefined Reference
    sdh_soc_observers1$$Base                  - Undefined Reference
    sdh_soc_observers1$$Limit                 - Undefined Reference
    sdh_stack_observers1$$Base                - Undefined Reference
    sdh_stack_observers1$$Limit               - Undefined Reference
    sdh_state_observers1$$Base                - Undefined Reference
    sdh_state_observers1$$Limit               - Undefined Reference
    __Vectors_Size                           0x00000200   Number         0  arm_startup_nrf52840.o ABSOLUTE
    __Vectors                                0x00022000   Data           4  arm_startup_nrf52840.o(RESET)
    __Vectors_End                            0x00022200   Data           0  arm_startup_nrf52840.o(RESET)
    __main                                   0x00022201   Thumb Code     0  entry.o(.ARM.Collect$$$$00000000)
    _main_stk                                0x00022201   Thumb Code     0  entry2.o(.ARM.Collect$$$$00000001)
    _main_scatterload                        0x00022205   Thumb Code     0  entry5.o(.ARM.Collect$$$$00000004)
    __main_after_scatterload                 0x00022209   Thumb Code     0  entry5.o(.ARM.Collect$$$$00000004)
    _main_clock                              0x00022209   Thumb Code     0  entry7b.o(.ARM.Collect$$$$00000008)
    _main_cpp_init                           0x00022209   Thumb Code     0  entry8b.o(.ARM.Collect$$$$0000000A)
    _main_init                               0x00022209   Thumb Code     0  entry9a.o(.ARM.Collect$$$$0000000B)
    __rt_final_cpp                           0x00022211   Thumb Code     0  entry10a.o(.ARM.Collect$$$$0000000D)
    __rt_final_exit                          0x00022211   Thumb Code     0  entry11a.o(.ARM.Collect$$$$0000000F)
    __asm___12_nrf_memobj_c_9bb9f865__nrf_atomic_internal_mov 0x00022215   Thumb Code    24  nrf_memobj.o(.emb_text)
    __asm___12_nrf_memobj_c_9bb9f865__nrf_atomic_internal_orr 0x0002222d   Thumb Code    26  nrf_memobj.o(.emb_text)
    __asm___12_nrf_memobj_c_9bb9f865__nrf_atomic_internal_and 0x00022247   Thumb Code    26  nrf_memobj.o(.emb_text)
    __asm___12_nrf_memobj_c_9bb9f865__nrf_atomic_internal_eor 0x00022261   Thumb Code    26  nrf_memobj.o(.emb_text)
    __asm___12_nrf_memobj_c_9bb9f865__nrf_atomic_internal_add 0x0002227b   Thumb Code    26  nrf_memobj.o(.emb_text)
    __asm___12_nrf_memobj_c_9bb9f865__nrf_atomic_internal_sub 0x00022295   Thumb Code    26  nrf_memobj.o(.emb_text)
    __asm___14_nrf_pwr_mgmt_c_f22138a6__nrf_atomic_internal_mov 0x000222b1   Thumb Code    24  nrf_pwr_mgmt.o(.emb_text)
    __asm___14_nrf_pwr_mgmt_c_f22138a6__nrf_atomic_internal_orr 0x000222c9   Thumb Code    26  nrf_pwr_mgmt.o(.emb_text)
    __asm___14_nrf_pwr_mgmt_c_f22138a6__nrf_atomic_internal_and 0x000222e3   Thumb Code    26  nrf_pwr_mgmt.o(.emb_text)
    __asm___14_nrf_pwr_mgmt_c_f22138a6__nrf_atomic_internal_eor 0x000222fd   Thumb Code    26  nrf_pwr_mgmt.o(.emb_text)
    __asm___14_nrf_pwr_mgmt_c_f22138a6__nrf_atomic_internal_add 0x00022317   Thumb Code    26  nrf_pwr_mgmt.o(.emb_text)
    __asm___14_nrf_pwr_mgmt_c_f22138a6__nrf_atomic_internal_sub 0x00022331   Thumb Code    26  nrf_pwr_mgmt.o(.emb_text)
    __asm___18_nrf_log_frontend_c_bc460776__nrf_atomic_internal_mov 0x0002234d   Thumb Code    24  nrf_log_frontend.o(.emb_text)
    __asm___18_nrf_log_frontend_c_bc460776__nrf_atomic_internal_orr 0x00022365   Thumb Code    26  nrf_log_frontend.o(.emb_text)
    __asm___18_nrf_log_frontend_c_bc460776__nrf_atomic_internal_and 0x0002237f   Thumb Code    26  nrf_log_frontend.o(.emb_text)
    __asm___18_nrf_log_frontend_c_bc460776__nrf_atomic_internal_eor 0x00022399   Thumb Code    26  nrf_log_frontend.o(.emb_text)
    __asm___18_nrf_log_frontend_c_bc460776__nrf_atomic_internal_add 0x000223b3   Thumb Code    26  nrf_log_frontend.o(.emb_text)
    __asm___18_nrf_log_frontend_c_bc460776__nrf_atomic_internal_sub 0x000223cd   Thumb Code    26  nrf_log_frontend.o(.emb_text)
    Reset_Handler                            0x000223e9   Thumb Code     8  arm_startup_nrf52840.o(.text)
    NMI_Handler                              0x000223f1   Thumb Code     2  arm_startup_nrf52840.o(.text)
    HardFault_Handler                        0x000223f3   Thumb Code     2  arm_startup_nrf52840.o(.text)
    MemoryManagement_Handler                 0x000223f5   Thumb Code     2  arm_startup_nrf52840.o(.text)
    BusFault_Handler                         0x000223f7   Thumb Code     2  arm_startup_nrf52840.o(.text)
    UsageFault_Handler                       0x000223f9   Thumb Code     2  arm_startup_nrf52840.o(.text)
    SVC_Handler                              0x000223fb   Thumb Code     2  arm_startup_nrf52840.o(.text)
    DebugMon_Handler                         0x000223fd   Thumb Code     2  arm_startup_nrf52840.o(.text)
    PendSV_Handler                           0x000223ff   Thumb Code     2  arm_startup_nrf52840.o(.text)
    SysTick_Handler                          0x00022401   Thumb Code     2  arm_startup_nrf52840.o(.text)
    CCM_AAR_IRQHandler                       0x00022403   Thumb Code     0  arm_startup_nrf52840.o(.text)
    COMP_LPCOMP_IRQHandler                   0x00022403   Thumb Code     0  arm_startup_nrf52840.o(.text)
    CRYPTOCELL_IRQHandler                    0x00022403   Thumb Code     0  arm_startup_nrf52840.o(.text)
    ECB_IRQHandler                           0x00022403   Thumb Code     0  arm_startup_nrf52840.o(.text)
    FPU_IRQHandler                           0x00022403   Thumb Code     0  arm_startup_nrf52840.o(.text)
    I2S_IRQHandler                           0x00022403   Thumb Code     0  arm_startup_nrf52840.o(.text)
    MWU_IRQHandler                           0x00022403   Thumb Code     0  arm_startup_nrf52840.o(.text)
    NFCT_IRQHandler                          0x00022403   Thumb Code     0  arm_startup_nrf52840.o(.text)
    PDM_IRQHandler                           0x00022403   Thumb Code     0  arm_startup_nrf52840.o(.text)
    PWM0_IRQHandler                          0x00022403   Thumb Code     0  arm_startup_nrf52840.o(.text)
    PWM1_IRQHandler                          0x00022403   Thumb Code     0  arm_startup_nrf52840.o(.text)
    PWM2_IRQHandler                          0x00022403   Thumb Code     0  arm_startup_nrf52840.o(.text)
    PWM3_IRQHandler                          0x00022403   Thumb Code     0  arm_startup_nrf52840.o(.text)
    QDEC_IRQHandler                          0x00022403   Thumb Code     0  arm_startup_nrf52840.o(.text)
    QSPI_IRQHandler                          0x00022403   Thumb Code     0  arm_startup_nrf52840.o(.text)
    RADIO_IRQHandler                         0x00022403   Thumb Code     0  arm_startup_nrf52840.o(.text)
    RNG_IRQHandler                           0x00022403   Thumb Code     0  arm_startup_nrf52840.o(.text)
    RTC0_IRQHandler                          0x00022403   Thumb Code     0  arm_startup_nrf52840.o(.text)
    RTC2_IRQHandler                          0x00022403   Thumb Code     0  arm_startup_nrf52840.o(.text)
    SAADC_IRQHandler                         0x00022403   Thumb Code     0  arm_startup_nrf52840.o(.text)
    SPIM0_SPIS0_TWIM0_TWIS0_SPI0_TWI0_IRQHandler 0x00022403   Thumb Code     0  arm_startup_nrf52840.o(.text)
    SPIM1_SPIS1_TWIM1_TWIS1_SPI1_TWI1_IRQHandler 0x00022403   Thumb Code     0  arm_startup_nrf52840.o(.text)
    SPIM2_SPIS2_SPI2_IRQHandler              0x00022403   Thumb Code     0  arm_startup_nrf52840.o(.text)
    SPIM3_IRQHandler                         0x00022403   Thumb Code     0  arm_startup_nrf52840.o(.text)
    SWI1_EGU1_IRQHandler                     0x00022403   Thumb Code     0  arm_startup_nrf52840.o(.text)
    SWI3_EGU3_IRQHandler                     0x00022403   Thumb Code     0  arm_startup_nrf52840.o(.text)
    SWI4_EGU4_IRQHandler                     0x00022403   Thumb Code     0  arm_startup_nrf52840.o(.text)
    SWI5_EGU5_IRQHandler                     0x00022403   Thumb Code     0  arm_startup_nrf52840.o(.text)
    TEMP_IRQHandler                          0x00022403   Thumb Code     0  arm_startup_nrf52840.o(.text)
    TIMER0_IRQHandler                        0x00022403   Thumb Code     0  arm_startup_nrf52840.o(.text)
    TIMER1_IRQHandler                        0x00022403   Thumb Code     0  arm_startup_nrf52840.o(.text)
    TIMER2_IRQHandler                        0x00022403   Thumb Code     0  arm_startup_nrf52840.o(.text)
    TIMER3_IRQHandler                        0x00022403   Thumb Code     0  arm_startup_nrf52840.o(.text)
    TIMER4_IRQHandler                        0x00022403   Thumb Code     0  arm_startup_nrf52840.o(.text)
    UARTE1_IRQHandler                        0x00022403   Thumb Code     0  arm_startup_nrf52840.o(.text)
    USBD_IRQHandler                          0x00022403   Thumb Code     0  arm_startup_nrf52840.o(.text)
    WDT_IRQHandler                           0x00022403   Thumb Code     0  arm_startup_nrf52840.o(.text)
    __aeabi_uldivmod                         0x0002240d   Thumb Code    98  uldiv.o(.text)
    __rt_ctype_table                         0x00022471   Thumb Code     4  ctype_o.o(.text)
    __aeabi_memcpy                           0x00022479   Thumb Code    36  memcpya.o(.text)
    __aeabi_memcpy4                          0x00022479   Thumb Code     0  memcpya.o(.text)
    __aeabi_memcpy8                          0x00022479   Thumb Code     0  memcpya.o(.text)
    __aeabi_memset                           0x0002249d   Thumb Code    14  memseta.o(.text)
    __aeabi_memset4                          0x0002249d   Thumb Code     0  memseta.o(.text)
    __aeabi_memset8                          0x0002249d   Thumb Code     0  memseta.o(.text)
    __aeabi_memclr                           0x000224ab   Thumb Code     4  memseta.o(.text)
    __aeabi_memclr4                          0x000224ab   Thumb Code     0  memseta.o(.text)
    __aeabi_memclr8                          0x000224ab   Thumb Code     0  memseta.o(.text)
    _memset$wrapper                          0x000224af   Thumb Code    18  memseta.o(.text)
    strlen                                   0x000224c1   Thumb Code    14  strlen.o(.text)
    strcpy                                   0x000224cf   Thumb Code    18  strcpy.o(.text)
    __aeabi_llsl                             0x000224e1   Thumb Code    30  llshl.o(.text)
    _ll_shift_l                              0x000224e1   Thumb Code     0  llshl.o(.text)
    __aeabi_llsr                             0x000224ff   Thumb Code    32  llushr.o(.text)
    _ll_ushift_r                             0x000224ff   Thumb Code     0  llushr.o(.text)
    __scatterload                            0x00022521   Thumb Code    28  init.o(.text)
    __scatterload_rt2                        0x00022521   Thumb Code     0  init.o(.text)
    __decompress                             0x00022545   Thumb Code     0  __dczerorl2.o(.text)
    __decompress1                            0x00022545   Thumb Code    86  __dczerorl2.o(.text)
    GPIOTE_IRQHandler                        0x0002259d   Thumb Code   564  nrf_drv_gpiote.o(i.GPIOTE_IRQHandler)
    POWER_CLOCK_IRQHandler                   0x0002284d   Thumb Code    74  nrf_drv_clock.o(i.POWER_CLOCK_IRQHandler)
    RTC1_IRQHandler                          0x0002289d   Thumb Code    44  app_timer.o(i.RTC1_IRQHandler)
    SEGGER_RTT_Init                          0x000228d1   Thumb Code     8  segger_rtt.o(i.SEGGER_RTT_Init)
    SEGGER_RTT_WriteNoLock                   0x000228d9   Thumb Code   126  segger_rtt.o(i.SEGGER_RTT_WriteNoLock)
    SWI0_EGU0_IRQHandler                     0x0002295d   Thumb Code     8  app_timer.o(i.SWI0_EGU0_IRQHandler)
    SWI2_EGU2_IRQHandler                     0x00022965   Thumb Code     8  nrf_sdh.o(i.SWI2_EGU2_IRQHandler)
    SystemCoreClockUpdate                    0x0002296d   Thumb Code     8  system_nrf52840.o(i.SystemCoreClockUpdate)
    SystemInit                               0x0002297d   Thumb Code   494  system_nrf52840.o(i.SystemInit)
    UARTE0_UART0_IRQHandler                  0x00022bad   Thumb Code    28  nrf_drv_uart.o(i.UARTE0_UART0_IRQHandler)
    __0printf$bare                           0x00022d1d   Thumb Code     8  printfb.o(i.__0printf$bare)
    __1printf$bare                           0x00022d1d   Thumb Code     0  printfb.o(i.__0printf$bare)
    __2printf                                0x00022d1d   Thumb Code     0  printfb.o(i.__0printf$bare)
    __scatterload_copy                       0x00022d2d   Thumb Code    14  handlers.o(i.__scatterload_copy)
    __scatterload_null                       0x00022d3b   Thumb Code     2  handlers.o(i.__scatterload_null)
    __scatterload_zeroinit                   0x00022d3d   Thumb Code    14  handlers.o(i.__scatterload_zeroinit)
    app_button_enable                        0x00022e15   Thumb Code    34  app_button.o(i.app_button_enable)
    app_button_init                          0x00022e41   Thumb Code   132  app_button.o(i.app_button_init)
    app_error_fault_handler                  0x00022ee9   Thumb Code   134  app_error_weak.o(i.app_error_fault_handler)
    app_error_handler_bare                   0x00022f99   Thumb Code    28  app_error.o(i.app_error_handler_bare)
    app_fifo_get                             0x00022fb5   Thumb Code    30  app_fifo.o(i.app_fifo_get)
    app_fifo_init                            0x00022fd3   Thumb Code    36  app_fifo.o(i.app_fifo_init)
    app_fifo_put                             0x00022ff7   Thumb Code    34  app_fifo.o(i.app_fifo_put)
    app_timer_create                         0x00023019   Thumb Code    56  app_timer.o(i.app_timer_create)
    app_timer_init                           0x00023055   Thumb Code    70  app_timer.o(i.app_timer_init)
    app_timer_start                          0x000230b1   Thumb Code    78  app_timer.o(i.app_timer_start)
    app_timer_stop                           0x00023105   Thumb Code    44  app_timer.o(i.app_timer_stop)
    app_uart_get                             0x00023135   Thumb Code    66  app_uart_fifo.o(i.app_uart_get)
    app_uart_init                            0x00023189   Thumb Code   200  app_uart_fifo.o(i.app_uart_init)
    app_uart_put                             0x00023271   Thumb Code    50  app_uart_fifo.o(i.app_uart_put)
    app_util_critical_region_enter           0x000232b1   Thumb Code    12  app_util_platform.o(i.app_util_critical_region_enter)
    app_util_critical_region_exit            0x000232bd   Thumb Code    62  app_util_platform.o(i.app_util_critical_region_exit)
    ble_db_discovery_evt_register            0x00023421   Thumb Code    42  ble_db_discovery.o(i.ble_db_discovery_evt_register)
    ble_db_discovery_init                    0x00023455   Thumb Code    40  ble_db_discovery.o(i.ble_db_discovery_init)
    ble_db_discovery_on_ble_evt              0x0002348d   Thumb Code   144  ble_db_discovery.o(i.ble_db_discovery_on_ble_evt)
    ble_db_discovery_start                   0x00023521   Thumb Code    62  ble_db_discovery.o(i.ble_db_discovery_start)
    ble_nus_c_handles_assign                 0x0002390d   Thumb Code    34  ble_nus_c.o(i.ble_nus_c_handles_assign)
    ble_nus_c_init                           0x00023931   Thumb Code    94  ble_nus_c.o(i.ble_nus_c_init)
    ble_nus_c_on_ble_evt                     0x00023995   Thumb Code   102  ble_nus_c.o(i.ble_nus_c_on_ble_evt)
    ble_nus_c_on_db_disc_evt                 0x000239fb   Thumb Code   148  ble_nus_c.o(i.ble_nus_c_on_db_disc_evt)
    ble_nus_c_string_send                    0x00023a91   Thumb Code   100  ble_nus_c.o(i.ble_nus_c_string_send)
    ble_nus_c_tx_notif_enable                0x00023b2d   Thumb Code    44  ble_nus_c.o(i.ble_nus_c_tx_notif_enable)
    bsp_board_button_idx_to_pin              0x00023cb1   Thumb Code     8  boards.o(i.bsp_board_button_idx_to_pin)
    bsp_board_button_state_get               0x00023cbd   Thumb Code    48  boards.o(i.bsp_board_button_state_get)
    bsp_board_led_invert                     0x00023cf1   Thumb Code    50  boards.o(i.bsp_board_led_invert)
    bsp_board_led_off                        0x00023d29   Thumb Code    16  boards.o(i.bsp_board_led_off)
    bsp_board_led_on                         0x00023d3d   Thumb Code    16  boards.o(i.bsp_board_led_on)
    bsp_board_led_state_get                  0x00023d51   Thumb Code    48  boards.o(i.bsp_board_led_state_get)
    bsp_board_leds_init                      0x00023d85   Thumb Code    42  boards.o(i.bsp_board_leds_init)
    bsp_board_leds_off                       0x00023db5   Thumb Code    20  boards.o(i.bsp_board_leds_off)
    bsp_board_leds_on                        0x00023dc9   Thumb Code    20  boards.o(i.bsp_board_leds_on)
    bsp_board_pin_to_button_idx              0x00023ddd   Thumb Code    32  boards.o(i.bsp_board_pin_to_button_idx)
    bsp_btn_ble_init                         0x00023e01   Thumb Code    36  bsp_btn_ble.o(i.bsp_btn_ble_init)
    bsp_btn_ble_sleep_mode_prepare           0x00023e2d   Thumb Code    50  bsp_btn_ble.o(i.bsp_btn_ble_sleep_mode_prepare)
    bsp_button_is_pressed                    0x00023f25   Thumb Code    12  bsp.o(i.bsp_button_is_pressed)
    bsp_event_handler                        0x00023f31   Thumb Code    60  main.o(i.bsp_event_handler)
    bsp_event_to_button_action_assign        0x00023f71   Thumb Code    86  bsp.o(i.bsp_event_to_button_action_assign)
    bsp_indication_set                       0x00023fcd   Thumb Code    28  bsp.o(i.bsp_indication_set)
    bsp_init                                 0x00023fed   Thumb Code   134  bsp.o(i.bsp_init)
    bsp_wakeup_button_enable                 0x00024415   Thumb Code    22  bsp.o(i.bsp_wakeup_button_enable)
    buffer_is_empty                          0x000244dd   Thumb Code    20  nrf_log_frontend.o(i.buffer_is_empty)
    fputc                                    0x00024cb1   Thumb Code    16  retarget.o(i.fputc)
    gatt_evt_handler                         0x00024cc1   Thumb Code    64  main.o(i.gatt_evt_handler)
    gatt_init                                0x00024d4d   Thumb Code    60  main.o(i.gatt_init)
    main                                     0x0002538d   Thumb Code    78  main.o(i.main)
    nrf_balloc_alloc                         0x0002552b   Thumb Code    82  nrf_balloc.o(i.nrf_balloc_alloc)
    nrf_balloc_free                          0x0002558d   Thumb Code    48  nrf_balloc.o(i.nrf_balloc_free)
    nrf_balloc_init                          0x000255c9   Thumb Code    60  nrf_balloc.o(i.nrf_balloc_init)
    nrf_ble_gatt_att_mtu_central_set         0x0002561b   Thumb Code    30  nrf_ble_gatt.o(i.nrf_ble_gatt_att_mtu_central_set)
    nrf_ble_gatt_init                        0x00025639   Thumb Code    52  nrf_ble_gatt.o(i.nrf_ble_gatt_init)
    nrf_ble_gatt_on_ble_evt                  0x0002566d   Thumb Code   190  nrf_ble_gatt.o(i.nrf_ble_gatt_on_ble_evt)
    nrf_drv_clock_init                       0x00025819   Thumb Code    94  nrf_drv_clock.o(i.nrf_drv_clock_init)
    nrf_drv_clock_lfclk_release              0x00025881   Thumb Code    42  nrf_drv_clock.o(i.nrf_drv_clock_lfclk_release)
    nrf_drv_common_irq_enable                0x000258b1   Thumb Code    84  nrf_drv_common.o(i.nrf_drv_common_irq_enable)
    nrf_drv_gpiote_in_event_enable           0x0002591d   Thumb Code   164  nrf_drv_gpiote.o(i.nrf_drv_gpiote_in_event_enable)
    nrf_drv_gpiote_in_init                   0x000259c9   Thumb Code   210  nrf_drv_gpiote.o(i.nrf_drv_gpiote_in_init)
    nrf_drv_gpiote_in_is_set                 0x00025aa9   Thumb Code    20  nrf_drv_gpiote.o(i.nrf_drv_gpiote_in_is_set)
    nrf_drv_gpiote_init                      0x00025abd   Thumb Code    90  nrf_drv_gpiote.o(i.nrf_drv_gpiote_init)
    nrf_drv_gpiote_is_init                   0x00025b1d   Thumb Code    16  nrf_drv_gpiote.o(i.nrf_drv_gpiote_is_init)
    nrf_drv_uart_init                        0x00025b45   Thumb Code   126  nrf_drv_uart.o(i.nrf_drv_uart_init)
    nrf_drv_uart_rx                          0x00025bc9   Thumb Code   208  nrf_drv_uart.o(i.nrf_drv_uart_rx)
    nrf_drv_uart_rx_enable                   0x00025c9d   Thumb Code    46  nrf_drv_uart.o(i.nrf_drv_uart_rx_enable)
    nrf_drv_uart_tx                          0x00025e65   Thumb Code    96  nrf_drv_uart.o(i.nrf_drv_uart_tx)
    nrf_drv_uart_tx_in_progress              0x00025fd1   Thumb Code    22  nrf_drv_uart.o(i.nrf_drv_uart_tx_in_progress)
    nrf_fprintf                              0x00025fed   Thumb Code    42  nrf_fprintf.o(i.nrf_fprintf)
    nrf_fprintf_buffer_flush                 0x00026017   Thumb Code    28  nrf_fprintf.o(i.nrf_fprintf_buffer_flush)
    nrf_fprintf_fmt                          0x00026033   Thumb Code   496  nrf_fprintf_format.o(i.nrf_fprintf_fmt)
    nrf_log_backend_add                      0x000264c1   Thumb Code    68  nrf_log_frontend.o(i.nrf_log_backend_add)
    nrf_log_backend_rtt_init                 0x0002650b   Thumb Code     8  nrf_log_backend_rtt.o(i.nrf_log_backend_rtt_init)
    nrf_log_backend_serial_put               0x00026535   Thumb Code   254  nrf_log_backend_serial.o(i.nrf_log_backend_serial_put)
    nrf_log_color_id_get                     0x00026635   Thumb Code    52  nrf_log_frontend.o(i.nrf_log_color_id_get)
    nrf_log_default_backends_init            0x0002666d   Thumb Code    32  nrf_log_default_backends.o(i.nrf_log_default_backends_init)
    nrf_log_frontend_dequeue                 0x00026691   Thumb Code   696  nrf_log_frontend.o(i.nrf_log_frontend_dequeue)
    nrf_log_frontend_std_0                   0x00026951   Thumb Code    20  nrf_log_frontend.o(i.nrf_log_frontend_std_0)
    nrf_log_frontend_std_1                   0x00026965   Thumb Code    24  nrf_log_frontend.o(i.nrf_log_frontend_std_1)
    nrf_log_frontend_std_2                   0x0002697d   Thumb Code    32  nrf_log_frontend.o(i.nrf_log_frontend_std_2)
    nrf_log_frontend_std_6                   0x0002699d   Thumb Code    60  nrf_log_frontend.o(i.nrf_log_frontend_std_6)
    nrf_log_hexdump_entry_process            0x000269d9   Thumb Code   158  nrf_log_str_formatter.o(i.nrf_log_hexdump_entry_process)
    nrf_log_init                             0x00026a91   Thumb Code    82  nrf_log_frontend.o(i.nrf_log_init)
    nrf_log_module_cnt_get                   0x00026af9   Thumb Code    10  nrf_log_frontend.o(i.nrf_log_module_cnt_get)
    nrf_log_module_name_get                  0x00026b0d   Thumb Code    30  nrf_log_frontend.o(i.nrf_log_module_name_get)
    nrf_log_panic                            0x00026b31   Thumb Code    46  nrf_log_frontend.o(i.nrf_log_panic)
    nrf_log_std_entry_process                0x00026b65   Thumb Code   200  nrf_log_str_formatter.o(i.nrf_log_std_entry_process)
    nrf_memobj_alloc                         0x00026c2d   Thumb Code   122  nrf_memobj.o(i.nrf_memobj_alloc)
    nrf_memobj_free                          0x00026ca7   Thumb Code    64  nrf_memobj.o(i.nrf_memobj_free)
    nrf_memobj_get                           0x00026ce7   Thumb Code    30  nrf_memobj.o(i.nrf_memobj_get)
    nrf_memobj_pool_init                     0x00026d05   Thumb Code    12  nrf_memobj.o(i.nrf_memobj_pool_init)
    nrf_memobj_put                           0x00026d11   Thumb Code    48  nrf_memobj.o(i.nrf_memobj_put)
    nrf_memobj_read                          0x00026d41   Thumb Code    28  nrf_memobj.o(i.nrf_memobj_read)
    nrf_memobj_write                         0x00026d5d   Thumb Code    28  nrf_memobj.o(i.nrf_memobj_write)
    nrf_pwr_mgmt_init                        0x00026d91   Thumb Code    46  nrf_pwr_mgmt.o(i.nrf_pwr_mgmt_init)
    nrf_pwr_mgmt_run                         0x00026dd1   Thumb Code   100  nrf_pwr_mgmt.o(i.nrf_pwr_mgmt_run)
    nrf_pwr_mgmt_shutdown                    0x00026e39   Thumb Code   100  nrf_pwr_mgmt.o(i.nrf_pwr_mgmt_shutdown)
    nrf_sdh_ble_app_ram_start_get            0x00026ea9   Thumb Code    18  nrf_sdh_ble.o(i.nrf_sdh_ble_app_ram_start_get)
    nrf_sdh_ble_default_cfg_set              0x00026ec1   Thumb Code   354  nrf_sdh_ble.o(i.nrf_sdh_ble_default_cfg_set)
    nrf_sdh_ble_enable                       0x00027041   Thumb Code   100  nrf_sdh_ble.o(i.nrf_sdh_ble_enable)
    nrf_sdh_enable_request                   0x00027181   Thumb Code    88  nrf_sdh.o(i.nrf_sdh_enable_request)
    nrf_sdh_evts_poll                        0x000271ed   Thumb Code    44  nrf_sdh.o(i.nrf_sdh_evts_poll)
    nrf_sdh_is_enabled                       0x0002721d   Thumb Code     6  nrf_sdh.o(i.nrf_sdh_is_enabled)
    nrf_section_iter_init                    0x00027283   Thumb Code    20  nrf_section_iter.o(i.nrf_section_iter_init)
    nrf_section_iter_next                    0x000272c5   Thumb Code    46  nrf_section_iter.o(i.nrf_section_iter_next)
    nrf_strerror_find                        0x000272f5   Thumb Code    60  nrf_strerror.o(i.nrf_strerror_find)
    nrf_strerror_get                         0x00027335   Thumb Code    22  nrf_strerror.o(i.nrf_strerror_get)
    uart_event_handle                        0x000285c5   Thumb Code   182  main.o(i.uart_event_handle)
    nrf_log_backend_rtt_api                  0x00028e38   Data          12  nrf_log_backend_rtt.o(.constdata)
    m_ram_start                              0x00028edc   Data           4  nrf_sdh_ble.o(.constdata)
    __ctype_table                            0x00028efc   Data         129  ctype_o.o(.constdata)
    Region$$Table$$Base                      0x00029670   Number         0  anon$$obj.o(Region$$Table)
    Region$$Table$$Limit                     0x00029690   Number         0  anon$$obj.o(Region$$Table)
    log_const_data$$Base                     0x00029690   Number         0  ble_db_discovery.o(log_const_data)
    m_nrf_log_ble_db_disc_logs_data_const    0x00029690   Data           8  ble_db_discovery.o(log_const_data)
    m_nrf_log_ble_gatt_logs_data_const       0x00029698   Data           8  nrf_ble_gatt.o(log_const_data)
    m_nrf_log_ble_nus_logs_data_const        0x000296a0   Data           8  ble_nus_c.o(log_const_data)
    m_nrf_log_clock_logs_data_const          0x000296a8   Data           8  nrf_drv_clock.o(log_const_data)
    m_nrf_log_gpiote_logs_data_const         0x000296b0   Data           8  nrf_drv_gpiote.o(log_const_data)
    m_nrf_log_uart_logs_data_const           0x000296b8   Data           8  nrf_drv_uart.o(log_const_data)
    m_nrf_log_balloc_logs_data_const         0x000296c0   Data           8  nrf_balloc.o(log_const_data)
    m_nrf_log_pwr_mgmt_logs_data_const       0x000296c8   Data           8  nrf_pwr_mgmt.o(log_const_data)
    m_nrf_log_app_logs_data_const            0x000296d0   Data           8  nrf_log_frontend.o(log_const_data)
    m_nrf_log_nrf_sdh_logs_data_const        0x000296d8   Data           8  nrf_sdh.o(log_const_data)
    m_nrf_log_nrf_sdh_ble_logs_data_const    0x000296e0   Data           8  nrf_sdh_ble.o(log_const_data)
    m_nrf_log_nrf_sdh_soc_logs_data_const    0x000296e8   Data           8  nrf_sdh_soc.o(log_const_data)
    log_const_data$$Limit                    0x000296f0   Number         0  nrf_sdh_soc.o(log_const_data)
    pwr_mgmt_data1$$Base                     0x000296f0   Number         0  main.o(pwr_mgmt_data1)
    pwr_mgmt_data1$$Limit                    0x000296f4   Number         0  main.o(pwr_mgmt_data1)
    sdh_ble_observers1$$Base                 0x000296f4   Number         0  main.o(sdh_ble_observers1)
    sdh_ble_observers1$$Limit                0x0002970c   Number         0  bsp_btn_ble.o(sdh_ble_observers1)
    sdh_ble_observers2$$Base                 0x0002970c   Number         0  main.o(sdh_ble_observers2)
    sdh_ble_observers2$$Limit                0x00029714   Number         0  main.o(sdh_ble_observers2)
    sdh_ble_observers3$$Base                 0x00029714   Number         0  main.o(sdh_ble_observers3)
    sdh_ble_observers3$$Limit                0x0002971c   Number         0  main.o(sdh_ble_observers3)
    sdh_soc_observers0$$Base                 0x0002971c   Number         0  nrf_drv_clock.o(sdh_soc_observers0)
    sdh_soc_observers0$$Limit                0x00029724   Number         0  nrf_drv_clock.o(sdh_soc_observers0)
    sdh_stack_observers0$$Base               0x00029724   Number         0  nrf_sdh_ble.o(sdh_stack_observers0)
    sdh_stack_observers0$$Limit              0x00029734   Number         0  nrf_sdh_soc.o(sdh_stack_observers0)
    sdh_state_observers0$$Base               0x00029734   Number         0  nrf_drv_clock.o(sdh_state_observers0)
    sdh_state_observers0$$Limit              0x0002973c   Number         0  nrf_drv_clock.o(sdh_state_observers0)
    Image$$RW_IRAM1$$Base                    0x20002978   Number         0  anon$$obj.o ABSOLUTE
    __stdout                                 0x20002cbc   Data           4  retarget.o(.data)
    __stdin                                  0x20002cc0   Data           4  retarget.o(.data)
    SystemCoreClock                          0x20002d20   Data           4  system_nrf52840.o(.data)
    log_dynamic_data$$Base                   0x20002d24   Number         0  ble_db_discovery.o(log_dynamic_data)
    m_nrf_log_ble_db_disc_logs_data_dynamic  0x20002d24   Data          12  ble_db_discovery.o(log_dynamic_data)
    m_nrf_log_ble_gatt_logs_data_dynamic     0x20002d30   Data          12  nrf_ble_gatt.o(log_dynamic_data)
    m_nrf_log_ble_nus_logs_data_dynamic      0x20002d3c   Data          12  ble_nus_c.o(log_dynamic_data)
    m_nrf_log_clock_logs_data_dynamic        0x20002d48   Data          12  nrf_drv_clock.o(log_dynamic_data)
    m_nrf_log_gpiote_logs_data_dynamic       0x20002d54   Data          12  nrf_drv_gpiote.o(log_dynamic_data)
    m_nrf_log_uart_logs_data_dynamic         0x20002d60   Data          12  nrf_drv_uart.o(log_dynamic_data)
    m_nrf_log_balloc_logs_data_dynamic       0x20002d6c   Data          12  nrf_balloc.o(log_dynamic_data)
    m_nrf_log_pwr_mgmt_logs_data_dynamic     0x20002d78   Data          12  nrf_pwr_mgmt.o(log_dynamic_data)
    m_nrf_log_app_logs_data_dynamic          0x20002d84   Data          12  nrf_log_frontend.o(log_dynamic_data)
    m_nrf_log_nrf_sdh_logs_data_dynamic      0x20002d90   Data          12  nrf_sdh.o(log_dynamic_data)
    m_nrf_log_nrf_sdh_ble_logs_data_dynamic  0x20002d9c   Data          12  nrf_sdh_ble.o(log_dynamic_data)
    m_nrf_log_nrf_sdh_soc_logs_data_dynamic  0x20002da8   Data          12  nrf_sdh_soc.o(log_dynamic_data)
    nrf_nvic_state                           0x20003638   Data          12  app_util_platform.o(.bss)
    _SEGGER_RTT                              0x20003b70   Data         120  segger_rtt.o(.bss)
    __initial_sp                             0x20005df8   Data           0  arm_startup_nrf52840.o(STACK)



==============================================================================

Memory Map of the image

  Image Entry point : 0x00022201

  Load Region LR_IROM1 (Base: 0x00022000, Size: 0x00007b78, Max: 0x000de000, ABSOLUTE, COMPRESSED[0x00007784])

    Execution Region ER_IROM1 (Base: 0x00022000, Size: 0x0000773c, Max: 0x000de000, ABSOLUTE)

    Base Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x00022000   0x00000200   Data   RO         4136    RESET               arm_startup_nrf52840.o
    0x00022200   0x00000000   Code   RO         4212  * .ARM.Collect$$$$00000000  mc_w.l(entry.o)
    0x00022200   0x00000004   Code   RO         4515    .ARM.Collect$$$$00000001  mc_w.l(entry2.o)
    0x00022204   0x00000004   Code   RO         4518    .ARM.Collect$$$$00000004  mc_w.l(entry5.o)
    0x00022208   0x00000000   Code   RO         4520    .ARM.Collect$$$$00000008  mc_w.l(entry7b.o)
    0x00022208   0x00000000   Code   RO         4522    .ARM.Collect$$$$0000000A  mc_w.l(entry8b.o)
    0x00022208   0x00000008   Code   RO         4523    .ARM.Collect$$$$0000000B  mc_w.l(entry9a.o)
    0x00022210   0x00000000   Code   RO         4525    .ARM.Collect$$$$0000000D  mc_w.l(entry10a.o)
    0x00022210   0x00000000   Code   RO         4527    .ARM.Collect$$$$0000000F  mc_w.l(entry11a.o)
    0x00022210   0x00000004   Code   RO         4516    .ARM.Collect$$$$00002712  mc_w.l(entry2.o)
    0x00022214   0x0000009a   Code   RO         3009    .emb_text           nrf_memobj.o
    0x000222ae   0x00000002   PAD
    0x000222b0   0x0000009a   Code   RO         3097    .emb_text           nrf_pwr_mgmt.o
    0x0002234a   0x00000002   PAD
    0x0002234c   0x0000009a   Code   RO         3417    .emb_text           nrf_log_frontend.o
    0x000223e6   0x00000002   PAD
    0x000223e8   0x00000024   Code   RO         4137    .text               arm_startup_nrf52840.o
    0x0002240c   0x00000062   Code   RO         4215    .text               mc_w.l(uldiv.o)
    0x0002246e   0x00000002   PAD
    0x00022470   0x00000008   Code   RO         4217    .text               mc_w.l(ctype_o.o)
    0x00022478   0x00000024   Code   RO         4245    .text               mc_w.l(memcpya.o)
    0x0002249c   0x00000024   Code   RO         4247    .text               mc_w.l(memseta.o)
    0x000224c0   0x0000000e   Code   RO         4249    .text               mc_w.l(strlen.o)
    0x000224ce   0x00000012   Code   RO         4251    .text               mc_w.l(strcpy.o)
    0x000224e0   0x0000001e   Code   RO         4531    .text               mc_w.l(llshl.o)
    0x000224fe   0x00000020   Code   RO         4533    .text               mc_w.l(llushr.o)
    0x0002251e   0x00000002   PAD
    0x00022520   0x00000024   Code   RO         4546    .text               mc_w.l(init.o)
    0x00022544   0x00000056   Code   RO         4560    .text               mc_w.l(__dczerorl2.o)
    0x0002259a   0x00000002   PAD
    0x0002259c   0x00000240   Code   RO         1486    i.GPIOTE_IRQHandler  nrf_drv_gpiote.o
    0x000227dc   0x00000018   Code   RO         2376    i.NVIC_ClearPendingIRQ  app_timer.o
    0x000227f4   0x00000016   Code   RO         2377    i.NVIC_EnableIRQ    app_timer.o
    0x0002280a   0x00000002   PAD
    0x0002280c   0x00000018   Code   RO         2378    i.NVIC_SetPendingIRQ  app_timer.o
    0x00022824   0x00000028   Code   RO         2379    i.NVIC_SetPriority  app_timer.o
    0x0002284c   0x00000050   Code   RO         1248    i.POWER_CLOCK_IRQHandler  nrf_drv_clock.o
    0x0002289c   0x00000034   Code   RO         2380    i.RTC1_IRQHandler   app_timer.o
    0x000228d0   0x00000008   Code   RO         3676    i.SEGGER_RTT_Init   segger_rtt.o
    0x000228d8   0x00000084   Code   RO         3690    i.SEGGER_RTT_WriteNoLock  segger_rtt.o
    0x0002295c   0x00000008   Code   RO         2381    i.SWI0_EGU0_IRQHandler  app_timer.o
    0x00022964   0x00000008   Code   RO         3925    i.SWI2_EGU2_IRQHandler  nrf_sdh.o
    0x0002296c   0x00000010   Code   RO         4144    i.SystemCoreClockUpdate  system_nrf52840.o
    0x0002297c   0x00000230   Code   RO         4145    i.SystemInit        system_nrf52840.o
    0x00022bac   0x00000024   Code   RO         1785    i.UARTE0_UART0_IRQHandler  nrf_drv_uart.o
    0x00022bd0   0x00000070   Code   RO         3694    i._DoInit           segger_rtt.o
    0x00022c40   0x0000001c   Code   RO         3695    i._GetAvailWriteSpace  segger_rtt.o
    0x00022c5c   0x00000072   Code   RO         3697    i._WriteBlocking    segger_rtt.o
    0x00022cce   0x0000004c   Code   RO         3698    i._WriteNoCheck     segger_rtt.o
    0x00022d1a   0x00000002   PAD
    0x00022d1c   0x00000010   Code   RO         4256    i.__0printf$bare    mc_w.l(printfb.o)
    0x00022d2c   0x0000000e   Code   RO         4554    i.__scatterload_copy  mc_w.l(handlers.o)
    0x00022d3a   0x00000002   Code   RO         4555    i.__scatterload_null  mc_w.l(handlers.o)
    0x00022d3c   0x0000000e   Code   RO         4556    i.__scatterload_zeroinit  mc_w.l(handlers.o)
    0x00022d4a   0x00000002   PAD
    0x00022d4c   0x00000038   Code   RO         3926    i.__sd_nvic_app_accessible_irq  nrf_sdh.o
    0x00022d84   0x0000000c   Code   RO         2671    i.__sd_nvic_irq_disable  app_util_platform.o
    0x00022d90   0x00000022   Code   RO         4263    i._printf_core      mc_w.l(printfb.o)
    0x00022db2   0x00000054   Code   RO          608    i.advertising_buttons_configure  bsp_btn_ble.o
    0x00022e06   0x0000000c   Code   RO          491    i.alert_timer_handler  bsp.o
    0x00022e12   0x00000002   PAD
    0x00022e14   0x0000002c   Code   RO         2102    i.app_button_enable  app_button.o
    0x00022e40   0x000000a8   Code   RO         2103    i.app_button_init   app_button.o
    0x00022ee8   0x000000b0   Code   RO         2203    i.app_error_fault_handler  app_error_weak.o
    0x00022f98   0x0000001c   Code   RO         2164    i.app_error_handler_bare  app_error.o
    0x00022fb4   0x0000001e   Code   RO         2238    i.app_fifo_get      app_fifo.o
    0x00022fd2   0x00000024   Code   RO         2239    i.app_fifo_init     app_fifo.o
    0x00022ff6   0x00000022   Code   RO         2241    i.app_fifo_put      app_fifo.o
    0x00023018   0x0000003c   Code   RO         2384    i.app_timer_create  app_timer.o
    0x00023054   0x0000005c   Code   RO         2385    i.app_timer_init    app_timer.o
    0x000230b0   0x00000054   Code   RO         2388    i.app_timer_start   app_timer.o
    0x00023104   0x00000030   Code   RO         2389    i.app_timer_stop    app_timer.o
    0x00023134   0x00000054   Code   RO         2602    i.app_uart_get      app_uart_fifo.o
    0x00023188   0x000000e8   Code   RO         2603    i.app_uart_init     app_uart_fifo.o
    0x00023270   0x00000040   Code   RO         2604    i.app_uart_put      app_uart_fifo.o
    0x000232b0   0x0000000c   Code   RO         2672    i.app_util_critical_region_enter  app_util_platform.o
    0x000232bc   0x00000048   Code   RO         2673    i.app_util_critical_region_exit  app_util_platform.o
    0x00023304   0x000000e4   Code   RO         1786    i.apply_config      nrf_drv_uart.o
    0x000233e8   0x00000038   Code   RO         3418    i.backend_id_assign  nrf_log_frontend.o
    0x00023420   0x00000034   Code   RO          817    i.ble_db_discovery_evt_register  ble_db_discovery.o
    0x00023454   0x00000038   Code   RO          818    i.ble_db_discovery_init  ble_db_discovery.o
    0x0002348c   0x00000094   Code   RO          819    i.ble_db_discovery_on_ble_evt  ble_db_discovery.o
    0x00023520   0x00000048   Code   RO          820    i.ble_db_discovery_start  ble_db_discovery.o
    0x00023568   0x0000023c   Code   RO            5    i.ble_evt_handler   main.o
    0x000237a4   0x00000078   Code   RO          609    i.ble_evt_handler   bsp_btn_ble.o
    0x0002381c   0x000000f0   Code   RO            6    i.ble_nus_c_evt_handler  main.o
    0x0002390c   0x00000022   Code   RO         1156    i.ble_nus_c_handles_assign  ble_nus_c.o
    0x0002392e   0x00000002   PAD
    0x00023930   0x00000064   Code   RO         1157    i.ble_nus_c_init    ble_nus_c.o
    0x00023994   0x00000066   Code   RO         1158    i.ble_nus_c_on_ble_evt  ble_nus_c.o
    0x000239fa   0x00000094   Code   RO         1159    i.ble_nus_c_on_db_disc_evt  ble_nus_c.o
    0x00023a8e   0x00000002   PAD
    0x00023a90   0x0000009c   Code   RO         1160    i.ble_nus_c_string_send  ble_nus_c.o
    0x00023b2c   0x0000002c   Code   RO         1161    i.ble_nus_c_tx_notif_enable  ble_nus_c.o
    0x00023b58   0x00000100   Code   RO            7    i.ble_nus_chars_received_uart_print  main.o
    0x00023c58   0x00000056   Code   RO            8    i.ble_stack_init    main.o
    0x00023cae   0x00000002   PAD
    0x00023cb0   0x0000000c   Code   RO          372    i.bsp_board_button_idx_to_pin  boards.o
    0x00023cbc   0x00000034   Code   RO          373    i.bsp_board_button_state_get  boards.o
    0x00023cf0   0x00000038   Code   RO          376    i.bsp_board_led_invert  boards.o
    0x00023d28   0x00000014   Code   RO          377    i.bsp_board_led_off  boards.o
    0x00023d3c   0x00000014   Code   RO          378    i.bsp_board_led_on  boards.o
    0x00023d50   0x00000034   Code   RO          379    i.bsp_board_led_state_get  boards.o
    0x00023d84   0x00000030   Code   RO          380    i.bsp_board_leds_init  boards.o
    0x00023db4   0x00000014   Code   RO          381    i.bsp_board_leds_off  boards.o
    0x00023dc8   0x00000014   Code   RO          382    i.bsp_board_leds_on  boards.o
    0x00023ddc   0x00000024   Code   RO          383    i.bsp_board_pin_to_button_idx  boards.o
    0x00023e00   0x0000002c   Code   RO          610    i.bsp_btn_ble_init  bsp_btn_ble.o
    0x00023e2c   0x00000032   Code   RO          611    i.bsp_btn_ble_sleep_mode_prepare  bsp_btn_ble.o
    0x00023e5e   0x00000002   PAD
    0x00023e60   0x000000c4   Code   RO          492    i.bsp_button_event_handler  bsp.o
    0x00023f24   0x0000000c   Code   RO          493    i.bsp_button_is_pressed  bsp.o
    0x00023f30   0x00000040   Code   RO            9    i.bsp_event_handler  main.o
    0x00023f70   0x0000005c   Code   RO          496    i.bsp_event_to_button_action_assign  bsp.o
    0x00023fcc   0x00000020   Code   RO          497    i.bsp_indication_set  bsp.o
    0x00023fec   0x000000ac   Code   RO          498    i.bsp_init          bsp.o
    0x00024098   0x0000037c   Code   RO          499    i.bsp_led_indication  bsp.o
    0x00024414   0x00000016   Code   RO          501    i.bsp_wakeup_button_enable  bsp.o
    0x0002442a   0x00000002   PAD
    0x0002442c   0x00000090   Code   RO         3419    i.buf_prealloc      nrf_log_frontend.o
    0x000244bc   0x00000020   Code   RO         2964    i.buffer_add        nrf_fprintf_format.o
    0x000244dc   0x00000018   Code   RO         3420    i.buffer_is_empty   nrf_log_frontend.o
    0x000244f4   0x0000000e   Code   RO          502    i.button_timer_handler  bsp.o
    0x00024502   0x00000002   PAD
    0x00024504   0x00000040   Code   RO           10    i.buttons_leds_init  main.o
    0x00024544   0x00000030   Code   RO         1162    i.cccd_configure    ble_nus_c.o
    0x00024574   0x00000020   Code   RO         1487    i.channel_free      nrf_drv_gpiote.o
    0x00024594   0x00000010   Code   RO         1488    i.channel_handler_get  nrf_drv_gpiote.o
    0x000245a4   0x00000080   Code   RO         1489    i.channel_port_alloc  nrf_drv_gpiote.o
    0x00024624   0x0000000c   Code   RO         1490    i.channel_port_get  nrf_drv_gpiote.o
    0x00024630   0x00000060   Code   RO          821    i.characteristics_discover  ble_db_discovery.o
    0x00024690   0x00000030   Code   RO         1249    i.clock_clk_started_notify  nrf_drv_clock.o
    0x000246c0   0x00000090   Code   RO         2391    i.compare_reg_update  app_timer.o
    0x00024750   0x00000054   Code   RO          612    i.connection_buttons_configure  bsp_btn_ble.o
    0x000247a4   0x00000050   Code   RO         1037    i.data_length_update  nrf_ble_gatt.o
    0x000247f4   0x00000014   Code   RO           11    i.db_disc_handler   main.o
    0x00024808   0x00000024   Code   RO           12    i.db_discovery_init  main.o
    0x0002482c   0x000000b6   Code   RO          822    i.descriptors_discover  ble_db_discovery.o
    0x000248e2   0x00000002   PAD
    0x000248e4   0x0000008c   Code   RO         2105    i.detection_delay_timeout_handler  app_button.o
    0x00024970   0x000000a4   Code   RO          823    i.discovery_complete_evt_trigger  ble_db_discovery.o
    0x00024a14   0x00000048   Code   RO          824    i.discovery_error_evt_trigger  ble_db_discovery.o
    0x00024a5c   0x00000084   Code   RO          825    i.discovery_start   ble_db_discovery.o
    0x00024ae0   0x00000064   Code   RO         2392    i.elapsed_ticks_acquire  app_timer.o
    0x00024b44   0x0000001c   Code   RO         4146    i.errata_103        system_nrf52840.o
    0x00024b60   0x0000001c   Code   RO         4147    i.errata_115        system_nrf52840.o
    0x00024b7c   0x0000001c   Code   RO         4148    i.errata_120        system_nrf52840.o
    0x00024b98   0x0000001c   Code   RO         4149    i.errata_136        system_nrf52840.o
    0x00024bb4   0x0000001c   Code   RO         4150    i.errata_36         system_nrf52840.o
    0x00024bd0   0x0000001c   Code   RO         4151    i.errata_66         system_nrf52840.o
    0x00024bec   0x0000001c   Code   RO         4152    i.errata_98         system_nrf52840.o
    0x00024c08   0x00000058   Code   RO         2393    i.expired_timers_handler  app_timer.o
    0x00024c60   0x00000018   Code   RO         2244    i.fifo_get          app_fifo.o
    0x00024c78   0x0000000a   Code   RO         2245    i.fifo_length       app_fifo.o
    0x00024c82   0x0000000a   Code   RO         2605    i.fifo_length       app_uart_fifo.o
    0x00024c8c   0x00000012   Code   RO         2246    i.fifo_peek         app_fifo.o
    0x00024c9e   0x00000012   Code   RO         2247    i.fifo_put          app_fifo.o
    0x00024cb0   0x00000010   Code   RO         3250    i.fputc             retarget.o
    0x00024cc0   0x0000008c   Code   RO           13    i.gatt_evt_handler  main.o
    0x00024d4c   0x00000044   Code   RO           14    i.gatt_init         main.o
    0x00024d90   0x00000080   Code   RO         2106    i.gpiote_event_handler  app_button.o
    0x00024e10   0x000000be   Code   RO         2965    i.int_print         nrf_fprintf_format.o
    0x00024ece   0x00000002   PAD
    0x00024ed0   0x0000008c   Code   RO         1787    i.interrupts_enable  nrf_drv_uart.o
    0x00024f5c   0x00000024   Code   RO          826    i.is_char_discovery_reqd  ble_db_discovery.o
    0x00024f80   0x0000005e   Code   RO          827    i.is_desc_discovery_reqd  ble_db_discovery.o
    0x00024fde   0x000000fa   Code   RO           15    i.is_uuid_present   main.o
    0x000250d8   0x0000000c   Code   RO         1252    i.item_dequeue      nrf_drv_clock.o
    0x000250e4   0x00000028   Code   RO          503    i.leds_off          bsp.o
    0x0002510c   0x00000020   Code   RO          504    i.leds_timer_handler  bsp.o
    0x0002512c   0x0000001c   Code   RO         1255    i.lfclk_stop        nrf_drv_clock.o
    0x00025148   0x00000018   Code   RO         1038    i.link_init         nrf_ble_gatt.o
    0x00025160   0x0000013c   Code   RO         2394    i.list_insertions_handler  app_timer.o
    0x0002529c   0x00000022   Code   RO           16    i.log_init          main.o
    0x000252be   0x00000002   PAD
    0x000252c0   0x000000cc   Code   RO         3423    i.log_skip          nrf_log_frontend.o
    0x0002538c   0x0000009c   Code   RO           17    i.main              main.o
    0x00025428   0x000000ae   Code   RO         3010    i.memobj_op         nrf_memobj.o
    0x000254d6   0x00000002   PAD
    0x000254d8   0x0000003c   Code   RO         3424    i.module_idx_get    nrf_log_frontend.o
    0x00025514   0x00000016   Code   RO         3425    i.nrf_atomic_flag_set  nrf_log_frontend.o
    0x0002552a   0x00000052   Code   RO         2870    i.nrf_balloc_alloc  nrf_balloc.o
    0x0002557c   0x00000010   Code   RO         2871    i.nrf_balloc_block2idx  nrf_balloc.o
    0x0002558c   0x00000030   Code   RO         2872    i.nrf_balloc_free   nrf_balloc.o
    0x000255bc   0x0000000c   Code   RO         2873    i.nrf_balloc_idx2block  nrf_balloc.o
    0x000255c8   0x0000003c   Code   RO         2874    i.nrf_balloc_init   nrf_balloc.o
    0x00025604   0x00000016   Code   RO         1491    i.nrf_bitmask_bit_is_set  nrf_drv_gpiote.o
    0x0002561a   0x0000001e   Code   RO         1039    i.nrf_ble_gatt_att_mtu_central_set  nrf_ble_gatt.o
    0x00025638   0x00000034   Code   RO         1044    i.nrf_ble_gatt_init  nrf_ble_gatt.o
    0x0002566c   0x000000c8   Code   RO         1045    i.nrf_ble_gatt_on_ble_evt  nrf_ble_gatt.o
    0x00025734   0x00000012   Code   RO         1256    i.nrf_clock_event_check  nrf_drv_clock.o
    0x00025746   0x00000012   Code   RO         1257    i.nrf_clock_event_clear  nrf_drv_clock.o
    0x00025758   0x0000000c   Code   RO         1259    i.nrf_clock_int_disable  nrf_drv_clock.o
    0x00025764   0x00000010   Code   RO         1261    i.nrf_clock_lf_is_running  nrf_drv_clock.o
    0x00025774   0x00000008   Code   RO         1262    i.nrf_clock_task_trigger  nrf_drv_clock.o
    0x0002577c   0x0000009c   Code   RO         2395    i.nrf_delay_us      app_timer.o
    0x00025818   0x00000068   Code   RO         1268    i.nrf_drv_clock_init  nrf_drv_clock.o
    0x00025880   0x00000030   Code   RO         1272    i.nrf_drv_clock_lfclk_release  nrf_drv_clock.o
    0x000258b0   0x00000060   Code   RO         1450    i.nrf_drv_common_irq_enable  nrf_drv_common.o
    0x00025910   0x0000000a   Code   RO         1789    i.nrf_drv_get_IRQn  nrf_drv_uart.o
    0x0002591a   0x00000002   PAD
    0x0002591c   0x000000ac   Code   RO         1496    i.nrf_drv_gpiote_in_event_enable  nrf_drv_gpiote.o
    0x000259c8   0x000000e0   Code   RO         1497    i.nrf_drv_gpiote_in_init  nrf_drv_gpiote.o
    0x00025aa8   0x00000014   Code   RO         1498    i.nrf_drv_gpiote_in_is_set  nrf_drv_gpiote.o
    0x00025abc   0x00000060   Code   RO         1500    i.nrf_drv_gpiote_init  nrf_drv_gpiote.o
    0x00025b1c   0x00000014   Code   RO         1501    i.nrf_drv_gpiote_is_init  nrf_drv_gpiote.o
    0x00025b30   0x00000014   Code   RO         1790    i.nrf_drv_is_in_RAM  nrf_drv_uart.o
    0x00025b44   0x00000084   Code   RO         1792    i.nrf_drv_uart_init  nrf_drv_uart.o
    0x00025bc8   0x000000d4   Code   RO         1793    i.nrf_drv_uart_rx   nrf_drv_uart.o
    0x00025c9c   0x00000034   Code   RO         1796    i.nrf_drv_uart_rx_enable  nrf_drv_uart.o
    0x00025cd0   0x000000cc   Code   RO         1797    i.nrf_drv_uart_rx_for_uart  nrf_drv_uart.o
    0x00025d9c   0x000000c8   Code   RO         1798    i.nrf_drv_uart_rx_for_uarte  nrf_drv_uart.o
    0x00025e64   0x00000064   Code   RO         1800    i.nrf_drv_uart_tx   nrf_drv_uart.o
    0x00025ec8   0x0000008c   Code   RO         1802    i.nrf_drv_uart_tx_for_uart  nrf_drv_uart.o
    0x00025f54   0x0000007c   Code   RO         1803    i.nrf_drv_uart_tx_for_uarte  nrf_drv_uart.o
    0x00025fd0   0x0000001c   Code   RO         1804    i.nrf_drv_uart_tx_in_progress  nrf_drv_uart.o
    0x00025fec   0x0000002a   Code   RO         2921    i.nrf_fprintf       nrf_fprintf.o
    0x00026016   0x0000001c   Code   RO         2922    i.nrf_fprintf_buffer_flush  nrf_fprintf.o
    0x00026032   0x000001f0   Code   RO         2966    i.nrf_fprintf_fmt   nrf_fprintf_format.o
    0x00026222   0x00000034   Code   RO          385    i.nrf_gpio_cfg      boards.o
    0x00026256   0x00000034   Code   RO         1515    i.nrf_gpio_cfg      nrf_drv_gpiote.o
    0x0002628a   0x00000034   Code   RO         1806    i.nrf_gpio_cfg      nrf_drv_uart.o
    0x000262be   0x0000001a   Code   RO         1808    i.nrf_gpio_cfg_input  nrf_drv_uart.o
    0x000262d8   0x00000018   Code   RO         1809    i.nrf_gpio_cfg_output  nrf_drv_uart.o
    0x000262f0   0x00000044   Code   RO          505    i.nrf_gpio_cfg_sense_set  bsp.o
    0x00026334   0x0000003a   Code   RO         1517    i.nrf_gpio_cfg_sense_set  nrf_drv_gpiote.o
    0x0002636e   0x00000002   PAD
    0x00026370   0x00000020   Code   RO          386    i.nrf_gpio_pin_port_decode  boards.o
    0x00026390   0x00000020   Code   RO         1519    i.nrf_gpio_pin_port_decode  nrf_drv_gpiote.o
    0x000263b0   0x00000020   Code   RO         1810    i.nrf_gpio_pin_port_decode  nrf_drv_uart.o
    0x000263d0   0x0000001a   Code   RO         1520    i.nrf_gpio_pin_read  nrf_drv_gpiote.o
    0x000263ea   0x0000001a   Code   RO         1811    i.nrf_gpio_pin_set  nrf_drv_uart.o
    0x00026404   0x00000042   Code   RO          387    i.nrf_gpio_pin_write  boards.o
    0x00026446   0x00000002   PAD
    0x00026448   0x0000002c   Code   RO         1522    i.nrf_gpio_ports_read  nrf_drv_gpiote.o
    0x00026474   0x0000000c   Code   RO         1523    i.nrf_gpiote_event_addr_get  nrf_drv_gpiote.o
    0x00026480   0x0000001c   Code   RO         1524    i.nrf_gpiote_event_clear  nrf_drv_gpiote.o
    0x0002649c   0x00000016   Code   RO         1525    i.nrf_gpiote_event_is_set  nrf_drv_gpiote.o
    0x000264b2   0x00000002   PAD
    0x000264b4   0x0000000c   Code   RO         1526    i.nrf_gpiote_int_enable  nrf_drv_gpiote.o
    0x000264c0   0x00000048   Code   RO         3426    i.nrf_log_backend_add  nrf_log_frontend.o
    0x00026508   0x00000002   Code   RO         3286    i.nrf_log_backend_rtt_flush  nrf_log_backend_rtt.o
    0x0002650a   0x00000008   Code   RO         3287    i.nrf_log_backend_rtt_init  nrf_log_backend_rtt.o
    0x00026512   0x00000002   Code   RO         3288    i.nrf_log_backend_rtt_panic_set  nrf_log_backend_rtt.o
    0x00026514   0x00000020   Code   RO         3289    i.nrf_log_backend_rtt_put  nrf_log_backend_rtt.o
    0x00026534   0x000000fe   Code   RO         3350    i.nrf_log_backend_serial_put  nrf_log_backend_serial.o
    0x00026632   0x00000002   PAD
    0x00026634   0x00000038   Code   RO         3428    i.nrf_log_color_id_get  nrf_log_frontend.o
    0x0002666c   0x00000024   Code   RO         3384    i.nrf_log_default_backends_init  nrf_log_default_backends.o
    0x00026690   0x000002c0   Code   RO         3429    i.nrf_log_frontend_dequeue  nrf_log_frontend.o
    0x00026950   0x00000014   Code   RO         3431    i.nrf_log_frontend_std_0  nrf_log_frontend.o
    0x00026964   0x00000018   Code   RO         3432    i.nrf_log_frontend_std_1  nrf_log_frontend.o
    0x0002697c   0x00000020   Code   RO         3433    i.nrf_log_frontend_std_2  nrf_log_frontend.o
    0x0002699c   0x0000003c   Code   RO         3437    i.nrf_log_frontend_std_6  nrf_log_frontend.o
    0x000269d8   0x000000b8   Code   RO         3623    i.nrf_log_hexdump_entry_process  nrf_log_str_formatter.o
    0x00026a90   0x00000068   Code   RO         3438    i.nrf_log_init      nrf_log_frontend.o
    0x00026af8   0x00000014   Code   RO         3439    i.nrf_log_module_cnt_get  nrf_log_frontend.o
    0x00026b0c   0x00000024   Code   RO         3442    i.nrf_log_module_name_get  nrf_log_frontend.o
    0x00026b30   0x00000034   Code   RO         3443    i.nrf_log_panic     nrf_log_frontend.o
    0x00026b64   0x000000c8   Code   RO         3624    i.nrf_log_std_entry_process  nrf_log_str_formatter.o
    0x00026c2c   0x0000007a   Code   RO         3011    i.nrf_memobj_alloc  nrf_memobj.o
    0x00026ca6   0x00000040   Code   RO         3012    i.nrf_memobj_free   nrf_memobj.o
    0x00026ce6   0x0000001e   Code   RO         3013    i.nrf_memobj_get    nrf_memobj.o
    0x00026d04   0x0000000c   Code   RO         3014    i.nrf_memobj_pool_init  nrf_memobj.o
    0x00026d10   0x00000030   Code   RO         3015    i.nrf_memobj_put    nrf_memobj.o
    0x00026d40   0x0000001c   Code   RO         3016    i.nrf_memobj_read   nrf_memobj.o
    0x00026d5c   0x0000001c   Code   RO         3017    i.nrf_memobj_write  nrf_memobj.o
    0x00026d78   0x00000016   Code   RO         3098    i.nrf_mtx_unlock    nrf_pwr_mgmt.o
    0x00026d8e   0x00000002   PAD
    0x00026d90   0x00000040   Code   RO         3100    i.nrf_pwr_mgmt_init  nrf_pwr_mgmt.o
    0x00026dd0   0x00000068   Code   RO         3101    i.nrf_pwr_mgmt_run  nrf_pwr_mgmt.o
    0x00026e38   0x00000070   Code   RO         3102    i.nrf_pwr_mgmt_shutdown  nrf_pwr_mgmt.o
    0x00026ea8   0x00000018   Code   RO         4051    i.nrf_sdh_ble_app_ram_start_get  nrf_sdh_ble.o
    0x00026ec0   0x00000180   Code   RO         4052    i.nrf_sdh_ble_default_cfg_set  nrf_sdh_ble.o
    0x00027040   0x000000dc   Code   RO         4053    i.nrf_sdh_ble_enable  nrf_sdh_ble.o
    0x0002711c   0x00000064   Code   RO         4054    i.nrf_sdh_ble_evts_poll  nrf_sdh_ble.o
    0x00027180   0x0000006c   Code   RO         3928    i.nrf_sdh_enable_request  nrf_sdh.o
    0x000271ec   0x00000030   Code   RO         3929    i.nrf_sdh_evts_poll  nrf_sdh.o
    0x0002721c   0x0000000c   Code   RO         3930    i.nrf_sdh_is_enabled  nrf_sdh.o
    0x00027228   0x00000054   Code   RO         4106    i.nrf_sdh_soc_evts_poll  nrf_sdh_soc.o
    0x0002727c   0x00000006   Code   RO         3935    i.nrf_section_iter_get  nrf_sdh.o
    0x00027282   0x00000014   Code   RO         3181    i.nrf_section_iter_init  nrf_section_iter.o
    0x00027296   0x0000002e   Code   RO         3182    i.nrf_section_iter_item_set  nrf_section_iter.o
    0x000272c4   0x0000002e   Code   RO         3183    i.nrf_section_iter_next  nrf_section_iter.o
    0x000272f2   0x00000002   PAD
    0x000272f4   0x00000040   Code   RO         3216    i.nrf_strerror_find  nrf_strerror.o
    0x00027334   0x0000001c   Code   RO         3217    i.nrf_strerror_get  nrf_strerror.o
    0x00027350   0x0000000c   Code   RO         1812    i.nrf_uart_errorsrc_get_and_clear  nrf_drv_uart.o
    0x0002735c   0x0000000e   Code   RO         1813    i.nrf_uart_event_check  nrf_drv_uart.o
    0x0002736a   0x0000000e   Code   RO         1814    i.nrf_uart_event_clear  nrf_drv_uart.o
    0x00027378   0x0000000c   Code   RO         1815    i.nrf_uart_hwfc_pins_set  nrf_drv_uart.o
    0x00027384   0x00000006   Code   RO         1816    i.nrf_uart_int_disable  nrf_drv_uart.o
    0x0002738a   0x00000006   Code   RO         1817    i.nrf_uart_int_enable  nrf_drv_uart.o
    0x00027390   0x00000012   Code   RO         1818    i.nrf_uart_int_enable_check  nrf_drv_uart.o
    0x000273a2   0x00000006   Code   RO         1819    i.nrf_uart_task_trigger  nrf_drv_uart.o
    0x000273a8   0x0000000e   Code   RO         1820    i.nrf_uart_txrx_pins_set  nrf_drv_uart.o
    0x000273b6   0x0000000c   Code   RO         1821    i.nrf_uarte_errorsrc_get_and_clear  nrf_drv_uart.o
    0x000273c2   0x0000000e   Code   RO         1822    i.nrf_uarte_event_check  nrf_drv_uart.o
    0x000273d0   0x0000000e   Code   RO         1823    i.nrf_uarte_event_clear  nrf_drv_uart.o
    0x000273de   0x0000000c   Code   RO         1824    i.nrf_uarte_hwfc_pins_set  nrf_drv_uart.o
    0x000273ea   0x00000006   Code   RO         1825    i.nrf_uarte_int_disable  nrf_drv_uart.o
    0x000273f0   0x00000006   Code   RO         1826    i.nrf_uarte_int_enable  nrf_drv_uart.o
    0x000273f6   0x0000000a   Code   RO         1827    i.nrf_uarte_rx_amount_get  nrf_drv_uart.o
    0x00027400   0x00000006   Code   RO         1828    i.nrf_uarte_task_trigger  nrf_drv_uart.o
    0x00027406   0x0000000e   Code   RO         1829    i.nrf_uarte_txrx_pins_set  nrf_drv_uart.o
    0x00027414   0x0000002c   Code   RO           18    i.nus_c_init        main.o
    0x00027440   0x00000180   Code   RO          828    i.on_characteristic_discovery_rsp  ble_db_discovery.o
    0x000275c0   0x00000084   Code   RO         1046    i.on_connected_evt  nrf_ble_gatt.o
    0x00027644   0x00000054   Code   RO         1047    i.on_data_length_update_evt  nrf_ble_gatt.o
    0x00027698   0x00000060   Code   RO         1048    i.on_data_length_update_request_evt  nrf_ble_gatt.o
    0x000276f8   0x00000130   Code   RO          829    i.on_descriptor_discovery_rsp  ble_db_discovery.o
    0x00027828   0x0000001e   Code   RO          830    i.on_disconnected   ble_db_discovery.o
    0x00027846   0x00000014   Code   RO         1049    i.on_disconnected_evt  nrf_ble_gatt.o
    0x0002785a   0x00000002   PAD
    0x0002785c   0x0000008c   Code   RO         1050    i.on_exchange_mtu_request_evt  nrf_ble_gatt.o
    0x000278e8   0x00000064   Code   RO         1051    i.on_exchange_mtu_rsp_evt  nrf_ble_gatt.o
    0x0002794c   0x00000038   Code   RO         1163    i.on_hvx            ble_nus_c.o
    0x00027984   0x00000080   Code   RO          831    i.on_primary_srv_discovery_rsp  ble_db_discovery.o
    0x00027a04   0x0000009c   Code   RO          832    i.on_srv_disc_completion  ble_db_discovery.o
    0x00027aa0   0x00000034   Code   RO          833    i.pending_user_evts_send  ble_db_discovery.o
    0x00027ad4   0x0000001c   Code   RO         1529    i.pin_in_use_by_gpiote  nrf_drv_gpiote.o
    0x00027af0   0x00000018   Code   RO         1530    i.pin_in_use_by_port  nrf_drv_gpiote.o
    0x00027b08   0x00000020   Code   RO         1531    i.pin_in_use_by_te  nrf_drv_gpiote.o
    0x00027b28   0x0000000c   Code   RO         1532    i.pin_in_use_clear  nrf_drv_gpiote.o
    0x00027b34   0x00000044   Code   RO         3625    i.postfix_process   nrf_log_str_formatter.o
    0x00027b78   0x0000001c   Code   RO           19    i.power_init        main.o
    0x00027b94   0x0000005c   Code   RO         3626    i.prefix_process    nrf_log_str_formatter.o
    0x00027bf0   0x00000010   Code   RO         4055    i.ram_end_address_get  nrf_sdh_ble.o
    0x00027c00   0x00000040   Code   RO          834    i.registered_handler_get  ble_db_discovery.o
    0x00027c40   0x00000044   Code   RO          835    i.registered_handler_set  ble_db_discovery.o
    0x00027c84   0x0000000c   Code   RO         2396    i.rtc1_compare0_set  app_timer.o
    0x00027c90   0x0000000c   Code   RO         2397    i.rtc1_counter_get  app_timer.o
    0x00027c9c   0x00000018   Code   RO         2398    i.rtc1_init         app_timer.o
    0x00027cb4   0x0000003c   Code   RO         2399    i.rtc1_start        app_timer.o
    0x00027cf0   0x00000058   Code   RO         2400    i.rtc1_stop         app_timer.o
    0x00027d48   0x0000003e   Code   RO         1831    i.rx_byte           nrf_drv_uart.o
    0x00027d86   0x0000001e   Code   RO         1832    i.rx_done_event     nrf_drv_uart.o
    0x00027da4   0x00000022   Code   RO         1833    i.rx_enable         nrf_drv_uart.o
    0x00027dc6   0x00000002   PAD
    0x00027dc8   0x0000003c   Code   RO           20    i.scan_start        main.o
    0x00027e04   0x000000a0   Code   RO         3936    i.sd_nvic_EnableIRQ  nrf_sdh.o
    0x00027ea4   0x00000068   Code   RO         2678    i.sd_nvic_critical_region_enter  app_util_platform.o
    0x00027f0c   0x0000006c   Code   RO         1275    i.sd_state_evt_handler  nrf_drv_clock.o
    0x00027f78   0x0000003c   Code   RO         3937    i.sdh_request_observer_notify  nrf_sdh.o
    0x00027fb4   0x00000034   Code   RO         3938    i.sdh_state_observer_notify  nrf_sdh.o
    0x00027fe8   0x0000003e   Code   RO         3290    i.serial_tx         nrf_log_backend_rtt.o
    0x00028026   0x00000042   Code   RO           21    i.shutdown_handler  main.o
    0x00028068   0x000000cc   Code   RO         3103    i.shutdown_process  nrf_pwr_mgmt.o
    0x00028134   0x00000010   Code   RO         1276    i.soc_evt_handler   nrf_drv_clock.o
    0x00028144   0x0000001e   Code   RO         3940    i.softdevices_evt_irq_enable  nrf_sdh.o
    0x00028162   0x00000026   Code   RO          613    i.startup_event_extract  bsp_btn_ble.o
    0x00028188   0x00000050   Code   RO         3445    i.std_header_set    nrf_log_frontend.o
    0x000281d8   0x0000006c   Code   RO         3446    i.std_n             nrf_log_frontend.o
    0x00028244   0x00000074   Code   RO         2967    i.string_print      nrf_fprintf_format.o
    0x000282b8   0x0000000a   Code   RO         2401    i.ticks_diff_get    app_timer.o
    0x000282c2   0x0000000c   Code   RO         2402    i.timeout_handler_exec  app_timer.o
    0x000282ce   0x0000001c   Code   RO           22    i.timer_init        main.o
    0x000282ea   0x00000002   PAD
    0x000282ec   0x00000050   Code   RO         2403    i.timer_list_handler  app_timer.o
    0x0002833c   0x0000000a   Code   RO         2404    i.timer_list_handler_sched  app_timer.o
    0x00028346   0x00000002   PAD
    0x00028348   0x00000068   Code   RO         2405    i.timer_list_insert  app_timer.o
    0x000283b0   0x00000088   Code   RO         2406    i.timer_list_remove  app_timer.o
    0x00028438   0x0000005e   Code   RO         2407    i.timer_start_op_schedule  app_timer.o
    0x00028496   0x00000042   Code   RO         2408    i.timer_stop_op_schedule  app_timer.o
    0x000284d8   0x00000098   Code   RO         2409    i.timer_timeouts_check  app_timer.o
    0x00028570   0x0000000a   Code   RO         2410    i.timer_timeouts_check_sched  app_timer.o
    0x0002857a   0x00000026   Code   RO         1834    i.tx_byte           nrf_drv_uart.o
    0x000285a0   0x00000022   Code   RO         1835    i.tx_done_event     nrf_drv_uart.o
    0x000285c2   0x00000002   PAD
    0x000285c4   0x0000012c   Code   RO           23    i.uart_event_handle  main.o
    0x000286f0   0x000000d4   Code   RO         2606    i.uart_event_handler  app_uart_fifo.o
    0x000287c4   0x0000005c   Code   RO           24    i.uart_init         main.o
    0x00028820   0x00000142   Code   RO         1836    i.uart_irq_handler  nrf_drv_uart.o
    0x00028962   0x0000010c   Code   RO         1837    i.uarte_irq_handler  nrf_drv_uart.o
    0x00028a6e   0x00000002   PAD
    0x00028a70   0x000000b8   Code   RO         2968    i.unsigned_print    nrf_fprintf_format.o
    0x00028b28   0x0000003c   Code   RO         2411    i.user_op_alloc     app_timer.o
    0x00028b64   0x0000000c   Code   RO         2412    i.user_op_enque     app_timer.o
    0x00028b70   0x0000002c   Data   RO           26    .constdata          main.o
    0x00028b9c   0x00000008   Data   RO          388    .constdata          boards.o
    0x00028ba4   0x0000002c   Data   RO          507    .constdata          bsp.o
    0x00028bd0   0x0000007c   Data   RO          837    .constdata          ble_db_discovery.o
    0x00028c4c   0x00000016   Data   RO         1052    .constdata          nrf_ble_gatt.o
    0x00028c62   0x00000002   PAD
    0x00028c64   0x00000028   Data   RO         1164    .constdata          ble_nus_c.o
    0x00028c8c   0x0000004b   Data   RO         1534    .constdata          nrf_drv_gpiote.o
    0x00028cd7   0x00000001   PAD
    0x00028cd8   0x00000008   Data   RO         2108    .constdata          app_button.o
    0x00028ce0   0x00000020   Data   RO         2608    .constdata          app_uart_fifo.o
    0x00028d00   0x00000010   Data   RO         2969    .constdata          nrf_fprintf_format.o
    0x00028d10   0x00000024   Data   RO         3105    .constdata          nrf_pwr_mgmt.o
    0x00028d34   0x00000104   Data   RO         3218    .constdata          nrf_strerror.o
    0x00028e38   0x0000000c   Data   RO         3292    .constdata          nrf_log_backend_rtt.o
    0x00028e44   0x00000014   Data   RO         3448    .constdata          nrf_log_frontend.o
    0x00028e58   0x00000058   Data   RO         3941    .constdata          nrf_sdh.o
    0x00028eb0   0x00000030   Data   RO         4056    .constdata          nrf_sdh_ble.o
    0x00028ee0   0x0000001c   Data   RO         4107    .constdata          nrf_sdh_soc.o
    0x00028efc   0x00000081   Data   RO         4218    .constdata          mc_w.l(ctype_o.o)
    0x00028f7d   0x00000003   PAD
    0x00028f80   0x00000004   Data   RO         4219    .constdata          mc_w.l(ctype_o.o)
    0x00028f84   0x0000012d   Data   RO         1053    .conststring        nrf_ble_gatt.o
    0x000290b1   0x00000003   PAD
    0x000290b4   0x00000307   Data   RO         3219    .conststring        nrf_strerror.o
    0x000293bb   0x00000001   PAD
    0x000293bc   0x00000009   Data   RO         3449    .conststring        nrf_log_frontend.o
    0x000293c5   0x00000003   PAD
    0x000293c8   0x00000066   Data   RO         3627    .conststring        nrf_log_str_formatter.o
    0x0002942e   0x00000002   PAD
    0x00029430   0x000001cf   Data   RO         4057    .conststring        nrf_sdh_ble.o
    0x000295ff   0x00000001   PAD
    0x00029600   0x0000000c   Data   RO          838    .conststrlit        ble_db_discovery.o
    0x0002960c   0x00000009   Data   RO         1054    .conststrlit        nrf_ble_gatt.o
    0x00029615   0x00000003   PAD
    0x00029618   0x00000008   Data   RO         1165    .conststrlit        ble_nus_c.o
    0x00029620   0x00000006   Data   RO         1279    .conststrlit        nrf_drv_clock.o
    0x00029626   0x00000002   PAD
    0x00029628   0x00000007   Data   RO         1535    .conststrlit        nrf_drv_gpiote.o
    0x0002962f   0x00000001   PAD
    0x00029630   0x00000005   Data   RO         1839    .conststrlit        nrf_drv_uart.o
    0x00029635   0x00000003   PAD
    0x00029638   0x00000007   Data   RO         2875    .conststrlit        nrf_balloc.o
    0x0002963f   0x00000001   PAD
    0x00029640   0x00000009   Data   RO         3106    .conststrlit        nrf_pwr_mgmt.o
    0x00029649   0x00000003   PAD
    0x0002964c   0x00000004   Data   RO         3450    .conststrlit        nrf_log_frontend.o
    0x00029650   0x00000008   Data   RO         3942    .conststrlit        nrf_sdh.o
    0x00029658   0x0000000c   Data   RO         4058    .conststrlit        nrf_sdh_ble.o
    0x00029664   0x0000000c   Data   RO         4108    .conststrlit        nrf_sdh_soc.o
    0x00029670   0x00000020   Data   RO         4552    Region$$Table       anon$$obj.o
    0x00029690   0x00000008   Data   RO          840    log_const_data      ble_db_discovery.o
    0x00029698   0x00000008   Data   RO         1055    log_const_data      nrf_ble_gatt.o
    0x000296a0   0x00000008   Data   RO         1166    log_const_data      ble_nus_c.o
    0x000296a8   0x00000008   Data   RO         1280    log_const_data      nrf_drv_clock.o
    0x000296b0   0x00000008   Data   RO         1536    log_const_data      nrf_drv_gpiote.o
    0x000296b8   0x00000008   Data   RO         1840    log_const_data      nrf_drv_uart.o
    0x000296c0   0x00000008   Data   RO         2876    log_const_data      nrf_balloc.o
    0x000296c8   0x00000008   Data   RO         3108    log_const_data      nrf_pwr_mgmt.o
    0x000296d0   0x00000008   Data   RO         3452    log_const_data      nrf_log_frontend.o
    0x000296d8   0x00000008   Data   RO         3944    log_const_data      nrf_sdh.o
    0x000296e0   0x00000008   Data   RO         4059    log_const_data      nrf_sdh_ble.o
    0x000296e8   0x00000008   Data   RO         4109    log_const_data      nrf_sdh_soc.o
    0x000296f0   0x00000004   Data   RO           28    pwr_mgmt_data1      main.o
    0x000296f4   0x00000010   Data   RO           29    sdh_ble_observers1  main.o
    0x00029704   0x00000008   Data   RO          615    sdh_ble_observers1  bsp_btn_ble.o
    0x0002970c   0x00000008   Data   RO           30    sdh_ble_observers2  main.o
    0x00029714   0x00000008   Data   RO           31    sdh_ble_observers3  main.o
    0x0002971c   0x00000008   Data   RO         1282    sdh_soc_observers0  nrf_drv_clock.o
    0x00029724   0x00000008   Data   RO         4061    sdh_stack_observers0  nrf_sdh_ble.o
    0x0002972c   0x00000008   Data   RO         4111    sdh_stack_observers0  nrf_sdh_soc.o
    0x00029734   0x00000008   Data   RO         1283    sdh_state_observers0  nrf_drv_clock.o


    Execution Region RW_IRAM1 (Base: 0x20002978, Size: 0x00003480, Max: 0x0003d688, ABSOLUTE, COMPRESSED[0x00000048])

    Base Addr    Size         Type   Attr      Idx    E Section Name        Object

    0x20002978   0x000002d0   Data   RW           27    .data               main.o
    0x20002c48   0x00000015   Data   RW          508    .data               bsp.o
    0x20002c5d   0x00000003   PAD
    0x20002c60   0x00000008   Data   RW          614    .data               bsp_btn_ble.o
    0x20002c68   0x0000000d   Data   RW          839    .data               ble_db_discovery.o
    0x20002c75   0x00000003   PAD
    0x20002c78   0x00000014   Data   RW         2109    .data               app_button.o
    0x20002c8c   0x00000014   Data   RW         2414    .data               app_timer.o
    0x20002ca0   0x0000000f   Data   RW         2609    .data               app_uart_fifo.o
    0x20002caf   0x00000001   PAD
    0x20002cb0   0x00000009   Data   RW         3107    .data               nrf_pwr_mgmt.o
    0x20002cb9   0x00000003   PAD
    0x20002cbc   0x00000008   Data   RW         3251    .data               retarget.o
    0x20002cc4   0x0000000c   Data   RW         3385    .data               nrf_log_default_backends.o
    0x20002cd0   0x00000014   Data   RW         3451    .data               nrf_log_frontend.o
    0x20002ce4   0x00000038   Data   RW         3628    .data               nrf_log_str_formatter.o
    0x20002d1c   0x00000003   Data   RW         3943    .data               nrf_sdh.o
    0x20002d1f   0x00000001   PAD
    0x20002d20   0x00000004   Data   RW         4153    .data               system_nrf52840.o
    0x20002d24   0x0000000c   Data   RW          841    log_dynamic_data    ble_db_discovery.o
    0x20002d30   0x0000000c   Data   RW         1056    log_dynamic_data    nrf_ble_gatt.o
    0x20002d3c   0x0000000c   Data   RW         1167    log_dynamic_data    ble_nus_c.o
    0x20002d48   0x0000000c   Data   RW         1281    log_dynamic_data    nrf_drv_clock.o
    0x20002d54   0x0000000c   Data   RW         1537    log_dynamic_data    nrf_drv_gpiote.o
    0x20002d60   0x0000000c   Data   RW         1841    log_dynamic_data    nrf_drv_uart.o
    0x20002d6c   0x0000000c   Data   RW         2877    log_dynamic_data    nrf_balloc.o
    0x20002d78   0x0000000c   Data   RW         3109    log_dynamic_data    nrf_pwr_mgmt.o
    0x20002d84   0x0000000c   Data   RW         3453    log_dynamic_data    nrf_log_frontend.o
    0x20002d90   0x0000000c   Data   RW         3945    log_dynamic_data    nrf_sdh.o
    0x20002d9c   0x0000000c   Data   RW         4060    log_dynamic_data    nrf_sdh_ble.o
    0x20002da8   0x0000000c   Data   RW         4110    log_dynamic_data    nrf_sdh_soc.o
    0x20002db4   0x00000318   Zero   RW           25    .bss                main.o
    0x200030cc   0x0000006c   Zero   RW          506    .bss                bsp.o
    0x20003138   0x00000318   Zero   RW          836    .bss                ble_db_discovery.o
    0x20003450   0x00000014   Zero   RW         1277    .bss                nrf_drv_clock.o
    0x20003464   0x00000068   Zero   RW         1533    .bss                nrf_drv_gpiote.o
    0x200034cc   0x00000020   Zero   RW         1838    .bss                nrf_drv_uart.o
    0x200034ec   0x00000020   Zero   RW         2107    .bss                app_button.o
    0x2000350c   0x0000010c   Zero   RW         2413    .bss                app_timer.o
    0x20003618   0x00000020   Zero   RW         2607    .bss                app_uart_fifo.o
    0x20003638   0x0000000c   Zero   RW         2679    .bss                app_util_platform.o
    0x20003644   0x0000000c   Zero   RW         3104    .bss                nrf_pwr_mgmt.o
    0x20003650   0x00000040   Zero   RW         3291    .bss                nrf_log_backend_rtt.o
    0x20003690   0x000004e0   Zero   RW         3447    .bss                nrf_log_frontend.o
    0x20003b70   0x00000288   Zero   RW         3699    .bss                segger_rtt.o
    0x20003df8   0x00002000   Zero   RW         4134    STACK               arm_startup_nrf52840.o


==============================================================================

Image component sizes


      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Object Name

       480         80          8         20         32      10242   app_button.o
        28          0          0          0          0       2141   app_error.o
       176         42          0          0          0      30365   app_error_weak.o
       170          0          0          0          0       6158   app_fifo.o
      2200        248          0         20        268      53159   app_timer.o
       602         92         32         15         32      11382   app_uart_fifo.o
       200         24          0          0         12      10394   app_util_platform.o
        36          8        512          0       8192        936   arm_startup_nrf52840.o
         0          0          0          0          0        392   ble_advdata.o
      2290        132        144         25        792      28319   ble_db_discovery.o
       688         66         56         12          0      20110   ble_nus_c.o
       486         42          8          0          0      14108   boards.o
      1584        130         44         21        108      15575   bsp.o
       420         16          8          8          0       6100   bsp_btn_ble.o
      2604        656         80        720        792     126622   main.o
       218          0         15         12          0       5125   nrf_balloc.o
       958         64        340         12          0      35827   nrf_ble_gatt.o
       516         52         30         12         20      43115   nrf_drv_clock.o
        96         12          0          0          0      27675   nrf_drv_common.o
      1700        110         90         12        104      35756   nrf_drv_gpiote.o
      2770         80         13         12         32      51323   nrf_drv_uart.o
        70          0          0          0          0       3605   nrf_fprintf.o
      1018          6         16          0          0       6170   nrf_fprintf_format.o
       106          8         12          0         64       5701   nrf_log_backend_rtt.o
       254          0          0          0          0      10507   nrf_log_backend_serial.o
        36          4          0         12          0       3202   nrf_log_default_backends.o
      2032         92         41         32       1248      34188   nrf_log_frontend.o
       544         70        102         56          0       5404   nrf_log_str_formatter.o
       660          0          0          0          0      13403   nrf_memobj.o
       660         56         53         21         12      52087   nrf_pwr_mgmt.o
       540         56        104         15          0      45821   nrf_sdh.o
       744        166        539         12          0       6603   nrf_sdh_ble.o
        84          4         56         12          0       2828   nrf_sdh_soc.o
       112          0          0          0          0       2852   nrf_section_iter.o
        92         10       1035          0          0       2779   nrf_strerror.o
        16          0          0          8          0       2914   retarget.o
       470         44          0          0        648       8549   segger_rtt.o
       772        102          0          4          0       6023   system_nrf52840.o

    ----------------------------------------------------------------------
     26490       2472       3396       1084      12356     747460   Object Totals
         0          0         32          0          0          0   (incl. Generated)
        58          0         26         11          0          0   (incl. Padding)

    ----------------------------------------------------------------------

      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Library Member Name

        86          0          0          0          0          0   __dczerorl2.o
         8          4        133          0          0         68   ctype_o.o
         0          0          0          0          0          0   entry.o
         0          0          0          0          0          0   entry10a.o
         0          0          0          0          0          0   entry11a.o
         8          4          0          0          0          0   entry2.o
         4          0          0          0          0          0   entry5.o
         0          0          0          0          0          0   entry7b.o
         0          0          0          0          0          0   entry8b.o
         8          4          0          0          0          0   entry9a.o
        30          0          0          0          0          0   handlers.o
        36          8          0          0          0         68   init.o
        30          0          0          0          0         68   llshl.o
        32          0          0          0          0         68   llushr.o
        36          0          0          0          0         68   memcpya.o
        36          0          0          0          0        108   memseta.o
        50          8          0          0          0        152   printfb.o
        18          0          0          0          0         68   strcpy.o
        14          0          0          0          0         68   strlen.o
        98          0          0          0          0         92   uldiv.o

    ----------------------------------------------------------------------
       502         28        136          0          0        828   Library Totals
         8          0          3          0          0          0   (incl. Padding)

    ----------------------------------------------------------------------

      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   Library Name

       494         28        133          0          0        828   mc_w.l

    ----------------------------------------------------------------------
       502         28        136          0          0        828   Library Totals

    ----------------------------------------------------------------------

==============================================================================


      Code (inc. data)   RO Data    RW Data    ZI Data      Debug   

     26992       2500       3532       1084      12356     716760   Grand Totals
     26992       2500       3532         72      12356     716760   ELF Image Totals (compressed)
     26992       2500       3532         72          0          0   ROM Totals

==============================================================================

    Total RO  Size (Code + RO Data)                30524 (  29.81kB)
    Total RW  Size (RW Data + ZI Data)             13440 (  13.13kB)
    Total ROM Size (Code + RO Data + RW Data)      30596 (  29.88kB)

==============================================================================

